(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "nRF51x22-QFxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "nRF51x22-QFxx"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://infocenter.nordicsemi.com/pdf/nRF51822_PS_v3.3.pdf"
			(at -10.16 -2.54 0)
		)
		(property "Description" "Multiprotocol BLE/2.4GHz Cortex-M0+ SoC"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE 2.4GHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "nRF51x22-QFxx_0_1")
		(symbol "nRF51x22-QFxx_1_1"
			(pin output line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "ANT1")
				(number "31")
			)
			(pin output line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "ANT2")
				(number "32")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "XC1")
				(number "37")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "XC2")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "SWDIO/~{RST}")
				(number "23")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "SWDCLK")
				(number "24")
			)
			(pin passive line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "DEC1")
				(number "39")
			)
			(pin passive line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "DEC2")
				(number "29")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "13")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "34")
			)
			(pin power_out line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD_PA")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "EP")
				(number "49")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "AVDD")
				(number "35")
			)
			(pin passive line
				(at 7.62 45.72 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "36")
			)
			(pin power_out line
				(at 12.7 45.72 270)
				(length 2.54)
				(name "DCC")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "P0.0")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "P0.1")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "P0.2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "P0.3")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "P0.4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "P0.5")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "P0.6")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "P0.7")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "P0.8")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "P0.9")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "P0.10")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "P0.11")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "P0.12")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "P0.13")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "P0.14")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "P0.15")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "P0.16")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "P0.17")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "P0.18")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "P0.19")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "P0.20")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "P0.21")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "P0.22")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "P0.23")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "P0.24")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "P0.25")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "P0.26")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "P0.27")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "P0.28")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "P0.29")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "P0.30")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF52810-QCxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "nRF52810-QCxx"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "http://infocenter.nordicsemi.com/pdf/nRF52810_PS_v1.1.pdf"
			(at -12.7 5.08 0)
		)
		(property "Description" "Multiprotocol BLE/2.4GHz Cortex-M4 SoC, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE 2.4GHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "nRF52810-QCxx_0_1")
		(symbol "nRF52810-QCxx_1_1"
			(pin passive line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "ANT")
				(number "19")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "XC1")
				(number "23")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "XC2")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "P0.21/~{RESET}")
				(number "16")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "SWDCLK")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "SWDIO")
				(number "18")
			)
			(pin passive line
				(at -12.7 25.4 270)
				(length 2.54)
				(name "DEC1")
				(number "1")
			)
			(pin passive line
				(at -10.16 25.4 270)
				(length 2.54)
				(name "DEC2")
				(number "21")
			)
			(pin passive line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "DEC3")
				(number "22")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "DEC4")
				(number "30")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "25")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "DCC")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "P0.00/XL1")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "P0.01/XL2")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "P0.04/AIN2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "P0.05/AIN3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "P0.06")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "P0.09")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "P0.10")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "P0.12")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "P0.14")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "P0.15")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "P0.16")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "P0.18")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "P0.20")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "P0.25")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "P0.28/AIN4")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "P0.30/AIN6")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF52810-QFxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "nRF52810-QFxx"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm"
			(at 0 -52.07 0)
		)
		(property "Datasheet" "http://infocenter.nordicsemi.com/pdf/nRF52810_PS_v1.1.pdf"
			(at -12.7 5.08 0)
		)
		(property "Description" "Multiprotocol BLE/2.4GHz Cortex-M4 SoC, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE 2.4GHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "nRF52810-QFxx_0_1")
		(symbol "nRF52810-QFxx_1_1"
			(pin passive line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "ANT")
				(number "30")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "XC1")
				(number "34")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "XC2")
				(number "35")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "P0.21/~{RESET}")
				(number "24")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "SWDCLK")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "SWDIO")
				(number "26")
			)
			(pin no_connect line
				(at -20.32 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "44")
			)
			(pin passive line
				(at -12.7 43.18 270)
				(length 2.54)
				(name "DEC1")
				(number "1")
			)
			(pin passive line
				(at -10.16 43.18 270)
				(length 2.54)
				(name "DEC2")
				(number "32")
			)
			(pin passive line
				(at -7.62 43.18 270)
				(length 2.54)
				(name "DEC3")
				(number "33")
			)
			(pin passive line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "DEC4")
				(number "46")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "36")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_out line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "DCC")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "P0.00/XL1")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "P0.01/XL2")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "P0.02/AIN0")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "P0.03/AIN1")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "P0.04/AIN2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "P0.05/AIN3")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "P0.06")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "P0.07")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "P0.08")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "P0.09")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "P0.10")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "P0.11")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "P0.12")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "P0.13")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "P0.14")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "P0.15")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "P0.16")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "P0.17")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "P0.18")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "P0.19")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "P0.20")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "P0.22")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "P0.23")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "P0.24")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "P0.25")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "P0.26")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "P0.27")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "P0.28/AIN4")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "P0.29/AIN5")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "P0.30/AIN6")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "P0.31/AIN7")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF52811-QCxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "nRF52811-QCxx"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm_ThermalVias"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://infocenter.nordicsemi.com/pdf/nRF52811_PS_v1.0.pdf"
			(at -16.51 48.26 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE ANT 2.4GHz 802.15.4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "nRF52811-QCxx_0_1")
		(symbol "nRF52811-QCxx_1_1"
			(pin passive line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "ANT")
				(number "19")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "XC1")
				(number "23")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "XC2")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "P0.21/~{RESET}")
				(number "16")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "SWDCLK")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "SWDIO")
				(number "18")
			)
			(pin passive line
				(at -15.24 25.4 270)
				(length 2.54)
				(name "DEC1")
				(number "1")
			)
			(pin passive line
				(at -12.7 25.4 270)
				(length 2.54)
				(name "DEC2")
				(number "21")
			)
			(pin passive line
				(at -10.16 25.4 270)
				(length 2.54)
				(name "DEC3")
				(number "22")
			)
			(pin passive line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "DEC4")
				(number "30")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "25")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_out line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "DCC")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "XL1/P0.00")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "XL2/P0.01")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "AIN2/P0.04")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "AIN3/P0.05")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "P0.06")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "P0.09")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "P0.10")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "P0.12")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "P0.14")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "P0.15")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "P0.16")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "P0.18")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "P0.20")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "P0.25")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "AIN4/P0.28")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "AIN6/P0.30")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF52820-QDxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 0 0)
		)
		(property "Value" "nRF52820-QDxx"
			(at -2.54 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.6x3.6mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://infocenter.nordicsemi.com/pdf/nRF52820_PS_v1.0.pdf"
			(at -16.51 48.26 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4 SoC, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE ANT 2.4GHz 802.15.4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "nRF52820-QDxx_0_1")
		(symbol "nRF52820-QDxx_1_1"
			(pin passive line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "ANT")
				(number "24")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "XC1")
				(number "28")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "XC2")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "D+")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "D-")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "P0.18/~{RESET}")
				(number "16")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "SWDCLK")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "SWDIO")
				(number "19")
			)
			(pin passive line
				(at -22.86 25.4 270)
				(length 2.54)
				(name "DEC1")
				(number "1")
			)
			(pin passive line
				(at -20.32 25.4 270)
				(length 2.54)
				(name "DEC3")
				(number "27")
			)
			(pin passive line
				(at -17.78 25.4 270)
				(length 2.54)
				(name "DEC4")
				(number "38")
			)
			(pin passive line
				(at -15.24 25.4 270)
				(length 2.54)
				(name "DEC5")
				(number "21")
			)
			(pin passive line
				(at -12.7 25.4 270)
				(length 2.54)
				(name "DEC6")
				(number "26")
			)
			(pin passive line
				(at -10.16 25.4 270)
				(length 2.54)
				(name "DECUSB")
				(number "11")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS_PA")
				(number "25")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VDDH")
				(number "9")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "VBUS")
				(number "10")
			)
			(pin power_out line
				(at 12.7 25.4 270)
				(length 2.54)
				(name "DCC")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "XL1/P0.00")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "XL2/P0.01")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "AIN0/P0.02")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "AIN1/P0.03")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "AIN2/P0.04")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "AIN3/P0.05")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "P0.06")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "P0.07")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "P0.08")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "P0.14")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "P0.15")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "P0.16")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "P0.17")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "P0.20")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "P0.28")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "P0.29")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "P0.30")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF52832-QFxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "nRF52832-QFxx"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "http://infocenter.nordicsemi.com/pdf/nRF52832_PS_v1.4.pdf"
			(at -12.7 5.08 0)
		)
		(property "Description" "Multiprotocol BLE/2.4GHz Cortex-M4 SoC, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE 2.4GHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "nRF52832-QFxx_0_1")
		(symbol "nRF52832-QFxx_1_1"
			(pin passive line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "ANT")
				(number "30")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "XC1")
				(number "34")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "XC2")
				(number "35")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "P0.21/~{RESET}")
				(number "24")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "SWDCLK")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "SWDIO")
				(number "26")
			)
			(pin no_connect line
				(at -20.32 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "44")
			)
			(pin passive line
				(at -12.7 43.18 270)
				(length 2.54)
				(name "DEC1")
				(number "1")
			)
			(pin passive line
				(at -10.16 43.18 270)
				(length 2.54)
				(name "DEC2")
				(number "32")
			)
			(pin passive line
				(at -7.62 43.18 270)
				(length 2.54)
				(name "DEC3")
				(number "33")
			)
			(pin passive line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "DEC4")
				(number "46")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "36")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_out line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "DCC")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "P0.00/XL1")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "P0.01/XL2")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "P0.02/AIN0")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "P0.03/AIN1")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "P0.04/AIN2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "P0.05/AIN3")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "P0.06")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "P0.07")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "P0.08")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "NFC1/P0.09")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "NFC2/P0.10")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "P0.11")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "P0.12")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "P0.13")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "P0.14")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "P0.15")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "P0.16")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "P0.17")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "P0.18/SWO")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "P0.19")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "P0.20")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "P0.22")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "P0.23")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "P0.24")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "P0.25")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "P0.26")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "P0.27")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "P0.28/AIN4")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "P0.29/AIN5")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "P0.30/AIN6")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "P0.31/AIN7")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF52833_QDxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "nRF52833_QDxx"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.6x3.6mm"
			(at 0 -73.66 0)
		)
		(property "Datasheet" "https://infocenter.nordicsemi.com/pdf/nRF52833_PS_v1.5.pdf"
			(at -16.51 48.26 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE ANT 2.4GHz 802.15.4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "nRF52833_QDxx_0_1")
		(symbol "nRF52833_QDxx_1_1"
			(pin passive line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "ANT")
				(number "24")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "XC1")
				(number "28")
			)
			(pin input line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "XC2")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "P0.18/~{RESET}")
				(number "16")
			)
			(pin input line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "SWDCLK")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "SWDIO")
				(number "19")
			)
			(pin passive line
				(at -20.32 71.12 270)
				(length 5.08)
				(name "DEC1")
				(number "1")
			)
			(pin passive line
				(at -15.24 71.12 270)
				(length 5.08)
				(name "DEC3")
				(number "27")
			)
			(pin passive line
				(at -12.7 71.12 270)
				(length 5.08)
				(name "DEC4")
				(number "38")
			)
			(pin passive line
				(at -10.16 71.12 270)
				(length 5.08)
				(name "DEC5")
				(number "21")
			)
			(pin passive line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "DEC6")
				(number "26")
			)
			(pin passive line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "DECUSB")
				(number "11")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "18")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDDH")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSS_PA")
				(number "25")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VBUS")
				(number "10")
			)
			(pin power_out line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "DCC")
				(number "39")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "XL1/P0.00")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "XL2/P0.01")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "AIN0/P0.02")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "AIN1/P0.03")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "AIN2/P0.04")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "AIN3/P0.05")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "NFC1/P0.09")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "NFC2/P0.10")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "P0.11")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "P0.15")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "P0.17")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "P0.20")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "AIN4/P0.28")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "AIN5/P0.29")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "AIN6/P0.30")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "AIN7/P0.31")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "P1.09")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "D-")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "D+")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF52833_QIxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "nRF52833_QIxx"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:Nordic_AQFN-73-1EP_7x7mm_P0.5mm"
			(at 0 -73.66 0)
		)
		(property "Datasheet" "https://infocenter.nordicsemi.com/pdf/nRF52833_PS_v1.5.pdf"
			(at -16.51 48.26 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, AQFN-73"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE ANT 2.4GHz 802.15.4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nordic*AQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "nRF52833_QIxx_0_1")
		(symbol "nRF52833_QIxx_1_1"
			(pin passive line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "ANT")
				(number "H23")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "XC1")
				(number "B24")
			)
			(pin input line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "XC2")
				(number "A23")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "P0.18/~{RESET}")
				(number "AC13")
			)
			(pin input line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "SWDCLK")
				(number "AA24")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "SWDIO")
				(number "AC24")
			)
			(pin passive line
				(at -20.32 71.12 270)
				(length 5.08)
				(name "DEC1")
				(number "C1")
			)
			(pin no_connect line
				(at -17.78 66.04 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A18")
			)
			(pin passive line
				(at -15.24 71.12 270)
				(length 5.08)
				(name "DEC3")
				(number "D23")
			)
			(pin passive line
				(at -12.7 71.12 270)
				(length 5.08)
				(name "DEC4")
				(number "B5")
			)
			(pin passive line
				(at -10.16 71.12 270)
				(length 5.08)
				(name "DEC5")
				(number "N24")
			)
			(pin passive line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "DEC6")
				(number "E24")
			)
			(pin passive line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "DECUSB")
				(number "AC5")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "A22")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AD14")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AD23")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "B1")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "W1")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "EP")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDDH")
				(number "Y2")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSS_PA")
				(number "F23")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VBUS")
				(number "AD2")
			)
			(pin power_out line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "DCC")
				(number "B3")
			)
			(pin no_connect line
				(at 12.7 66.04 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AB2")
			)
			(pin no_connect line
				(at 27.94 -43.18 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AC21")
			)
			(pin no_connect line
				(at 27.94 -45.72 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B19")
			)
			(pin no_connect line
				(at 27.94 -48.26 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AC19")
			)
			(pin no_connect line
				(at 27.94 -50.8 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "T23")
			)
			(pin no_connect line
				(at 27.94 -53.34 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "V23")
			)
			(pin no_connect line
				(at 27.94 -55.88 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AC15")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "XL1/P0.00")
				(number "D2")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "XL2/P0.01")
				(number "F2")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "AIN0/P0.02")
				(number "A12")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "AIN1/P0.03")
				(number "B13")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "AIN2/P0.04")
				(number "J1")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "AIN3/P0.05")
				(number "K2")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "P0.06")
				(number "L1")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "TRACECLK/P0.07")
				(number "M2")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "P0.08")
				(number "N1")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "NFC1/P0.09")
				(number "L24")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "NFC2/P0.10")
				(number "J24")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "TRACEDATA2/P0.11")
				(number "T2")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "TRACEDATA1/P0.12")
				(number "U1")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "P0.13")
				(number "AD8")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "P0.14")
				(number "AC9")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "P0.15")
				(number "AD10")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "P0.16")
				(number "AC11")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "P0.17")
				(number "AD12")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "P0.19")
				(number "A14")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "P0.20")
				(number "AD16")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "P0.21")
				(number "AC17")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "P0.22")
				(number "AD18")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "P0.23")
				(number "B17")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "P0.24")
				(number "AD20")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "P0.25")
				(number "A20")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "P0.26")
				(number "G1")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "P0.27")
				(number "H2")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "AIN4/P0.28")
				(number "B11")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "AIN5/P0.29")
				(number "A10")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "AIN6/P0.30")
				(number "B9")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "AIN7/P0.31")
				(number "A8")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "TRACEDATA0/P1.00")
				(number "AD22")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "P1.01")
				(number "Y23")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "P1.02")
				(number "W24")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "P1.03")
				(number "B15")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "P1.04")
				(number "U24")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "P1.05")
				(number "A16")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "P1.06")
				(number "R24")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "P1.07")
				(number "P23")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "P1.08")
				(number "P2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "TRACEDATA3/P1.09")
				(number "R1")
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "D-")
				(number "AD4")
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "D+")
				(number "AD6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF52840"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "nRF52840"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:Nordic_AQFN-73-1EP_7x7mm_P0.5mm"
			(at 0 -73.66 0)
		)
		(property "Datasheet" "http://infocenter.nordicsemi.com/topic/com.nordic.infocenter.nrf52/dita/nrf52/chips/nrf52840.html"
			(at -16.51 48.26 0)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, AQFN-73"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU ARM BLE ANT 2.4GHz 802.15.4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nordic*AQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "nRF52840_0_1")
		(symbol "nRF52840_1_1"
			(pin passive line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "ANT")
				(number "H23")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "XC1")
				(number "B24")
			)
			(pin input line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "XC2")
				(number "A23")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "P0.18/~{RESET}")
				(number "AC13")
			)
			(pin input line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "SWDCLK")
				(number "AA24")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "SWDIO")
				(number "AC24")
			)
			(pin passive line
				(at -20.32 71.12 270)
				(length 5.08)
				(name "DEC1")
				(number "C1")
			)
			(pin passive line
				(at -17.78 71.12 270)
				(length 5.08)
				(name "DEC2")
				(number "A18")
			)
			(pin passive line
				(at -15.24 71.12 270)
				(length 5.08)
				(name "DEC3")
				(number "D23")
			)
			(pin passive line
				(at -12.7 71.12 270)
				(length 5.08)
				(name "DEC4")
				(number "B5")
			)
			(pin passive line
				(at -10.16 71.12 270)
				(length 5.08)
				(name "DEC5")
				(number "N24")
			)
			(pin passive line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "DEC6")
				(number "E24")
			)
			(pin passive line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "DECUSB")
				(number "AC5")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "A22")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AD14")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AD23")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "B1")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "W1")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "EP")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDDH")
				(number "Y2")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSS_PA")
				(number "F23")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VBUS")
				(number "AD2")
			)
			(pin power_out line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "DCC")
				(number "B3")
			)
			(pin power_out line
				(at 12.7 71.12 270)
				(length 5.08)
				(name "DCCH")
				(number "AB2")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "XL1/P0.00")
				(number "D2")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "XL2/P0.01")
				(number "F2")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "AIN0/P0.02")
				(number "A12")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "AIN1/P0.03")
				(number "B13")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "AIN2/P0.04")
				(number "J1")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "AIN3/P0.05")
				(number "K2")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "P0.06")
				(number "L1")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "TRACECLK/P0.07")
				(number "M2")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "P0.08")
				(number "N1")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "NFC1/P0.09")
				(number "L24")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "NFC2/P0.10")
				(number "J24")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "TRACEDATA2/P0.11")
				(number "T2")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "TRACEDATA1/P0.12")
				(number "U1")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "P0.13")
				(number "AD8")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "P0.14")
				(number "AC9")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "P0.15")
				(number "AD10")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "P0.16")
				(number "AC11")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "P0.17")
				(number "AD12")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "P0.19")
				(number "AC15")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "P0.20")
				(number "AD16")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "P0.21")
				(number "AC17")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "P0.22")
				(number "AD18")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "P0.23")
				(number "AC19")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "P0.24")
				(number "AD20")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "P0.25")
				(number "AC21")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "P0.26")
				(number "G1")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "P0.27")
				(number "H2")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "AIN4/P0.28")
				(number "B11")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "AIN5/P0.29")
				(number "A10")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "AIN6/P0.30")
				(number "B9")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "AIN7/P0.31")
				(number "A8")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "TRACEDATA0/P1.00")
				(number "AD22")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "P1.01")
				(number "Y23")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "P1.02")
				(number "W24")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "P1.03")
				(number "V23")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "P1.04")
				(number "U24")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "P1.05")
				(number "T23")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "P1.06")
				(number "R24")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "P1.07")
				(number "P23")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "P1.08")
				(number "P2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "TRACEDATA3/P1.09")
				(number "R1")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "P1.10")
				(number "A20")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "P1.11")
				(number "B19")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "P1.12")
				(number "B17")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "P1.13")
				(number "A16")
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "P1.14")
				(number "B15")
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "P1.15")
				(number "A14")
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "D-")
				(number "AD4")
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "D+")
				(number "AD6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF5340-QKxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U1"
			(at 2.0194 -72.39 0)
		)
		(property "Value" "nRF5340-QKxx"
			(at 2.0194 -74.93 0)
		)
		(property "Footprint" "Package_DFN_QFN:Nordic_AQFN-94-1EP_7x7mm_P0.4mm"
			(at 35.56 73.66 0)
		)
		(property "Datasheet" "https://infocenter.nordicsemi.com/pdf/nRF5340_PS_v1.2.pdf"
			(at 35.56 71.12 0)
		)
		(property "Description" "nRF5340, BLE, NFC, Thread, Zigbee, ARM M33 SoC, Dual Core, AQFN-94"
			(at 0 0 0)
		)
		(property "ki_keywords" "nordic nrf nRF5340 aQFN94 BLE Zigbee NFC Thread M33"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nordic*AQFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "nRF5340-QKxx_0_1")
		(symbol "nRF5340-QKxx_1_1"
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "SWDCLK")
				(number "W31")
			)
			(pin bidirectional line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "SWDIO")
				(number "AA31")
			)
			(pin input line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "~{RESET}")
				(number "AC31")
			)
			(pin input line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "XC1")
				(number "C31")
			)
			(pin input line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "XC2")
				(number "B30")
			)
			(pin power_out line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "DCC")
				(number "A21")
			)
			(pin passive line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "DECR")
				(number "A27")
			)
			(pin passive line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "DECRF")
				(number "G31")
			)
			(pin power_out line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "DCCD")
				(number "B10")
			)
			(pin passive line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "DECD")
				(number "A15")
			)
			(pin passive line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "ANT")
				(number "L31")
			)
			(pin power_in line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "VBUS")
				(number "A5")
			)
			(pin passive line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "DECUSB")
				(number "B6")
			)
			(pin passive line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "DECN")
				(number "A23")
			)
			(pin passive line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "DECA")
				(number "A13")
			)
			(pin no_connect line
				(at -27.94 58.42 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A25")
			)
			(pin no_connect line
				(at -27.94 55.88 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B12")
			)
			(pin no_connect line
				(at -27.94 53.34 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B26")
			)
			(pin no_connect line
				(at -27.94 50.8 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "D2")
			)
			(pin no_connect line
				(at -27.94 48.26 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "F2")
			)
			(pin no_connect line
				(at -27.94 45.72 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G1")
			)
			(pin no_connect line
				(at -27.94 40.64 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H2")
			)
			(pin no_connect line
				(at -27.94 38.1 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J31")
			)
			(pin no_connect line
				(at -27.94 35.56 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "K2")
			)
			(pin no_connect line
				(at -27.94 30.48 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "T2")
			)
			(pin no_connect line
				(at -27.94 27.94 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AG31")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A19")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AC1")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AG1")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AJ31")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AL11")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AL17")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AL25")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AL3")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "AL7")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "B28")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "B8")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "C1")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E31")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L1")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "N31")
			)
			(pin passive line
				(at -2.54 73.66 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "U1")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDDH")
				(number "E1")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 5.08)
				(name "VSS")
				(number "EP")
			)
			(pin passive line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "DCCH")
				(number "J1")
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "XL1/P0.00")
				(number "N1")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "XL2/P0.01")
				(number "R1")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "NFC1/P0.02")
				(number "W1")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "NFC2/P0.03")
				(number "AA1")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "AIN0/P0.04")
				(number "V2")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "AIN1/P0.05")
				(number "Y2")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "AIN2/P0.06")
				(number "AB2")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "AIN3/P0.07")
				(number "AD2")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "SCK/TRACEDATA3/P0.08")
				(number "AH2")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "MOSI/TRACEDATA2/P0.09")
				(number "AJ1")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "MISO/TRACEDATA1/P0.10")
				(number "AK2")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "CSN/TRACEDATA0/P0.11")
				(number "AK4")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "DCX/TRACECLK/P0.12")
				(number "AK6")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "IO0/P0.13")
				(number "AL5")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "IO1/P0.14")
				(number "AK8")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "IO2/P0.15")
				(number "AK10")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "IO3/P0.16")
				(number "AL9")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "SCK/P0.17")
				(number "AK12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "CSN/P0.18")
				(number "AK14")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "P0.19")
				(number "AL13")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "P0.20")
				(number "AK16")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "P0.21")
				(number "AL15")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "P0.22")
				(number "AK18")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "P0.23")
				(number "AK20")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "P0.24")
				(number "AL27")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "AIN4/P0.25")
				(number "AK28")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "AIN5/P0.26")
				(number "AL29")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "AIN6/P0.27")
				(number "AK30")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "AIN7/P0.28")
				(number "AE31")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "P0.29")
				(number "U31")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "P0.30")
				(number "B24")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "P0.31")
				(number "B22")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "P1.00")
				(number "M2")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "P1.01")
				(number "P2")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "TWI/P1.02")
				(number "AE1")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "TWI/P1.03")
				(number "AF2")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "P1.04")
				(number "AL19")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "P1.05")
				(number "AK22")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "P1.06")
				(number "AL21")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "P1.07")
				(number "AK24")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "P1.08")
				(number "AL23")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "P1.09")
				(number "AK26")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "P1.10")
				(number "R31")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "P1.11")
				(number "B20")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "P1.12")
				(number "B18")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "P1.13")
				(number "A17")
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "P1.14")
				(number "B16")
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "P1.15")
				(number "B14")
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "D-")
				(number "B4")
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "D+")
				(number "B2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "nRF9160-SIxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 -50.8 0)
		)
		(property "Value" "nRF9160-SIxA"
			(at 1.27 -53.34 0)
		)
		(property "Footprint" "Package_LGA:Nordic_nRF9160-SIxx_LGA-102-59EP_16.0x10.5mm_P0.5mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf9160/attach/nRF9160_PS_v2.2.pdf"
			(at 0 -68.58 0)
		)
		(property "Description" "Low power SiP with integrated LTE-M/NB-IoT modem and GNSS"
			(at 0.254 -66.04 0)
		)
		(property "ki_keywords" "MCU ARM M33 cellular GPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nordic*nRF9160*LGA?102?59EP*16.0x10.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "nRF9160-SIxA_1_0"
			(pin no_connect line
				(at -20.32 33.02 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "70")
			)
			(pin no_connect line
				(at -20.32 30.48 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "51")
			)
			(pin no_connect line
				(at -20.32 27.94 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -20.32 17.78 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "71")
			)
			(pin no_connect line
				(at -20.32 15.24 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin no_connect line
				(at -20.32 12.7 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "104")
			)
			(pin no_connect line
				(at -20.32 10.16 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "105")
			)
			(pin no_connect line
				(at -20.32 7.62 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "106")
			)
			(pin no_connect line
				(at -20.32 2.54 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "107")
			)
			(pin no_connect line
				(at -20.32 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "108")
			)
			(pin no_connect line
				(at -20.32 -5.08 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "109")
			)
			(pin no_connect line
				(at -20.32 -7.62 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "110")
			)
			(pin no_connect line
				(at -20.32 -12.7 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "111")
			)
			(pin no_connect line
				(at -20.32 -15.24 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "112")
			)
			(pin no_connect line
				(at -20.32 -17.78 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "113")
			)
			(pin no_connect line
				(at -20.32 -20.32 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "114")
			)
			(pin no_connect line
				(at -20.32 -22.86 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "115")
			)
			(pin no_connect line
				(at -15.24 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "116")
			)
			(pin no_connect line
				(at -12.7 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "117")
			)
			(pin no_connect line
				(at -10.16 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "118")
			)
			(pin no_connect line
				(at -7.62 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "119")
			)
			(pin no_connect line
				(at -5.08 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "120")
			)
			(pin no_connect line
				(at -2.54 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "121")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "1")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "11")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "14")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "17")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "21")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "27")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "31")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "36")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "41")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "44")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "47")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "5")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "50")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "52")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "56")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "6")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "60")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "62")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "63")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "65")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "66")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "68")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "69")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "7")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "72")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "74")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "75")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "76")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "77")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "78")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "79")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "8")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "80")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "81")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "82")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "85")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "9")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "90")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "94")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "GND_Shield")
				(number "98")
			)
			(pin no_connect line
				(at 2.54 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "122")
			)
			(pin no_connect line
				(at 5.08 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "123")
			)
			(pin no_connect line
				(at 7.62 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "124")
			)
			(pin no_connect line
				(at 10.16 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "125")
			)
			(pin no_connect line
				(at 12.7 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "126")
			)
			(pin no_connect line
				(at 15.24 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "127")
			)
		)
		(symbol "nRF9160-SIxA_1_1"
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "ENABLE")
				(number "101")
			)
			(pin input line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "~{RESET}")
				(number "32")
			)
			(pin input line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "SWDCLK")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "SWDIO")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "COEX0")
				(number "93")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "COEX1")
				(number "92")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "COEX2")
				(number "91")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "ANT")
				(number "61")
			)
			(pin passive line
				(at -25.4 0 0)
				(length 5.08)
				(name "AUX")
				(number "64")
			)
			(pin passive line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "GPS")
				(number "67")
			)
			(pin power_out line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "SIM_1V8")
				(number "49")
			)
			(pin output line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "SIM_CLK")
				(number "46")
			)
			(pin output line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "SIM_RST")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "SIM_IO")
				(number "48")
			)
			(pin power_out line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "VIO")
				(number "57")
			)
			(pin output line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "SCLK")
				(number "58")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "SDATA")
				(number "59")
			)
			(pin no_connect line
				(at -20.32 -35.56 0)
				(length 5.08)
				(hide yes)
				(name "SIM_DET")
				(number "45")
			)
			(pin passive line
				(at -5.08 53.34 270)
				(length 5.08)
				(name "DEC0")
				(number "13")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VDD1")
				(number "102")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "103")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDD2")
				(number "22")
			)
			(pin power_in line
				(at 7.62 53.34 270)
				(length 5.08)
				(name "VDD_GPIO")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "P0.00")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "P0.01")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "P0.02")
				(number "97")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "P0.03")
				(number "99")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "P0.04")
				(number "100")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "P0.05")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "P0.06")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "P0.07")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "P0.08")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "P0.09")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "P0.10")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "P0.11")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "P0.12")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "AIN0/P0.13")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "AIN1/P0.14")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "AIN2/P0.15")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "AIN3/P0.16")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "AIN4/P0.17")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "AIN5/P0.18")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "AIN6/P0.19")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "AIN7/P0.20")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "TRACECLK/P0.21")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "TRACEDATA0/P0.22")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "TRACEDATA1/P0.23")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "TRACEDATA2/P0.24")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "TRACEDATA3/P0.25")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "P0.26")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "P0.27")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "P0.28")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "P0.29")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "P0.30")
				(number "88")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "P0.31")
				(number "89")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "MAGPIO0")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "MAGPIO1")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "MAGPIO2")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
)
