(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "P8X32A-D40"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "P8X32A-D40"
			(at 1.27 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "https://www.parallax.com/sites/default/files/downloads/P8X32A-Propeller-Datasheet-v1.4.0_0.pdf"
			(at 0 0 0)
		)
		(property "Description" "Parallax Propeller 8 core, 32 bit, 80 MHz microcontroller, 3.3VDC, 40-pin DIP"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller multicore Parallax Propeller DIP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*40*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "P8X32A-D40_0_1"
			(text "SCL"
				(at 8.89 -15.24 0)
			)
			(text "SDA"
				(at 8.89 -17.78 0)
			)
			(text "TX"
				(at 8.89 -20.32 0)
			)
			(text "RX"
				(at 8.89 -22.86 0)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "~{RES}")
				(number "11")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "~{BOE}")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "P0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "P1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "P2")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P3")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "P4")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P5")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P6")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P7")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P8")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P9")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P10")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "P11")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "P12")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "P13")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "P14")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "P15")
				(number "20")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin input line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "XI")
				(number "30")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "XO")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "P16")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "P17")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "P18")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "P19")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "P20")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "P21")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "P22")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "P23")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "P24")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "P25")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "P26")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "P27")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "P28")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "P29")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "P30")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "P31")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "P8X32A-M44"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "P8X32A-M44"
			(at 3.81 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_9x9mm_P0.65mm_EP7.5x7.5mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "https://www.parallax.com/sites/default/files/downloads/P8X32A-Propeller-Datasheet-v1.4.0_0.pdf"
			(at 0 0 0)
		)
		(property "Description" "Parallax Propeller 8 core, 32 bit, 80 MHz microcontroller, 3.3VDC, 44-pin QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller multicore Parallax Propeller QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*44*1EP*9x9mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "P8X32A-M44_0_1"
			(text "SCL"
				(at 8.89 -15.24 0)
			)
			(text "SDA"
				(at 8.89 -17.78 0)
			)
			(text "TX"
				(at 8.89 -20.32 0)
			)
			(text "RX"
				(at 8.89 -22.86 0)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "~{RES}")
				(number "7")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "~{BOE}")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "P0")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "P1")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "P2")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P3")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "P4")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P5")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P6")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P7")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P8")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P9")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P10")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "P11")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "P12")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "P13")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "P14")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "P15")
				(number "16")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "27")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "45")
			)
			(pin input line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "XI")
				(number "28")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "XO")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "P16")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "P17")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "P18")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "P19")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "P20")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "P21")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "P22")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "P23")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "P24")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "P25")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "P26")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "P27")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "P28")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "P29")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "P30")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "P31")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "P8X32A-Q44"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "P8X32A-Q44"
			(at 3.81 25.4 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 0 30.48 0)
		)
		(property "Datasheet" "https://www.parallax.com/sites/default/files/downloads/P8X32A-Propeller-Datasheet-v1.4.0_0.pdf"
			(at 0 0 0)
		)
		(property "Description" "Parallax Propeller 8 core, 32 bit, 80 MHz microcontroller, 3.3VDC, 44-pin LQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller multicore Parallax Propeller LQFP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "P8X32A-Q44_0_1"
			(text "SCL"
				(at 8.89 -15.24 0)
			)
			(text "SDA"
				(at 8.89 -17.78 0)
			)
			(text "TX"
				(at 8.89 -20.32 0)
			)
			(text "RX"
				(at 8.89 -22.86 0)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "~{RES}")
				(number "7")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "~{BOE}")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "P0")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "P1")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "P2")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P3")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "P4")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P5")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P6")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P7")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P8")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P9")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P10")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "P11")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "P12")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "P13")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "P14")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "P15")
				(number "16")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "27")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin input line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "XI")
				(number "28")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "XO")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "P16")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "P17")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "P18")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "P19")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "P20")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "P21")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "P22")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "P23")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "P24")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "P25")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "P26")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "P27")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "P28")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "P29")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "P30")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "P31")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
)
