(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PY32F002AF15P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.638 0)
		)
		(property "Value" "PY32F002AF15P"
			(at 8.636 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0.254 -37.846 0)
		)
		(property "Datasheet" "https://www.puyasemi.com/download_path/%E6%95%B0%E6%8D%AE%E6%89%8B%E5%86%8C/MCU%20%E5%BE%AE%E5%A4%84%E7%90%86%E5%99%A8/PY32F002A_Datasheet_V0.2.pdf"
			(at 0 -42.926 0)
		)
		(property "Description" "Puya PY32 ARM Cortex-M0 MCU, 20 KB Flash, 3 KB RAM, 24 MHz, 1.7-5.5V, 18 GPIO, TSSOP20"
			(at 0 -40.386 0)
		)
		(property "ki_keywords" "puya py32 arm cortex-m0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PY32F002AF15P_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PF0/OSCIN")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF1/OSCOUT")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF2/~{RST}")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB6/PF4/BOOT0")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13/SWD")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14/SWC")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB2")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
)
