(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "RP2040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 45.72 0)
		)
		(property "Value" "RP2040"
			(at 17.78 43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "A microcontroller by Raspberry Pi"
			(at 0 0 0)
		)
		(property "ki_keywords" "RP2040 ARM Cortex-M0+ USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm?P0.4mm*"
			(at 0 0 0)
		)
		(symbol "RP2040_0_1")
		(symbol "RP2040_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "RUN")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "USB_DP")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "USB_DM")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "QSPI_SS")
				(number "56")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "QSPI_SD0")
				(number "53")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "QSPI_SD1")
				(number "55")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "QSPI_SD2")
				(number "54")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "QSPI_SD3")
				(number "51")
			)
			(pin output line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "QSPI_SCLK")
				(number "52")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "XIN")
				(number "20")
			)
			(pin passive line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "XOUT")
				(number "21")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "SWCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "SWD")
				(number "25")
			)
			(pin input line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "TESTEN")
				(number "19")
			)
			(pin power_out line
				(at -5.08 45.72 270)
				(length 3.81)
				(name "VREG_VOUT")
				(number "45")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "DVDD")
				(number "23")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "DVDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "IOVDD")
				(number "1")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "IOVDD")
				(number "10")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "IOVDD")
				(number "22")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "IOVDD")
				(number "33")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "IOVDD")
				(number "42")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "IOVDD")
				(number "49")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 3.81)
				(name "USB_VDD")
				(number "48")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 3.81)
				(name "ADC_AVDD")
				(number "43")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 3.81)
				(name "VREG_IN")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "GPIO0")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "GPIO1")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "GPIO2")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "GPIO3")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "GPIO4")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "GPIO5")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "GPIO6")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "GPIO7")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "GPIO8")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "GPIO9")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "GPIO10")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "GPIO11")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "GPIO12")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "GPIO13")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "GPIO14")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "GPIO15")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "GPIO16")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "GPIO17")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "GPIO18")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "GPIO19")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "GPIO20")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "GPIO21")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "GPIO22")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "GPIO23")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "GPIO24")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "GPIO25")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "GPIO26_ADC0")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "GPIO27_ADC1")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "GPIO28_ADC2")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "GPIO29_ADC3")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
)
