(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "R7FS12878xA01CFL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 36.83 0)
		)
		(property "Value" "R7FS12878xA01CFL"
			(at 8.89 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -7.62 -38.1 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/doc/products/renesas-synergy/doc/r01ds0309eu0100-synergy-s128.pdf"
			(at 1.27 10.16 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 32MHz, 256KB Flash, 24KB RAM, 1.65-3.6V, 37 GPIO, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "R7FS12878xA01CFL_0_1")
		(symbol "R7FS12878xA01CFL_1_1"
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "P000")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "P001")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "P002")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "P010/VREFH0")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "P011/VREFL0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "P012")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "P013")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "P014")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "P015")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "P200")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "P201/MD")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "P206")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "P212/EXTAL")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "P213/XTAL")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "P214/XCOUT")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "P215/XCIN")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "P400")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "P401")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "P407")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "P408")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "P409")
				(number "10")
			)
			(pin passive line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "VCL")
				(number "3")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "30")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "AVCC0")
				(number "42")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "AVSS0")
				(number "43")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VCC_USB_LDO")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSS_USB")
				(number "13")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VCC_USB")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "P100")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "P101")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "P102")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "P103")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "P104")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SWDIO/P108")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "P109")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "P110")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "P111")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "P112")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "SWCLK/P300")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "P301")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "P302")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "P500")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "USB_DP/P914")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "USB_DM/P915")
				(number "14")
			)
			(pin input line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "RES")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
)
