(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32C011D6Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 13.97 0)
		)
		(property "Value" "STM32C011D6Yx"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-12_1.7x1.42mm_Layout4x6_P0.35mm_Stagger"
			(at -22.86 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011d6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 10 GPIO, WLCSP12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*1.7x1.42mm*Layout4x6*P0.35mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32C011D6Yx_0_1")
		(symbol "STM32C011D6Yx_1_1"
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "B3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "A4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB6")
				(number "A2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB7")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "E4")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA0/PA1/PA2/PF2")
				(number "F3")
				(alternate "ADC1_IN0 (PA0)" bidirectional line)
				(alternate "ADC1_IN1 (PA1)" bidirectional line)
				(alternate "ADC1_IN2 (PA2)" bidirectional line)
				(alternate "I2C1_SMBA (PA1)" bidirectional line)
				(alternate "I2S1_CK (PA1)" bidirectional line)
				(alternate "I2S1_SD (PA2)" bidirectional line)
				(alternate "PA0" bidirectional line)
				(alternate "PA1" bidirectional line)
				(alternate "PA2" bidirectional line)
				(alternate "PF2" bidirectional line)
				(alternate "PWR_WKUP1 (PA0)" bidirectional line)
				(alternate "PWR_WKUP4 (PA2)" bidirectional line)
				(alternate "RCC_LSCO (PA2)" bidirectional line)
				(alternate "RCC_MCO (PF2)" bidirectional line)
				(alternate "SPI1_MOSI (PA2)" bidirectional line)
				(alternate "SPI1_SCK (PA1)" bidirectional line)
				(alternate "TIM16_CH1 (PA0)" bidirectional line)
				(alternate "TIM16_CH1N (PA2)" bidirectional line)
				(alternate "TIM17_CH1 (PA1)" bidirectional line)
				(alternate "TIM1_CH1 (PA0)" bidirectional line)
				(alternate "TIM1_CH2 (PA1)" bidirectional line)
				(alternate "TIM1_CH3 (PA2)" bidirectional line)
				(alternate "TIM1_CH4 (PF2)" bidirectional line)
				(alternate "TIM3_ETR (PA2)" bidirectional line)
				(alternate "USART1_RX (PA1)" bidirectional line)
				(alternate "USART1_TX (PA0)" bidirectional line)
				(alternate "USART2_CK (PA1)" bidirectional line)
				(alternate "USART2_CTS (PA0)" bidirectional line)
				(alternate "USART2_DE (PA1)" bidirectional line)
				(alternate "USART2_NSS (PA0)" bidirectional line)
				(alternate "USART2_RTS (PA1)" bidirectional line)
				(alternate "USART2_TX (PA2)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA3/PA4/PA5/PA6")
				(number "F1")
				(alternate "ADC1_IN3 (PA3)" bidirectional line)
				(alternate "ADC1_IN4 (PA4)" bidirectional line)
				(alternate "ADC1_IN5 (PA5)" bidirectional line)
				(alternate "ADC1_IN6 (PA6)" bidirectional line)
				(alternate "I2S1_CK (PA5)" bidirectional line)
				(alternate "I2S1_MCK (PA6)" bidirectional line)
				(alternate "I2S1_WS (PA4)" bidirectional line)
				(alternate "PA3" bidirectional line)
				(alternate "PA4" bidirectional line)
				(alternate "PA5" bidirectional line)
				(alternate "PA6" bidirectional line)
				(alternate "PWR_WKUP2 (PA4)" bidirectional line)
				(alternate "RTC_OUT1 (PA4)" bidirectional line)
				(alternate "RTC_TS (PA4)" bidirectional line)
				(alternate "SPI1_MISO (PA6)" bidirectional line)
				(alternate "SPI1_NSS (PA4)" bidirectional line)
				(alternate "SPI1_SCK (PA5)" bidirectional line)
				(alternate "TIM14_CH1 (PA4)" bidirectional line)
				(alternate "TIM16_CH1 (PA6)" bidirectional line)
				(alternate "TIM17_CH1N (PA4)" bidirectional line)
				(alternate "TIM1_BKIN (PA6)" bidirectional line)
				(alternate "TIM1_CH1 (PA5)" bidirectional line)
				(alternate "TIM1_CH1N (PA3)" bidirectional line)
				(alternate "TIM1_CH2N (PA4)" bidirectional line)
				(alternate "TIM1_CH3N (PA5)" bidirectional line)
				(alternate "TIM1_CH4 (PA3)" bidirectional line)
				(alternate "TIM3_CH1 (PA6)" bidirectional line)
				(alternate "USART2_RX (PA3)" bidirectional line)
				(alternate "USART2_RX (PA5)" bidirectional line)
				(alternate "USART2_TX (PA4)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA7/PA10/PA12")
				(number "E2")
				(alternate "ADC1_IN12 (PA12)" bidirectional line)
				(alternate "ADC1_IN7 (PA7)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA7)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "PA7" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI1_MOSI (PA7)" bidirectional line)
				(alternate "TIM14_CH1 (PA7)" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM17_CH1 (PA7)" bidirectional line)
				(alternate "TIM1_CH1N (PA7)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "TIM3_CH2 (PA7)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA8/PA9/PA11")
				(number "D1")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN11 (PA11)" bidirectional line)
				(alternate "ADC1_IN8 (PA8)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S1_WS (PA8)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "RCC_MCO_2 (PA8)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI1_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_BKIN2 (PA11)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH2N (PA8)" bidirectional line)
				(alternate "TIM1_CH3N (PA8)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TIM3_CH3 (PA8)" bidirectional line)
				(alternate "TIM3_CH4 (PA8)" bidirectional line)
				(alternate "TIM3_ETR (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_RX (PA8)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USART2_TX (PA8)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "B1")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C2")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C011F_4-6_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C011F_4-6_Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32C011F_4-6_Px_0_1")
		(symbol "STM32C011F_4-6_Px_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB6")
				(number "20")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB7")
				(number "1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "16")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "TIM1_BKIN2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TIM3_ETR (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "17")
				(alternate "ADC1_IN12 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "19")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C011F_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C011F_4-6_Ux"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, UFQFPN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C011F_4-6_Ux_0_1")
		(symbol "STM32C011F_4-6_Ux_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "4")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB6")
				(number "18")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "9")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA6")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "14")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "TIM1_BKIN2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TIM3_ETR (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "15")
				(alternate "ADC1_IN12 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "16")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C011J_4-6_Mx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 11.43 0)
		)
		(property "Value" "STM32C011J_4-6_Mx"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -22.86 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011j4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 6 GPIO, SO8N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STM32C011J_4-6_Mx_0_1")
		(symbol "STM32C011J_4-6_Mx_1_1"
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB7/PC14")
				(number "1")
				(alternate "I2C1_SCL (PB7)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "I2C1_SDA (PC14)" bidirectional line)
				(alternate "IR_OUT (PC14)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSCX_IN (PC14)" bidirectional line)
				(alternate "RTC_REFIN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB7)" bidirectional line)
				(alternate "TIM17_CH1 (PC14)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "TIM1_BKIN2 (PC14)" bidirectional line)
				(alternate "TIM1_CH4 (PB7)" bidirectional line)
				(alternate "TIM1_ETR (PC14)" bidirectional line)
				(alternate "TIM3_CH1 (PB7)" bidirectional line)
				(alternate "TIM3_CH2 (PC14)" bidirectional line)
				(alternate "TIM3_CH4 (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
				(alternate "USART1_TX (PC14)" bidirectional line)
				(alternate "USART2_CK (PC14)" bidirectional line)
				(alternate "USART2_CTS (PB7)" bidirectional line)
				(alternate "USART2_DE (PC14)" bidirectional line)
				(alternate "USART2_NSS (PB7)" bidirectional line)
				(alternate "USART2_RTS (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA0/PA1/PA2/PF2")
				(number "4")
				(alternate "ADC1_IN0 (PA0)" bidirectional line)
				(alternate "ADC1_IN1 (PA1)" bidirectional line)
				(alternate "ADC1_IN2 (PA2)" bidirectional line)
				(alternate "I2C1_SMBA (PA1)" bidirectional line)
				(alternate "I2S1_CK (PA1)" bidirectional line)
				(alternate "I2S1_SD (PA2)" bidirectional line)
				(alternate "PA0" bidirectional line)
				(alternate "PA1" bidirectional line)
				(alternate "PA2" bidirectional line)
				(alternate "PF2" bidirectional line)
				(alternate "PWR_WKUP1 (PA0)" bidirectional line)
				(alternate "PWR_WKUP4 (PA2)" bidirectional line)
				(alternate "RCC_LSCO (PA2)" bidirectional line)
				(alternate "RCC_MCO (PF2)" bidirectional line)
				(alternate "SPI1_MOSI (PA2)" bidirectional line)
				(alternate "SPI1_SCK (PA1)" bidirectional line)
				(alternate "TIM16_CH1 (PA0)" bidirectional line)
				(alternate "TIM16_CH1N (PA2)" bidirectional line)
				(alternate "TIM17_CH1 (PA1)" bidirectional line)
				(alternate "TIM1_CH1 (PA0)" bidirectional line)
				(alternate "TIM1_CH2 (PA1)" bidirectional line)
				(alternate "TIM1_CH3 (PA2)" bidirectional line)
				(alternate "TIM1_CH4 (PF2)" bidirectional line)
				(alternate "TIM3_ETR (PA2)" bidirectional line)
				(alternate "USART1_RX (PA1)" bidirectional line)
				(alternate "USART1_TX (PA0)" bidirectional line)
				(alternate "USART2_CK (PA1)" bidirectional line)
				(alternate "USART2_CTS (PA0)" bidirectional line)
				(alternate "USART2_DE (PA1)" bidirectional line)
				(alternate "USART2_NSS (PA0)" bidirectional line)
				(alternate "USART2_RTS (PA1)" bidirectional line)
				(alternate "USART2_TX (PA2)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA8/PA9/PA11")
				(number "5")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN11 (PA11)" bidirectional line)
				(alternate "ADC1_IN8 (PA8)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S1_WS (PA8)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "RCC_MCO_2 (PA8)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI1_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_BKIN2 (PA11)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH2N (PA8)" bidirectional line)
				(alternate "TIM1_CH3N (PA8)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TIM3_CH3 (PA8)" bidirectional line)
				(alternate "TIM3_CH4 (PA8)" bidirectional line)
				(alternate "TIM3_ETR (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_RX (PA8)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USART2_TX (PA8)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "6")
				(alternate "ADC1_IN12 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "7")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA14/PB6/PC15")
				(number "8")
				(alternate "ADC1_IN14 (PA14)" bidirectional line)
				(alternate "DEBUG_SWCLK (PA14)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB6)" bidirectional line)
				(alternate "I2S1_CK (PB6)" bidirectional line)
				(alternate "I2S1_MCK (PB6)" bidirectional line)
				(alternate "I2S1_SD (PB6)" bidirectional line)
				(alternate "I2S1_WS (PA14)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "PC15" bidirectional line)
				(alternate "PWR_WKUP3 (PB6)" bidirectional line)
				(alternate "RCC_MCO_2 (PA14)" bidirectional line)
				(alternate "RCC_OSC32_EN (PC15)" bidirectional line)
				(alternate "RCC_OSCX_OUT (PC15)" bidirectional line)
				(alternate "RCC_OSC_EN (PC15)" bidirectional line)
				(alternate "SPI1_MISO (PB6)" bidirectional line)
				(alternate "SPI1_MOSI (PB6)" bidirectional line)
				(alternate "SPI1_NSS (PA14)" bidirectional line)
				(alternate "SPI1_SCK (PB6)" bidirectional line)
				(alternate "TIM16_BKIN (PB6)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BKIN (PB6)" bidirectional line)
				(alternate "TIM1_CH1 (PA14)" bidirectional line)
				(alternate "TIM1_CH2 (PB6)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM1_ETR (PC15)" bidirectional line)
				(alternate "TIM3_CH1 (PB6)" bidirectional line)
				(alternate "TIM3_CH2 (PB6)" bidirectional line)
				(alternate "TIM3_CH3 (PB6)" bidirectional line)
				(alternate "TIM3_CH3 (PC15)" bidirectional line)
				(alternate "USART1_CK (PA14)" bidirectional line)
				(alternate "USART1_CK (PB6)" bidirectional line)
				(alternate "USART1_CTS (PB6)" bidirectional line)
				(alternate "USART1_DE (PA14)" bidirectional line)
				(alternate "USART1_DE (PB6)" bidirectional line)
				(alternate "USART1_NSS (PB6)" bidirectional line)
				(alternate "USART1_RTS (PA14)" bidirectional line)
				(alternate "USART1_RTS (PB6)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
				(alternate "USART2_RX (PA14)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C031C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C031C_4-6_Tx"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 45 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C031C_4-6_Tx_0_1")
		(symbol "STM32C031C_4-6_Tx_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C031C_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C031C_4-6_Ux"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 45 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C031C_4-6_Ux_0_1")
		(symbol "STM32C031C_4-6_Ux_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C031F_4-6_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C031F_4-6_Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32C031F_4-6_Px_0_1")
		(symbol "STM32C031F_4-6_Px_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB6")
				(number "20")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB7")
				(number "1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "16")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "TIM1_BKIN2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TIM3_ETR (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "17")
				(alternate "ADC1_IN12 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "19")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C031G_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "STM32C031G_4-6_Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -7.62 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C031G_4-6_Ux_0_1")
		(symbol "STM32C031G_4-6_Ux_1_1"
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "18")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "19")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C031K_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C031K_4-6_Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32C031K_4-6_Tx_0_1")
		(symbol "STM32C031K_4-6_Tx_1_1"
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C031K_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C031K_4-6_Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C031K_4-6_Ux_0_1")
		(symbol "STM32C031K_4-6_Ux_1_1"
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071C8Tx"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 45 GPIO, LQFP48_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071C8Tx_0_1")
		(symbol "STM32C071C8Tx_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071C8TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071C8TxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -10.16 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 43 GPIO, LQFP48_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071C8TxN_0_1")
		(symbol "STM32C071C8TxN_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071C8Ux"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 45 GPIO, UFQFPN48_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071C8Ux_0_1")
		(symbol "STM32C071C8Ux_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071C8UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071C8UxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -10.16 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 43 GPIO, UFQFPN48_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071C8UxN_0_1")
		(symbol "STM32C071C8UxN_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071CBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071CBTx"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 45 GPIO, LQFP48_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071CBTx_0_1")
		(symbol "STM32C071CBTx_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071CBTxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071CBTxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -10.16 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 43 GPIO, LQFP48_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071CBTxN_0_1")
		(symbol "STM32C071CBTxN_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071CBUx"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 45 GPIO, UFQFPN48_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071CBUx_0_1")
		(symbol "STM32C071CBUx_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071CBUxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071CBUxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -10.16 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 43 GPIO, UFQFPN48_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071CBUxN_0_1")
		(symbol "STM32C071CBUxN_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071F8Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32C071F8Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 18 GPIO, TSSOP20_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071F8Px_0_1")
		(symbol "STM32C071F8Px_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2C1_SMBA (PB6)" bidirectional line)
				(alternate "I2C2_SCL (PB3)" bidirectional line)
				(alternate "I2C2_SDA (PB4)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_CK (PB6)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_MCK (PB6)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "I2S1_SD (PB6)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "PWR_WKUP3 (PB6)" bidirectional line)
				(alternate "PWR_WKUP6 (PB5)" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MISO (PB6)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_MOSI (PB6)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI1_SCK (PB6)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "TIM16_BKIN (PB5)" bidirectional line)
				(alternate "TIM16_BKIN (PB6)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BKIN (PB4)" bidirectional line)
				(alternate "TIM17_BKIN (PB6)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH2 (PB6)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH1 (PB6)" bidirectional line)
				(alternate "TIM3_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "TIM3_CH2 (PB6)" bidirectional line)
				(alternate "TIM3_CH3 (PB5)" bidirectional line)
				(alternate "TIM3_CH3 (PB6)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_CTS (PB6)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_NSS (PB6)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "I2C1_SCL (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "RTC_REFIN (PB7)" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "TIM1_CH4 (PB7)" bidirectional line)
				(alternate "TIM3_CH1 (PB7)" bidirectional line)
				(alternate "TIM3_CH1 (PB8)" bidirectional line)
				(alternate "TIM3_CH4 (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
				(alternate "USART2_CTS (PB7)" bidirectional line)
				(alternate "USART2_CTS (PB8)" bidirectional line)
				(alternate "USART2_NSS (PB7)" bidirectional line)
				(alternate "USART2_NSS (PB8)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "16")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "17")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN14 (PA14)" bidirectional line)
				(alternate "DEBUG_SWCLK (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "RCC_MCO2 (PA14)" bidirectional line)
				(alternate "RCC_MCO2 (PA15)" bidirectional line)
				(alternate "SPI1_NSS (PA14)" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "TIM1_CH1 (PA14)" bidirectional line)
				(alternate "TIM1_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART1_CK (PA14)" bidirectional line)
				(alternate "USART1_CK (PA15)" bidirectional line)
				(alternate "USART1_DE (PA14)" bidirectional line)
				(alternate "USART1_DE (PA15)" bidirectional line)
				(alternate "USART1_RTS (PA14)" bidirectional line)
				(alternate "USART1_RTS (PA15)" bidirectional line)
				(alternate "USART2_RX (PA14)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
				(alternate "USB_NOE (PA15)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071F8PxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32C071F8PxN"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 17 GPIO, TSSOP20_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071F8PxN_0_1")
		(symbol "STM32C071F8PxN_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2C1_SMBA (PB6)" bidirectional line)
				(alternate "I2C2_SCL (PB3)" bidirectional line)
				(alternate "I2C2_SDA (PB4)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_CK (PB6)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_MCK (PB6)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "I2S1_SD (PB6)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "PWR_WKUP3 (PB6)" bidirectional line)
				(alternate "PWR_WKUP6 (PB5)" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MISO (PB6)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_MOSI (PB6)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI1_SCK (PB6)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "TIM16_BKIN (PB5)" bidirectional line)
				(alternate "TIM16_BKIN (PB6)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BKIN (PB4)" bidirectional line)
				(alternate "TIM17_BKIN (PB6)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH2 (PB6)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH1 (PB6)" bidirectional line)
				(alternate "TIM3_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "TIM3_CH2 (PB6)" bidirectional line)
				(alternate "TIM3_CH3 (PB5)" bidirectional line)
				(alternate "TIM3_CH3 (PB6)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_CTS (PB6)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_NSS (PB6)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "I2C1_SCL (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "RTC_REFIN (PB7)" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "TIM1_CH4 (PB7)" bidirectional line)
				(alternate "TIM3_CH1 (PB7)" bidirectional line)
				(alternate "TIM3_CH1 (PB8)" bidirectional line)
				(alternate "TIM3_CH4 (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
				(alternate "USART2_CTS (PB7)" bidirectional line)
				(alternate "USART2_CTS (PB8)" bidirectional line)
				(alternate "USART2_NSS (PB7)" bidirectional line)
				(alternate "USART2_NSS (PB8)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDIO2")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "16")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "17")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN14 (PA14)" bidirectional line)
				(alternate "DEBUG_SWCLK (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "RCC_MCO2 (PA14)" bidirectional line)
				(alternate "RCC_MCO2 (PA15)" bidirectional line)
				(alternate "SPI1_NSS (PA14)" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "TIM1_CH1 (PA14)" bidirectional line)
				(alternate "TIM1_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART1_CK (PA14)" bidirectional line)
				(alternate "USART1_CK (PA15)" bidirectional line)
				(alternate "USART1_DE (PA14)" bidirectional line)
				(alternate "USART1_DE (PA15)" bidirectional line)
				(alternate "USART1_RTS (PA14)" bidirectional line)
				(alternate "USART1_RTS (PA15)" bidirectional line)
				(alternate "USART2_RX (PA14)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
				(alternate "USB_NOE (PA15)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071FBPx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32C071FBPx"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 18 GPIO, TSSOP20_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071FBPx_0_1")
		(symbol "STM32C071FBPx_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2C1_SMBA (PB6)" bidirectional line)
				(alternate "I2C2_SCL (PB3)" bidirectional line)
				(alternate "I2C2_SDA (PB4)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_CK (PB6)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_MCK (PB6)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "I2S1_SD (PB6)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "PWR_WKUP3 (PB6)" bidirectional line)
				(alternate "PWR_WKUP6 (PB5)" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MISO (PB6)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_MOSI (PB6)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI1_SCK (PB6)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "TIM16_BKIN (PB5)" bidirectional line)
				(alternate "TIM16_BKIN (PB6)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BKIN (PB4)" bidirectional line)
				(alternate "TIM17_BKIN (PB6)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH2 (PB6)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH1 (PB6)" bidirectional line)
				(alternate "TIM3_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "TIM3_CH2 (PB6)" bidirectional line)
				(alternate "TIM3_CH3 (PB5)" bidirectional line)
				(alternate "TIM3_CH3 (PB6)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_CTS (PB6)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_NSS (PB6)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "I2C1_SCL (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "RTC_REFIN (PB7)" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "TIM1_CH4 (PB7)" bidirectional line)
				(alternate "TIM3_CH1 (PB7)" bidirectional line)
				(alternate "TIM3_CH1 (PB8)" bidirectional line)
				(alternate "TIM3_CH4 (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
				(alternate "USART2_CTS (PB7)" bidirectional line)
				(alternate "USART2_CTS (PB8)" bidirectional line)
				(alternate "USART2_NSS (PB7)" bidirectional line)
				(alternate "USART2_NSS (PB8)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "16")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "17")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN14 (PA14)" bidirectional line)
				(alternate "DEBUG_SWCLK (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "RCC_MCO2 (PA14)" bidirectional line)
				(alternate "RCC_MCO2 (PA15)" bidirectional line)
				(alternate "SPI1_NSS (PA14)" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "TIM1_CH1 (PA14)" bidirectional line)
				(alternate "TIM1_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART1_CK (PA14)" bidirectional line)
				(alternate "USART1_CK (PA15)" bidirectional line)
				(alternate "USART1_DE (PA14)" bidirectional line)
				(alternate "USART1_DE (PA15)" bidirectional line)
				(alternate "USART1_RTS (PA14)" bidirectional line)
				(alternate "USART1_RTS (PA15)" bidirectional line)
				(alternate "USART2_RX (PA14)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
				(alternate "USB_NOE (PA15)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071FBPxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32C071FBPxN"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 17 GPIO, TSSOP20_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071FBPxN_0_1")
		(symbol "STM32C071FBPxN_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2C1_SMBA (PB6)" bidirectional line)
				(alternate "I2C2_SCL (PB3)" bidirectional line)
				(alternate "I2C2_SDA (PB4)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_CK (PB6)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_MCK (PB6)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "I2S1_SD (PB6)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "PWR_WKUP3 (PB6)" bidirectional line)
				(alternate "PWR_WKUP6 (PB5)" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MISO (PB6)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_MOSI (PB6)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI1_SCK (PB6)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "TIM16_BKIN (PB5)" bidirectional line)
				(alternate "TIM16_BKIN (PB6)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BKIN (PB4)" bidirectional line)
				(alternate "TIM17_BKIN (PB6)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH2 (PB6)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH1 (PB6)" bidirectional line)
				(alternate "TIM3_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "TIM3_CH2 (PB6)" bidirectional line)
				(alternate "TIM3_CH3 (PB5)" bidirectional line)
				(alternate "TIM3_CH3 (PB6)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_CTS (PB6)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_NSS (PB6)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "I2C1_SCL (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "RTC_REFIN (PB7)" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "TIM1_CH4 (PB7)" bidirectional line)
				(alternate "TIM3_CH1 (PB7)" bidirectional line)
				(alternate "TIM3_CH1 (PB8)" bidirectional line)
				(alternate "TIM3_CH4 (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
				(alternate "USART2_CTS (PB7)" bidirectional line)
				(alternate "USART2_CTS (PB8)" bidirectional line)
				(alternate "USART2_NSS (PB7)" bidirectional line)
				(alternate "USART2_NSS (PB8)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDIO2")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "16")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "17")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN14 (PA14)" bidirectional line)
				(alternate "DEBUG_SWCLK (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "RCC_MCO2 (PA14)" bidirectional line)
				(alternate "RCC_MCO2 (PA15)" bidirectional line)
				(alternate "SPI1_NSS (PA14)" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "TIM1_CH1 (PA14)" bidirectional line)
				(alternate "TIM1_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART1_CK (PA14)" bidirectional line)
				(alternate "USART1_CK (PA15)" bidirectional line)
				(alternate "USART1_DE (PA14)" bidirectional line)
				(alternate "USART1_DE (PA15)" bidirectional line)
				(alternate "USART1_RTS (PA14)" bidirectional line)
				(alternate "USART1_RTS (PA15)" bidirectional line)
				(alternate "USART2_RX (PA14)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
				(alternate "USB_NOE (PA15)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071G8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "STM32C071G8Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -7.62 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 26 GPIO, UFQFPN28_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071G8Ux_0_1")
		(symbol "STM32C071G8Ux_1_1"
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "18")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "19")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071G8UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32C071G8UxN"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 25 GPIO, UFQFPN28_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071G8UxN_0_1")
		(symbol "STM32C071G8UxN_1_1"
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDIO2")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "18")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "19")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071GBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "STM32C071GBUx"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -7.62 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071gb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 26 GPIO, UFQFPN28_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071GBUx_0_1")
		(symbol "STM32C071GBUx_1_1"
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "18")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "19")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071GBUxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32C071GBUxN"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071gb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 25 GPIO, UFQFPN28_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071GBUxN_0_1")
		(symbol "STM32C071GBUxN_1_1"
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDIO2")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "18")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "19")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071K8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C071K8Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 30 GPIO, LQFP32_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071K8Tx_0_1")
		(symbol "STM32C071K8Tx_1_1"
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071K8TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32C071K8TxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 29 GPIO, LQFP32_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071K8TxN_0_1")
		(symbol "STM32C071K8TxN_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071K8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C071K8Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 30 GPIO, UFQFPN32_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071K8Ux_0_1")
		(symbol "STM32C071K8Ux_1_1"
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071K8UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32C071K8UxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 29 GPIO, UFQFPN32_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071K8UxN_0_1")
		(symbol "STM32C071K8UxN_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071KBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C071KBTx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 30 GPIO, LQFP32_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071KBTx_0_1")
		(symbol "STM32C071KBTx_1_1"
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071KBTxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32C071KBTxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 29 GPIO, LQFP32_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071KBTxN_0_1")
		(symbol "STM32C071KBTxN_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071KBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C071KBUx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 30 GPIO, UFQFPN32_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071KBUx_0_1")
		(symbol "STM32C071KBUx_1_1"
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071KBUxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32C071KBUxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 29 GPIO, UFQFPN32_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071KBUxN_0_1")
		(symbol "STM32C071KBUxN_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "21")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071R8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071R8Tx"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 61 GPIO, LQFP64_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071R8Tx_0_1")
		(symbol "STM32C071R8Tx_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "40")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "41")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -40.64 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "42")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "43")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "44")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071R8TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071R8TxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 24KB RAM, 59 GPIO, LQFP64_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071R8TxN_0_1")
		(symbol "STM32C071R8TxN_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC0")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC1")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "41")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "42")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "43")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "44")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071RBIxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071RBIxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 59 GPIO, UFBGA64_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071RBIxN_0_1")
		(symbol "STM32C071RBIxN_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "D2")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "G1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "D3")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "A7")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "A6")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "C5")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "B5")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "A5")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC1")
				(number "F2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PC2")
				(number "G2")
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PC3")
				(number "H1")
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PC6")
				(number "E7")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PC7")
				(number "E5")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PC8")
				(number "A8")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PC9")
				(number "B7")
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PC11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PC13")
				(number "C2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "E1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "D8")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "H2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "F8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D7")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C7")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H7")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "B4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G6")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G7")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071RBTx"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 61 GPIO, LQFP64_GP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071RBTx_0_1")
		(symbol "STM32C071RBTx_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "40")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "41")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -40.64 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "42")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "43")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "44")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C071RBTxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C071RBTxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 59 GPIO, LQFP64_N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32C071RBTxN_0_1")
		(symbol "STM32C071RBTxN_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "PF3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC0")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC1")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "RCC_OSCX_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSCX_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "41")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "42")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "43")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "44")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "DEBUG_SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "DEBUG_SWCLK" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN19" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN20" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN21" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN22" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32C011F4Px"
		(extends "STM32C011F_4-6_Px")
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C011F4Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C011F4Ux"
		(extends "STM32C011F_4-6_Ux")
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C011F4Ux"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, UFQFPN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C011F6Px"
		(extends "STM32C011F_4-6_Px")
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C011F6Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C011F6Ux"
		(extends "STM32C011F_4-6_Ux")
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C011F6Ux"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, UFQFPN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C011J4Mx"
		(extends "STM32C011J_4-6_Mx")
		(property "Reference" "U"
			(at -22.86 11.43 0)
		)
		(property "Value" "STM32C011J4Mx"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -22.86 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011j4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 6 GPIO, SO8N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C011J6Mx"
		(extends "STM32C011J_4-6_Mx")
		(property "Reference" "U"
			(at -22.86 11.43 0)
		)
		(property "Value" "STM32C011J6Mx"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -22.86 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c011j6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 6 GPIO, SO8N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031C4Tx"
		(extends "STM32C031C_4-6_Tx")
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C031C4Tx"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 45 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031C4Ux"
		(extends "STM32C031C_4-6_Ux")
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C031C4Ux"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 45 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031C6Tx"
		(extends "STM32C031C_4-6_Tx")
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C031C6Tx"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 45 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031C6Ux"
		(extends "STM32C031C_4-6_Ux")
		(property "Reference" "U"
			(at -10.16 46.99 0)
		)
		(property "Value" "STM32C031C6Ux"
			(at 2.54 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -10.16 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 45 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031F4Px"
		(extends "STM32C031F_4-6_Px")
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C031F4Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031F6Px"
		(extends "STM32C031F_4-6_Px")
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32C031F6Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031G4Ux"
		(extends "STM32C031G_4-6_Ux")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "STM32C031G4Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -7.62 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031G6Ux"
		(extends "STM32C031G_4-6_Ux")
		(property "Reference" "U"
			(at -7.62 24.13 0)
		)
		(property "Value" "STM32C031G6Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -7.62 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031K4Tx"
		(extends "STM32C031K_4-6_Tx")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C031K4Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031K4Ux"
		(extends "STM32C031K_4-6_Ux")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C031K4Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031K6Tx"
		(extends "STM32C031K_4-6_Tx")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C031K6Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32C031K6Ux"
		(extends "STM32C031K_4-6_Ux")
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "STM32C031K6Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -7.62 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 48 MHz, 2.0-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
