(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32F030C6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F030C6Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f030c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 2.4-3.6V, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F030C6Tx_0_1")
		(symbol "STM32F030C6Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F030C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F030C8Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f030c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.4-3.6V, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F030C8Tx_0_1")
		(symbol "STM32F030C8Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F030CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F030CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f030cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.4-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F030CCTx_0_1")
		(symbol "STM32F030CCTx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F030F4Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32F030F4Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f030f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 4KB RAM, 48 MHz, 2.4-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32F030F4Px_0_1")
		(symbol "STM32F030F4Px_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "18")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F030K6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F030K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f030k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 2.4-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F030K6Tx_0_1")
		(symbol "STM32F030K6Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F030R8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "STM32F030R8Tx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -12.7 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f030r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.4-3.6V, 55 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F030R8Tx_0_1")
		(symbol "STM32F030R8Tx_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF4")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF5")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC11")
				(number "52")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F030RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F030RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f030rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.4-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F030RCTx_0_1")
		(symbol "STM32F030RCTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F031C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F031C_4-6_Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F031C_4-6_Tx_0_1")
		(symbol "STM32F031C_4-6_Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F031E6Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32F031E6Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die444"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031e6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 20 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die444*"
			(at 0 0 0)
		)
		(symbol "STM32F031E6Yx_0_1")
		(symbol "STM32F031E6Yx_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "C5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "A4")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PF0")
				(number "A5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PF1")
				(number "B5")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB0")
				(number "E3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB1")
				(number "E2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "C2")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "B2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "E1")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "D5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "B4")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "C4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "D4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "E5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "B3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "C3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "D3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "D2")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA9")
				(number "C1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA10")
				(number "B1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "A2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F031F_4-6_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32F031F_4-6_Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32F031F_4-6_Px_0_1")
		(symbol "STM32F031F_4-6_Px_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "18")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F031G_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32F031G_4-6_Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 23 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F031G_4-6_Ux_0_1")
		(symbol "STM32F031G_4-6_Ux_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "25")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "26")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F031K6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F031K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F031K6Tx_0_1")
		(symbol "STM32F031K6Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F031K_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F031K_4-6_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F031K_4-6_Ux_0_1")
		(symbol "STM32F031K_4-6_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F038C6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "STM32F038C6Tx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f038c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 1.65-1.95V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F038C6Tx_0_1")
		(symbol "STM32F038C6Tx_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F038E6Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32F038E6Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die444"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f038e6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 1.65-1.95V, 20 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die444*"
			(at 0 0 0)
		)
		(symbol "STM32F038E6Yx_0_1")
		(symbol "STM32F038E6Yx_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "C5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "A4")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PF0")
				(number "A5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PF1")
				(number "B5")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB0")
				(number "E3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB1")
				(number "E2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "C2")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "B2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "E1")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "D5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "B4")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "C4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "D4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "E5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "B3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "C3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "D3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "D2")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA9")
				(number "C1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA10")
				(number "B1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "A2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F038F6Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32F038F6Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f038f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 1.65-1.95V, 14 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32F038F6Px_0_1")
		(symbol "STM32F038F6Px_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "NPOR")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "18")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F038G6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32F038G6Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f038g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 1.65-1.95V, 22 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F038G6Ux_0_1")
		(symbol "STM32F038G6Ux_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "NPOR")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "25")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "26")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F038K6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F038K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f038k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 1.65-1.95V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F038K6Ux_0_1")
		(symbol "STM32F038K6Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "NPOR")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F042C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F042C_4-6_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F042C_4-6_Tx_0_1")
		(symbol "STM32F042C_4-6_Tx_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF11")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F042C_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F042C_4-6_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F042C_4-6_Ux_0_1")
		(symbol "STM32F042C_4-6_Ux_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF11")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F042F4Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32F042F4Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 16 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32F042F4Px_0_1")
		(symbol "STM32F042F4Px_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB8")
				(number "1")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSSA")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "17")
				(alternate "CAN_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TSC_G4_IO1 (PA9)" bidirectional line)
				(alternate "TSC_G4_IO3 (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "18")
				(alternate "CAN_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "TSC_G4_IO2 (PA10)" bidirectional line)
				(alternate "TSC_G4_IO4 (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F042F6Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32F042F6Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 16 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32F042F6Px_0_1")
		(symbol "STM32F042F6Px_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB8")
				(number "1")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSSA")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "17")
				(alternate "CAN_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TSC_G4_IO1 (PA9)" bidirectional line)
				(alternate "TSC_G4_IO3 (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "18")
				(alternate "CAN_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "TSC_G4_IO2 (PA10)" bidirectional line)
				(alternate "TSC_G4_IO4 (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F042G_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "STM32F042G_4-6_Ux"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -17.78 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 23 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F042G_4-6_Ux_0_1")
		(symbol "STM32F042G_4-6_Ux_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "25")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "26")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "1")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDIO2")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "19")
				(alternate "CAN_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TSC_G4_IO1 (PA9)" bidirectional line)
				(alternate "TSC_G4_IO3 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "20")
				(alternate "CAN_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "TSC_G4_IO2 (PA10)" bidirectional line)
				(alternate "TSC_G4_IO4 (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F042K_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32F042K_4-6_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F042K_4-6_Tx_0_1")
		(symbol "STM32F042K_4-6_Tx_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB8")
				(number "31")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F042K_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32F042K_4-6_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16-32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 28 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F042K_4-6_Ux_0_1")
		(symbol "STM32F042K_4-6_Ux_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PF11")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F042T6Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "STM32F042T6Yx"
			(at 5.08 29.21 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die445"
			(at -10.16 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042t6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 30 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die445*"
			(at 0 0 0)
		)
		(symbol "STM32F042T6Yx_0_1")
		(symbol "STM32F042T6Yx_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF0")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF1")
				(number "C5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "A6")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "F2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "D2")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "B3")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "E6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "B4")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "A5")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "E5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "F1")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E1")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "VSSA")
				(number "D6")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "D4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "E4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "C3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "D3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA8")
				(number "E2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "A1")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "B1")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F048C6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F048C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f048c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 1.65-1.95V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F048C6Ux_0_1")
		(symbol "STM32F048C6Ux_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF11")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F048G6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "STM32F048G6Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -17.78 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f048g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 1.65-1.95V, 22 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F048G6Ux_0_1")
		(symbol "STM32F048G6Ux_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "NPOR")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "25")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "26")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "27")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "1")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDIO2")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "19")
				(alternate "I2C1_SCL (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TSC_G4_IO1 (PA9)" bidirectional line)
				(alternate "TSC_G4_IO3 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "20")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "TSC_G4_IO2 (PA10)" bidirectional line)
				(alternate "TSC_G4_IO4 (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F048T6Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "STM32F048T6Yx"
			(at 5.08 29.21 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die445"
			(at -10.16 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f048t6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 1.65-1.95V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die445*"
			(at 0 0 0)
		)
		(symbol "STM32F048T6Yx_0_1")
		(symbol "STM32F048T6Yx_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "NPOR")
				(number "D2")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF0")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PF1")
				(number "C5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "A6")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "F2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB3")
				(number "B3")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB5")
				(number "E6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "PB8")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "A5")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "E5")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E1")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "D4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "E4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "C3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "D3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA8")
				(number "E2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "A1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "B1")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051C4Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F051C4Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051C4Tx_0_1")
		(symbol "STM32F051C4Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051C4Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F051C4Ux"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051C4Ux_0_1")
		(symbol "STM32F051C4Ux_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051C6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F051C6Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051C6Tx_0_1")
		(symbol "STM32F051C6Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051C6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F051C6Ux"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051C6Ux_0_1")
		(symbol "STM32F051C6Ux_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F051C8Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051C8Tx_0_1")
		(symbol "STM32F051C8Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F051C8Ux"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051C8Ux_0_1")
		(symbol "STM32F051C8Ux_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051K4Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F051K4Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051K4Tx_0_1")
		(symbol "STM32F051K4Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051K4Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F051K4Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051K4Ux_0_1")
		(symbol "STM32F051K4Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051K6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F051K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051K6Tx_0_1")
		(symbol "STM32F051K6Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051K6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F051K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051K6Ux_0_1")
		(symbol "STM32F051K6Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051K8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F051K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051K8Tx_0_1")
		(symbol "STM32F051K8Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051K8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F051K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051K8Ux_0_1")
		(symbol "STM32F051K8Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051R4Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "STM32F051R4Tx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -12.7 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 55 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051R4Tx_0_1")
		(symbol "STM32F051R4Tx_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF4")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF5")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "47")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "48")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC11")
				(number "52")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051R6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "STM32F051R6Tx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -12.7 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 55 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051R6Tx_0_1")
		(symbol "STM32F051R6Tx_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF4")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF5")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "47")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "48")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC11")
				(number "52")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051R8Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "STM32F051R8Hx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -12.7 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 55 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051R8Hx_0_1")
		(symbol "STM32F051R8Hx_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF4")
				(number "C2")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF5")
				(number "D2")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "D6")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "E6")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051R8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "STM32F051R8Tx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -12.7 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 55 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F051R8Tx_0_1")
		(symbol "STM32F051R8Tx_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF4")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF5")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC11")
				(number "52")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F051T8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "STM32F051T8Yx"
			(at 5.08 29.21 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die440"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f051t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 2.0-3.6V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die440*"
			(at 0 0 0)
		)
		(symbol "STM32F051T8Yx_0_1")
		(symbol "STM32F051T8Yx_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PF0")
				(number "B5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF1")
				(number "C5")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "A6")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "F2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB2")
				(number "D2")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB3")
				(number "B3")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB5")
				(number "E6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "A5")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "F1")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "VSSA")
				(number "D6")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "D4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "E4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "C3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "D3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA8")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA12")
				(number "A1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "B1")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F058C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "STM32F058C8Ux"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f058c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 1.65-1.95V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F058C8Ux_0_1")
		(symbol "STM32F058C8Ux_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F058R8Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "STM32F058R8Hx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -12.7 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f058r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 1.65-1.95V, 54 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F058R8Hx_0_1")
		(symbol "STM32F058R8Hx_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "NPOR")
				(number "G6")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF4")
				(number "C2")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF5")
				(number "D2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF6")
				(number "D6")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PF7")
				(number "E6")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F058R8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "STM32F058R8Tx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -12.7 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f058r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 1.65-1.95V, 54 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F058R8Tx_0_1")
		(symbol "STM32F058R8Tx_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "NPOR")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF4")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF5")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF6")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PF7")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PC11")
				(number "52")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F058T8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "STM32F058T8Yx"
			(at 5.08 31.75 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die440"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f058t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 8KB RAM, 48 MHz, 1.65-1.95V, 28 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die440*"
			(at 0 0 0)
		)
		(symbol "STM32F058T8Yx_0_1")
		(symbol "STM32F058T8Yx_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "NPOR")
				(number "D2")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "B5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "C5")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PC13")
				(number "A6")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PC14")
				(number "B6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB1")
				(number "F2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB3")
				(number "B3")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB5")
				(number "E6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "A5")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "F1")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDA")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "VSSA")
				(number "D6")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "D4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "E4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "C3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "D3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA8")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA12")
				(number "A1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B1")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F070C6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F070C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f070c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.4-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F070C6Tx_0_1")
		(symbol "STM32F070C6Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F070CBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F070CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f070cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.4-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F070CBTx_0_1")
		(symbol "STM32F070CBTx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F070F6Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "STM32F070F6Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -15.24 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f070f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.4-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32F070F6Px_0_1")
		(symbol "STM32F070F6Px_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "17")
				(alternate "I2C1_SCL (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "18")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "TIM17_BKIN (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F070RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F070RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f070rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.4-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F070RBTx_0_1")
		(symbol "STM32F070RBTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F071CBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F071CBYx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die448"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die448*"
			(at 0 0 0)
		)
		(symbol "STM32F071CBYx_0_1")
		(symbol "STM32F071CBYx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "D6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "D5")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "C7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "G5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "G4")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "G3")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "D4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "C5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "G2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "E2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B6")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "B7")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "F2")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "A6")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D3")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "E6")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "G7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "G6")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "B3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F071C_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F071C_8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F071C_8-B_Tx_0_1")
		(symbol "STM32F071C_8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F071C_8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F071C_8-B_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F071C_8-B_Ux_0_1")
		(symbol "STM32F071C_8-B_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F071RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F071RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F071RBTx_0_1")
		(symbol "STM32F071RBTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F071V_8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F071V_8-B_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F071V_8-B_Hx_0_1")
		(symbol "STM32F071V_8-B_Hx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "SYS_WKUP8" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF3")
				(number "L1")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E3")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "G11")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F071V_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F071V_8-B_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F071V_8-B_Tx_0_1")
		(symbol "STM32F071V_8-B_Tx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "SYS_WKUP8" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF3")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF6")
				(number "73")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F072CBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F072CBYx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die448"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die448*"
			(at 0 0 0)
		)
		(symbol "STM32F072CBYx_0_1")
		(symbol "STM32F072CBYx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "D6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "D5")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "C7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "G5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "G4")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "G3")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "D4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "C5")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "G2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "E2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B6")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "B7")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "F2")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "A6")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D3")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "E6")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "G7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "G6")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "B3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F072C_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F072C_8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F072C_8-B_Tx_0_1")
		(symbol "STM32F072C_8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F072C_8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F072C_8-B_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F072C_8-B_Ux_0_1")
		(symbol "STM32F072C_8-B_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F072RBHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F072RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F072RBHx_0_1")
		(symbol "STM32F072RBHx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F072RBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F072RBIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F072RBIx_0_1")
		(symbol "STM32F072RBIx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F072R_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F072R_8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F072R_8-B_Tx_0_1")
		(symbol "STM32F072R_8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F072V_8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F072V_8-B_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F072V_8-B_Hx_0_1")
		(symbol "STM32F072V_8-B_Hx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "SYS_WKUP8" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF3")
				(number "L1")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E3")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "G11")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F072V_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F072V_8-B_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64-128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F072V_8-B_Tx_0_1")
		(symbol "STM32F072V_8-B_Tx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "SYS_WKUP8" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF3")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF6")
				(number "73")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F078CBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 41.91 0)
		)
		(property "Value" "STM32F078CBTx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f078cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 1.65-1.95V, 36 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F078CBTx_0_1")
		(symbol "STM32F078CBTx_1_1"
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F078CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 41.91 0)
		)
		(property "Value" "STM32F078CBUx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f078cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 1.65-1.95V, 36 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F078CBUx_0_1")
		(symbol "STM32F078CBUx_1_1"
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F078CBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 41.91 0)
		)
		(property "Value" "STM32F078CBYx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die448"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f078cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 1.65-1.95V, 36 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die448*"
			(at 0 0 0)
		)
		(symbol "STM32F078CBYx_0_1")
		(symbol "STM32F078CBYx_1_1"
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "NPOR")
				(number "G3")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF0")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF1")
				(number "D6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "D5")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "C7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "G5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "G4")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "D4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "C5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "G2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "E2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "B6")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "B7")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "F2")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "A6")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D3")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "E6")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDIO2")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "G7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "G6")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "B3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F078RBHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F078RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f078rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 1.65-1.95V, 50 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F078RBHx_0_1")
		(symbol "STM32F078RBHx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NPOR")
				(number "G6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F078RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F078RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f078rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 1.65-1.95V, 50 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F078RBTx_0_1")
		(symbol "STM32F078RBTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NPOR")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F078VBHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 67.31 0)
		)
		(property "Value" "STM32F078VBHx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f078vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 1.65-1.95V, 86 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F078VBHx_0_1")
		(symbol "STM32F078VBHx_1_1"
			(pin input line
				(at -20.32 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -20.32 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "NPOR")
				(number "L6")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "SYS_WKUP8" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF3")
				(number "L1")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E3")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDIO2")
				(number "G11")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F078VBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 67.31 0)
		)
		(property "Value" "STM32F078VBTx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f078vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 1.65-1.95V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F078VBTx_0_1")
		(symbol "STM32F078VBTx_1_1"
			(pin input line
				(at -20.32 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "NPOR")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "SYS_WKUP8" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF3")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF6")
				(number "73")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDIO2")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F091C_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F091C_B-C_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128-256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F091C_B-C_Tx_0_1")
		(symbol "STM32F091C_B-C_Tx_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF11")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F091C_B-C_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F091C_B-C_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128-256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F091C_B-C_Ux_0_1")
		(symbol "STM32F091C_B-C_Ux_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF11")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F091RCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F091RCHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F091RCHx_0_1")
		(symbol "STM32F091RCHx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF11")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F091RCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F091RCYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die442"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 52 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die442*"
			(at 0 0 0)
		)
		(symbol "STM32F091RCYx_0_1")
		(symbol "STM32F091RCYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "D7")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "D8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "E8")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF11")
				(number "C6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "A4")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "E7")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "E6")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "F4")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "D1")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "E2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "E3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "A3")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "C4")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "B4")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "C8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "C7")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B8")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "G8")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H6")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B3")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "G4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H4")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "D4")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "D5")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "B5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "A6")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H3")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "G1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F091R_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F091R_B-C_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128-256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F091R_B-C_Tx_0_1")
		(symbol "STM32F091R_B-C_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF11")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F091VCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F091VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 88 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F091VCHx_0_1")
		(symbol "STM32F091VCHx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "SYS_WKUP8" bidirectional line)
				(alternate "USART7_CK" bidirectional line)
				(alternate "USART7_DE" bidirectional line)
				(alternate "USART7_RTS" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF3")
				(number "L1")
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF11")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART8_CK" bidirectional line)
				(alternate "USART8_DE" bidirectional line)
				(alternate "USART8_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TSC_G8_IO2" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TSC_G8_IO3" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USART7_CK" bidirectional line)
				(alternate "USART7_DE" bidirectional line)
				(alternate "USART7_RTS" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E3")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "G11")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F091V_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F091V_B-C_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128-256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 88 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F091V_B-C_Tx_0_1")
		(symbol "STM32F091V_B-C_Tx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "SYS_WKUP8" bidirectional line)
				(alternate "USART7_CK" bidirectional line)
				(alternate "USART7_DE" bidirectional line)
				(alternate "USART7_RTS" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF3")
				(number "22")
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF6")
				(number "73")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF11")
				(number "94")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART8_CK" bidirectional line)
				(alternate "USART8_DE" bidirectional line)
				(alternate "USART8_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TSC_G8_IO2" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TSC_G8_IO3" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USART7_CK" bidirectional line)
				(alternate "USART7_DE" bidirectional line)
				(alternate "USART7_RTS" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F098CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F098CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f098cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 1.65-1.95V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F098CCTx_0_1")
		(symbol "STM32F098CCTx_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF11")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F098CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F098CCUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f098cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 1.65-1.95V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F098CCUx_0_1")
		(symbol "STM32F098CCUx_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF11")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F098RCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F098RCHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f098rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 1.65-1.95V, 51 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F098RCHx_0_1")
		(symbol "STM32F098RCHx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "NPOR")
				(number "G6")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF11")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F098RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F098RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f098rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 1.65-1.95V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F098RCTx_0_1")
		(symbol "STM32F098RCTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "NPOR")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF11")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F098RCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F098RCYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die442"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f098rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 1.65-1.95V, 51 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die442*"
			(at 0 0 0)
		)
		(symbol "STM32F098RCYx_0_1")
		(symbol "STM32F098RCYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "D7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "NPOR")
				(number "H4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "D8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "E8")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF11")
				(number "C6")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "A4")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "E7")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "E6")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "F4")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "D1")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "E3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "A3")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "C4")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "B4")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "C8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "C7")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B8")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "G8")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F7")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H6")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B3")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "G4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "D4")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "D5")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "A5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "B5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "A6")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "H3")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "G1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F098VCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 67.31 0)
		)
		(property "Value" "STM32F098VCHx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f098vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 1.65-1.95V, 87 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F098VCHx_0_1")
		(symbol "STM32F098VCHx_1_1"
			(pin input line
				(at -20.32 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -20.32 55.88 0)
				(length 5.08)
				(name "NPOR")
				(number "L6")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "SYS_WKUP8" bidirectional line)
				(alternate "USART7_CK" bidirectional line)
				(alternate "USART7_DE" bidirectional line)
				(alternate "USART7_RTS" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF3")
				(number "L1")
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PF11")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART8_CK" bidirectional line)
				(alternate "USART8_DE" bidirectional line)
				(alternate "USART8_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TSC_G8_IO2" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TSC_G8_IO3" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USART7_CK" bidirectional line)
				(alternate "USART7_DE" bidirectional line)
				(alternate "USART7_RTS" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E3")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDIO2")
				(number "G11")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F098VCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 67.31 0)
		)
		(property "Value" "STM32F098VCTx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f098vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 1.65-1.95V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F098VCTx_0_1")
		(symbol "STM32F098VCTx_1_1"
			(pin input line
				(at -20.32 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 55.88 0)
				(length 5.08)
				(name "NPOR")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "SYS_WKUP8" bidirectional line)
				(alternate "USART7_CK" bidirectional line)
				(alternate "USART7_DE" bidirectional line)
				(alternate "USART7_RTS" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF3")
				(number "22")
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "73")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PF11")
				(number "94")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART8_CK" bidirectional line)
				(alternate "USART8_DE" bidirectional line)
				(alternate "USART8_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TSC_G8_IO2" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TSC_G8_IO3" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USART7_CK" bidirectional line)
				(alternate "USART7_DE" bidirectional line)
				(alternate "USART7_RTS" bidirectional line)
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDIO2")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP7" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F031C4Tx"
		(extends "STM32F031C_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F031C4Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F031C6Tx"
		(extends "STM32F031C_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32F031C6Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F031F4Px"
		(extends "STM32F031F_4-6_Px")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32F031F4Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F031F6Px"
		(extends "STM32F031F_4-6_Px")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32F031F6Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F031G4Ux"
		(extends "STM32F031G_4-6_Ux")
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32F031G4Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 23 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F031G6Ux"
		(extends "STM32F031G_4-6_Ux")
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32F031G6Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 23 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F031K4Ux"
		(extends "STM32F031K_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F031K4Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F031K6Ux"
		(extends "STM32F031K_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F031K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042C4Tx"
		(extends "STM32F042C_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F042C4Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042C4Ux"
		(extends "STM32F042C_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F042C4Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042C6Tx"
		(extends "STM32F042C_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F042C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042C6Ux"
		(extends "STM32F042C_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F042C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042G4Ux"
		(extends "STM32F042G_4-6_Ux")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "STM32F042G4Ux"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -17.78 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 23 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042G6Ux"
		(extends "STM32F042G_4-6_Ux")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "STM32F042G6Ux"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -17.78 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 23 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042K4Tx"
		(extends "STM32F042K_4-6_Tx")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32F042K4Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042K4Ux"
		(extends "STM32F042K_4-6_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32F042K4Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 16KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 28 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042K6Tx"
		(extends "STM32F042K_4-6_Tx")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32F042K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F042K6Ux"
		(extends "STM32F042K_4-6_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32F042K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f042k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 28 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F071C8Tx"
		(extends "STM32F071C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F071C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F071C8Ux"
		(extends "STM32F071C_8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F071C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F071CBTx"
		(extends "STM32F071C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F071CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F071CBUx"
		(extends "STM32F071C_8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F071CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F071V8Hx"
		(extends "STM32F071V_8-B_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F071V8Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F071V8Tx"
		(extends "STM32F071V_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F071V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F071VBHx"
		(extends "STM32F071V_8-B_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F071VBHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F071VBTx"
		(extends "STM32F071V_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F071VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f071vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072C8Tx"
		(extends "STM32F072C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F072C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072C8Ux"
		(extends "STM32F072C_8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F072C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072CBTx"
		(extends "STM32F072C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F072CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072CBUx"
		(extends "STM32F072C_8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F072CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072R8Tx"
		(extends "STM32F072R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F072R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072RBTx"
		(extends "STM32F072R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F072RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072V8Hx"
		(extends "STM32F072V_8-B_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F072V8Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072V8Tx"
		(extends "STM32F072V_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F072V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 64KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072VBHx"
		(extends "STM32F072V_8-B_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F072VBHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F072VBTx"
		(extends "STM32F072V_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F072VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f072vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F091CBTx"
		(extends "STM32F091C_B-C_Tx")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F091CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F091CBUx"
		(extends "STM32F091C_B-C_Ux")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F091CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F091CCTx"
		(extends "STM32F091C_B-C_Tx")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F091CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F091CCUx"
		(extends "STM32F091C_B-C_Ux")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32F091CCUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F091RBTx"
		(extends "STM32F091R_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F091RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F091RCTx"
		(extends "STM32F091R_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F091RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F091VBTx"
		(extends "STM32F091V_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F091VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 128KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 88 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F091VCTx"
		(extends "STM32F091V_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F091VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f091vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0 MCU, 256KB flash, 32KB RAM, 48 MHz, 2.0-3.6V, 88 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0 STM32F0 STM32F0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
