(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32F100C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F100C_4-6_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100C_4-6_Tx_0_1")
		(symbol "STM32F100C_4-6_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100C_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F100C_8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100C_8-B_Tx_0_1")
		(symbol "STM32F100C_8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100R_4-6_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R_4-6_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100R_4-6_Hx_0_1")
		(symbol "STM32F100R_4-6_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100R_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R_4-6_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100R_4-6_Tx_0_1")
		(symbol "STM32F100R_4-6_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100R_8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R_8-B_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100R_8-B_Hx_0_1")
		(symbol "STM32F100R_8-B_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100R_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R_8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100R_8-B_Tx_0_1")
		(symbol "STM32F100R_8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100R_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R_C-D-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 24-32KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100R_C-D-E_Tx_0_1")
		(symbol "STM32F100R_C-D-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100V_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F100V_8-B_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100V_8-B_Tx_0_1")
		(symbol "STM32F100V_8-B_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100V_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F100V_C-D-E_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 24-32KB RAM, 24 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100V_C-D-E_Tx_0_1")
		(symbol "STM32F100V_C-D-E_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100Z_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F100Z_C-D-E_Tx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 24-32KB RAM, 24 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F100Z_C-D-E_Tx_0_1")
		(symbol "STM32F100Z_C-D-E_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OSC_IN")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF6")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "106")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "CEC" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101C_4-6_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 4-6KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101C_4-6_Tx_0_1")
		(symbol "STM32F101C_4-6_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101C_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101C_8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101C_8-B_Tx_0_1")
		(symbol "STM32F101C_8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101C_8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101C_8-B_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101C_8-B_Ux_0_1")
		(symbol "STM32F101C_8-B_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101RBHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 36 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101RBHx_0_1")
		(symbol "STM32F101RBHx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101R_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101R_4-6_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 4-6KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101R_4-6_Tx_0_1")
		(symbol "STM32F101R_4-6_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101R_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101R_8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101R_8-B_Tx_0_1")
		(symbol "STM32F101R_8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101R_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101R_C-D-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 32-48KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101R_C-D-E_Tx_0_1")
		(symbol "STM32F101R_C-D-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101R_F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101R_F-G_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101rf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768-1024KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101R_F-G_Tx_0_1")
		(symbol "STM32F101R_F-G_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101T_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F101T_4-6_Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101t4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 4-6KB RAM, 36 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101T_4-6_Ux_0_1")
		(symbol "STM32F101T_4-6_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PD0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PD1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "30")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "31")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "32")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "33")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "34")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "5")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "20")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "21")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "22")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "24")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "25")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "28")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101T_8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F101T_8-B_Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 36 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101T_8-B_Ux_0_1")
		(symbol "STM32F101T_8-B_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PD0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PD1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "30")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "31")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "32")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "33")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "34")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "5")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "20")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "21")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "22")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "24")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "25")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "28")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101V_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101V_8-B_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101V_8-B_Tx_0_1")
		(symbol "STM32F101V_8-B_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101V_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101V_C-D-E_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 32-48KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101V_C-D-E_Tx_0_1")
		(symbol "STM32F101V_C-D-E_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101V_F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101V_F-G_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101vf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768-1024KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101V_F-G_Tx_0_1")
		(symbol "STM32F101V_F-G_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101Z_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F101Z_C-D-E_Tx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 32-48KB RAM, 36 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101Z_C-D-E_Tx_0_1")
		(symbol "STM32F101Z_C-D-E_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OSC_IN")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FSMC_INT3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "FSMC_NIORD" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "FSMC_NREG" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "FSMC_NIOWR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_NIOS16" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "106")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F101Z_F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F101Z_F-G_Tx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101zf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768-1024KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F101Z_F-G_Tx_0_1")
		(symbol "STM32F101Z_F-G_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OSC_IN")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FSMC_INT3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_NIOS16" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "106")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F102C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F102C_4-6_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 4-6KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F102C_4-6_Tx_0_1")
		(symbol "STM32F102C_4-6_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F102C_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F102C_8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F102C_8-B_Tx_0_1")
		(symbol "STM32F102C_8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F102R_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F102R_4-6_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 4-6KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F102R_4-6_Tx_0_1")
		(symbol "STM32F102R_4-6_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F102R_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F102R_8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F102R_8-B_Tx_0_1")
		(symbol "STM32F102R_8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103C6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F103C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103C6Ux_0_1")
		(symbol "STM32F103C6Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F103CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103CBUx_0_1")
		(symbol "STM32F103CBUx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F103C_4-6_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 6-10KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103C_4-6_Tx_0_1")
		(symbol "STM32F103C_4-6_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103C_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F103C_8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103C_8-B_Tx_0_1")
		(symbol "STM32F103C_8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103R_4-6_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R_4-6_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 6-10KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103R_4-6_Hx_0_1")
		(symbol "STM32F103R_4-6_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103R_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R_4-6_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 6-10KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103R_4-6_Tx_0_1")
		(symbol "STM32F103R_4-6_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103R_8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R_8-B_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103R_8-B_Hx_0_1")
		(symbol "STM32F103R_8-B_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103R_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R_8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103R_8-B_Tx_0_1")
		(symbol "STM32F103R_8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103R_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R_C-D-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 48-64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103R_C-D-E_Tx_0_1")
		(symbol "STM32F103R_C-D-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103R_C-D-E_Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R_C-D-E_Yx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die414"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 48-64KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die414*"
			(at 0 0 0)
		)
		(symbol "STM32F103R_C-D-E_Yx_0_1")
		(symbol "STM32F103R_C-D-E_Yx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "C7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A6")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "F7")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "D8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H6")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E3")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C4")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "C8")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "B8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "C6")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "E7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "G8")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E5")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "G4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E4")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D4")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "H4")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H3")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F2")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103R_F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R_F-G_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768-1024KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103R_F-G_Tx_0_1")
		(symbol "STM32F103R_F-G_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103T_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F103T_4-6_Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103t4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16-32KB flash, 6-10KB RAM, 72 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103T_4-6_Ux_0_1")
		(symbol "STM32F103T_4-6_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PD0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PD1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "30")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "31")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "32")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "33")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "34")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "5")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "20")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "21")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "22")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "24")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "25")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "28")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103T_8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F103T_8-B_Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103T_8-B_Ux_0_1")
		(symbol "STM32F103T_8-B_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PD0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PD1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "30")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "31")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "32")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "33")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "34")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "5")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "20")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "21")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "22")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "24")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "25")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "28")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103VBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VBIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103VBIx_0_1")
		(symbol "STM32F103VBIx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "CAN_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "CAN_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C11")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103V_8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103V_8-B_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103V_8-B_Hx_0_1")
		(symbol "STM32F103V_8-B_Hx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "D5")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "H1")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "D4")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "C4")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "A3")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "B3")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "C3")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "E3")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "H5")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "J5")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "K5")
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "G6")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "H6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "J6")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "K6")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "G7")
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "H7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "D8")
				(alternate "CAN_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "E8")
				(alternate "CAN_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "C7")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "D7")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "B6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "C6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "D6")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "H9")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "G9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "K10")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "J10")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "F8")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "G1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "J2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "K2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "G3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "H3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "J3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D9")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "C9")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "D10")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "B10")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A10")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A9")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "J4")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "G5")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A7")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A6")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "A5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "B4")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "J7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "K7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K8")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J8")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "H8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "G8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "F2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "E2")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "F3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "H4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F9")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E9")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "C8")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103V_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103V_8-B_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103V_8-B_Tx_0_1")
		(symbol "STM32F103V_8-B_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103V_C-D-E_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103V_C-D-E_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 48-64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103V_C-D-E_Hx_0_1")
		(symbol "STM32F103V_C-D-E_Hx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "D5")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "H1")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "D4")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "C4")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "A3")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "B3")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "C3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "E3")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "H5")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "J5")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "K5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "G6")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "H6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "J6")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "K6")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "G7")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "H7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "D8")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "E8")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "C7")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "D7")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "B6")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "C6")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "D6")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "H9")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "G9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "K10")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "J10")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "F8")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "G1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "J2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "K2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "G3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "H3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "J3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D9")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "C9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "D10")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "B10")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A10")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A9")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "J4")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "G5")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A7")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A6")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "A5")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "B4")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "J7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "K7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K8")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J8")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "H8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "G8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "F2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "E2")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "F3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "H4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F9")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B9")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "C8")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103V_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103V_C-D-E_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 48-64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103V_C-D-E_Tx_0_1")
		(symbol "STM32F103V_C-D-E_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103V_F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103V_F-G_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768-1024KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103V_F-G_Tx_0_1")
		(symbol "STM32F103V_F-G_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103Z_C-D-E_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103Z_C-D-E_Hx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 48-64KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103Z_C-D-E_Hx_0_1")
		(symbol "STM32F103Z_C-D-E_Hx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "F1")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "D5")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OSC_IN")
				(number "D1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "E1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "K6")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "J6")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "J12")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "J11")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "J10")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "H12")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "H11")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "H10")
				(alternate "FSMC_INT3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "G11")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "E8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "D7")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "C7")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "C3")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "C4")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "E2")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "E4")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF6")
				(number "F3")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "F2")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "G3")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "G2")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "G1")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "M5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_NIOS16" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "L5")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "K5")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "M6")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "L6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "A5")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A4")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "A3")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "B3")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "B4")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "K7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "J7")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "J8")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "K8")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "L8")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "M8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C11")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H5")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F9")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F10")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G5")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "J2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "K2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "L2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "M2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "M3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "E12")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "B12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A12")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A11")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "L4")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "J5")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A7")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A6")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "B6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "C6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "C5")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B5")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "M9")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "M10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "M11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "M12")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "L11")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "L12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "H2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "H3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "H4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "J4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "K4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "G12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "F12")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "F11")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "B10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "C10")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "A1")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "B1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "C1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "E10")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "D10")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "E9")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "D9")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "C9")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "B9")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "A8")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A9")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "L9")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J9")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "H9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "L10")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "K10")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "K11")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "K12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103Z_C-D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103Z_C-D-E_Tx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-512KB flash, 48-64KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103Z_C-D-E_Tx_0_1")
		(symbol "STM32F103Z_C-D-E_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OSC_IN")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FSMC_INT3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_NIOS16" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "106")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103Z_F-G_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103Z_F-G_Hx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768-1024KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103Z_F-G_Hx_0_1")
		(symbol "STM32F103Z_F-G_Hx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "F1")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "D5")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OSC_IN")
				(number "D1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "E1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "K6")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "J6")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "J12")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "J11")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "J10")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "H12")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "H11")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "H10")
				(alternate "FSMC_INT3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "G11")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "E8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "D7")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "C7")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "C3")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "C4")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "E2")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "E4")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF6")
				(number "F3")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "F2")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "G3")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "G2")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "G1")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "M5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_NIOS16" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "L5")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "K5")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "M6")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "L6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "A5")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A4")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "A3")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "B3")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "B4")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "K7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "J7")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "J8")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "K8")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "L8")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "M8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C11")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H5")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F9")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F10")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G5")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "J2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "K2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "L2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "M2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "M3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "E12")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "B12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A12")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A11")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "L4")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "J5")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A7")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A6")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "B6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "C6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "C5")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B5")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "M9")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "M10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "M11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "M12")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "L11")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "L12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "H2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "H3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "H4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "J4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "K4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "G12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "F12")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "F11")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "B10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "C10")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "A1")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "B1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "C1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "E10")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "D10")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "E9")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "D9")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "C9")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "B9")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "A8")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A9")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "L9")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J9")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "H9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "L10")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "K10")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "K11")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "K12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F103Z_F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103Z_F-G_Tx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768-1024KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F103Z_F-G_Tx_0_1")
		(symbol "STM32F103Z_F-G_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OSC_IN")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FSMC_INT3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_NIOS16" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "106")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "CAN_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "SDIO_D2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "SDIO_CK" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F105R_8-B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F105R_8-B-C_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F105R_8-B-C_Tx_0_1")
		(symbol "STM32F105R_8-B-C_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO" bidirectional line)
				(alternate "SYS_TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F105V_8-B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F105V_8-B-C_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F105V_8-B-C_Tx_0_1")
		(symbol "STM32F105V_8-B-C_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO" bidirectional line)
				(alternate "SYS_TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F105V_8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F105V_8-B_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F105V_8-B_Hx_0_1")
		(symbol "STM32F105V_8-B_Hx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "D5")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "H1")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "D4")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "C4")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "A3")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "B3")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "C3")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "E3")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "H5")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "J5")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "K5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "G6")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "H6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "J6")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "K6")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "G7")
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "H7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "D8")
				(alternate "CAN1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "E8")
				(alternate "CAN1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "C7")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "D7")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "B6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "C6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "D6")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "H9")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "G9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "K10")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "J10")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "F8")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "G1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "J2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "K2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "G3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "H3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "J3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D9")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "C9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "D10")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "B10")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A10")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A9")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "J4")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "G5")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A7")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO" bidirectional line)
				(alternate "SYS_TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A6")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "A5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "B4")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "J7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "K7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K8")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J8")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "H8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "G8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "F2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "E2")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "F3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "H4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F9")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B9")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "C8")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F107R_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F107R_B-C_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f107rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128-256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F107R_B-C_Tx_0_1")
		(symbol "STM32F107R_B-C_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PD0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO" bidirectional line)
				(alternate "SYS_TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F107VCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F107VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f107vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F107VCHx_0_1")
		(symbol "STM32F107VCHx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "D5")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "H1")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "D4")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "C4")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "A3")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "B3")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "C3")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "E3")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "H5")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "J5")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "K5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "G6")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "H6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "J6")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "K6")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "G7")
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "H7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "D8")
				(alternate "CAN1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "E8")
				(alternate "CAN1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "C7")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "D7")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "B6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "C6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "D6")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "H9")
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "G9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "K10")
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "J10")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "F8")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "G1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "J2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "K2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "G3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "H3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "J3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D9")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "C9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "D10")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "B10")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A10")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A9")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "J4")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "G5")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A7")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO" bidirectional line)
				(alternate "SYS_TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A6")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "A5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "B4")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "J7")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "K7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K8")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J8")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "H8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "G8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "F2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "E2")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "F3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "H4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F9")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B9")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "C8")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "B1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F107V_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F107V_B-C_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f107vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128-256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F107V_B-C_Tx_0_1")
		(symbol "STM32F107V_B-C_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "OSC_IN")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "OSC_OUT")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "SYS_TRACED3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "73")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO" bidirectional line)
				(alternate "SYS_TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT" bidirectional line)
				(alternate "RTC_TAMPER" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F100C4Tx"
		(extends "STM32F100C_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F100C4Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100C6Tx"
		(extends "STM32F100C_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F100C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100C8Tx"
		(extends "STM32F100C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F100C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100CBTx"
		(extends "STM32F100C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F100CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100R4Hx"
		(extends "STM32F100R_4-6_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R4Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100R4Tx"
		(extends "STM32F100R_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R4Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100R6Hx"
		(extends "STM32F100R_4-6_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R6Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100R6Tx"
		(extends "STM32F100R_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 4KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100R8Hx"
		(extends "STM32F100R_8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R8Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100R8Tx"
		(extends "STM32F100R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100RBHx"
		(extends "STM32F100R_8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100RBTx"
		(extends "STM32F100R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100RCTx"
		(extends "STM32F100R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 24KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100RDTx"
		(extends "STM32F100R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100RDTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 32KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100RETx"
		(extends "STM32F100R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F100RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 32KB RAM, 24 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100V8Tx"
		(extends "STM32F100V_8-B_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F100V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100VBTx"
		(extends "STM32F100V_8-B_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F100VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 8KB RAM, 24 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100VCTx"
		(extends "STM32F100V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F100VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 24KB RAM, 24 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100VDTx"
		(extends "STM32F100V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F100VDTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 32KB RAM, 24 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100VETx"
		(extends "STM32F100V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F100VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 32KB RAM, 24 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100ZCTx"
		(extends "STM32F100Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F100ZCTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 24KB RAM, 24 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100ZDTx"
		(extends "STM32F100Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F100ZDTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 32KB RAM, 24 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F100ZETx"
		(extends "STM32F100Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F100ZETx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f100ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 32KB RAM, 24 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101C4Tx"
		(extends "STM32F101C_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101C4Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 4KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101C6Tx"
		(extends "STM32F101C_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 6KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101C8Tx"
		(extends "STM32F101C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101C8Ux"
		(extends "STM32F101C_8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101CBTx"
		(extends "STM32F101C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101CBUx"
		(extends "STM32F101C_8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F101CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 36 MHz, 2.0-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101R4Tx"
		(extends "STM32F101R_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101R4Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 4KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101R6Tx"
		(extends "STM32F101R_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 6KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101R8Tx"
		(extends "STM32F101R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101RBTx"
		(extends "STM32F101R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101RCTx"
		(extends "STM32F101R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101RDTx"
		(extends "STM32F101R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101RDTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101RETx"
		(extends "STM32F101R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 48KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101RFTx"
		(extends "STM32F101R_F-G_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101RFTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101rf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101RGTx"
		(extends "STM32F101R_F-G_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F101RGTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101T4Ux"
		(extends "STM32F101T_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F101T4Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101t4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 4KB RAM, 36 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101T6Ux"
		(extends "STM32F101T_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F101T6Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101t6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 6KB RAM, 36 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101T8Ux"
		(extends "STM32F101T_8-B_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F101T8Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 36 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101TBUx"
		(extends "STM32F101T_8-B_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F101TBUx"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101tb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 36 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101V8Tx"
		(extends "STM32F101V_8-B_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101VBTx"
		(extends "STM32F101V_8-B_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101VCTx"
		(extends "STM32F101V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101VDTx"
		(extends "STM32F101V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101VDTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101VETx"
		(extends "STM32F101V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 48KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101VFTx"
		(extends "STM32F101V_F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101VFTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101vf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101VGTx"
		(extends "STM32F101V_F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F101VGTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101ZCTx"
		(extends "STM32F101Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F101ZCTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 36 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101ZDTx"
		(extends "STM32F101Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F101ZDTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 36 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101ZETx"
		(extends "STM32F101Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F101ZETx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 48KB RAM, 36 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101ZFTx"
		(extends "STM32F101Z_F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F101ZFTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101zf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F101ZGTx"
		(extends "STM32F101Z_F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F101ZGTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f101zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 80KB RAM, 36 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F101"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F102C4Tx"
		(extends "STM32F102C_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F102C4Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F102C6Tx"
		(extends "STM32F102C_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F102C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F102C8Tx"
		(extends "STM32F102C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F102C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F102CBTx"
		(extends "STM32F102C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F102CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F102R4Tx"
		(extends "STM32F102R_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F102R4Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 4KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F102R6Tx"
		(extends "STM32F102R_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F102R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 6KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F102R8Tx"
		(extends "STM32F102R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F102R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F102RBTx"
		(extends "STM32F102R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F102RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f102rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 48 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F102"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103C4Tx"
		(extends "STM32F103C_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F103C4Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 6KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103C6Tx"
		(extends "STM32F103C_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F103C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103C8Tx"
		(extends "STM32F103C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F103C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103CBTx"
		(extends "STM32F103C_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F103CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103R4Hx"
		(extends "STM32F103R_4-6_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R4Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 6KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103R4Tx"
		(extends "STM32F103R_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R4Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 6KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103R6Hx"
		(extends "STM32F103R_4-6_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R6Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103R6Tx"
		(extends "STM32F103R_4-6_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103R8Hx"
		(extends "STM32F103R_8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R8Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103R8Tx"
		(extends "STM32F103R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RBHx"
		(extends "STM32F103R_8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RBTx"
		(extends "STM32F103R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RCTx"
		(extends "STM32F103R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RCYx"
		(extends "STM32F103R_C-D-E_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RCYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die414"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die414*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RDTx"
		(extends "STM32F103R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RDTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RDYx"
		(extends "STM32F103R_C-D-E_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RDYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die414"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die414*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RETx"
		(extends "STM32F103R_C-D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103REYx"
		(extends "STM32F103R_C-D-E_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103REYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die414"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 50 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die414*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RFTx"
		(extends "STM32F103R_F-G_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RFTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103RGTx"
		(extends "STM32F103R_F-G_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F103RGTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103T4Ux"
		(extends "STM32F103T_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F103T4Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103t4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 16KB flash, 6KB RAM, 72 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103T6Ux"
		(extends "STM32F103T_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F103T6Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103t6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 72 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103T8Ux"
		(extends "STM32F103T_8-B_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F103T8Ux"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103TBUx"
		(extends "STM32F103T_8-B_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F103TBUx"
			(at 7.62 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103tb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103V8Hx"
		(extends "STM32F103V_8-B_Hx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103V8Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103V8Tx"
		(extends "STM32F103V_8-B_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VBHx"
		(extends "STM32F103V_8-B_Hx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VBHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VBTx"
		(extends "STM32F103V_8-B_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VCHx"
		(extends "STM32F103V_C-D-E_Hx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VCTx"
		(extends "STM32F103V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VDHx"
		(extends "STM32F103V_C-D-E_Hx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VDHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VDTx"
		(extends "STM32F103V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VDTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VEHx"
		(extends "STM32F103V_C-D-E_Hx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VEHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VETx"
		(extends "STM32F103V_C-D-E_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VFTx"
		(extends "STM32F103V_F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VFTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103VGTx"
		(extends "STM32F103V_F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F103VGTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZCHx"
		(extends "STM32F103Z_C-D-E_Hx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZCHx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZCTx"
		(extends "STM32F103Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZCTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZDHx"
		(extends "STM32F103Z_C-D-E_Hx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZDHx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZDTx"
		(extends "STM32F103Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZDTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZEHx"
		(extends "STM32F103Z_C-D-E_Hx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZEHx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZETx"
		(extends "STM32F103Z_C-D-E_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZETx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZFHx"
		(extends "STM32F103Z_F-G_Hx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZFHx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZFTx"
		(extends "STM32F103Z_F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZFTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZGHx"
		(extends "STM32F103Z_F-G_Hx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZGHx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F103ZGTx"
		(extends "STM32F103Z_F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F103ZGTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 96KB RAM, 72 MHz, 2.0-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F105R8Tx"
		(extends "STM32F105R_8-B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F105R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F105RBTx"
		(extends "STM32F105R_8-B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F105RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F105RCTx"
		(extends "STM32F105R_8-B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F105RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F105V8Hx"
		(extends "STM32F105V_8-B_Hx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F105V8Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F105V8Tx"
		(extends "STM32F105V_8-B-C_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F105V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F105VBHx"
		(extends "STM32F105V_8-B_Hx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F105VBHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:LFBGA-100_10x10mm_Layout10x10_P0.8mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFBGA*10x10mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F105VBTx"
		(extends "STM32F105V_8-B-C_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F105VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F105VCTx"
		(extends "STM32F105V_8-B-C_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F105VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f105vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F107RBTx"
		(extends "STM32F107R_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F107RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f107rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F107RCTx"
		(extends "STM32F107R_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F107RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f107rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F107VBTx"
		(extends "STM32F107V_B-C_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F107VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f107vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F107VCTx"
		(extends "STM32F107V_B-C_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F107VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f107vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F105/107"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
