(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32F205RGEx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F205RGEx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-66_Die411"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, EWLCSP66"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die411*"
			(at 0 0 0)
		)
		(symbol "STM32F205RGEx_0_1")
		(symbol "STM32F205RGEx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E8")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B6")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "F7")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "IRROFF")
				(number "C8")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "REGOFF")
				(number "H7")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PH0")
				(number "E9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PH1")
				(number "F9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD2")
				(number "C7")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC0")
				(number "G9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC2")
				(number "D7")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC3")
				(number "G8")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC5")
				(number "G3")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC7")
				(number "F2")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC8")
				(number "F3")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC11")
				(number "C3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC13")
				(number "B8")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC14")
				(number "B9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC15")
				(number "C9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "VCAP_1")
				(number "J3")
			)
			(pin power_out line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "VCAP_2")
				(number "C2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A9")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D9")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "J9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "H6")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "H5")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "J7")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "C1")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "J5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "J4")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A4")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B7")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "J2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "J1")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "H2")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "H1")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "G1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F205R_B-C-E-F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F205R_B-C-E-F-G_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128-1024KB flash, 64-128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F205R_B-C-E-F-G_Tx_0_1")
		(symbol "STM32F205R_B-C-E-F-G_Tx_1_1"
			(pin input line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "VCAP_1")
				(number "31")
			)
			(pin power_out line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "VCAP_2")
				(number "47")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F205R_E-G_Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F205R_E-G_Yx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-66_Die411"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, WLCSP66"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die411*"
			(at 0 0 0)
		)
		(symbol "STM32F205R_E-G_Yx_0_1")
		(symbol "STM32F205R_E-G_Yx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E8")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B6")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "F7")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "IRROFF")
				(number "C8")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "REGOFF")
				(number "H7")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PH0")
				(number "E9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PH1")
				(number "F9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD2")
				(number "C7")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC0")
				(number "G9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC2")
				(number "D7")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC3")
				(number "G8")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC5")
				(number "G3")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC6")
				(number "G2")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC7")
				(number "F2")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC8")
				(number "F3")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC11")
				(number "C3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC13")
				(number "B8")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC14")
				(number "B9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC15")
				(number "C9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "VCAP_1")
				(number "J3")
			)
			(pin power_out line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "VCAP_2")
				(number "C2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "A9")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D9")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "J9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "H6")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "H5")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "J7")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "C1")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "J5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "J4")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A4")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B7")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "J2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "J1")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "H2")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "H1")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "G1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F205V_B-C-E-F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F205V_B-C-E-F-G_Tx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128-1024KB flash, 64-128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F205V_B-C-E-F-G_Tx_0_1")
		(symbol "STM32F205V_B-C-E-F-G_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "VCAP_1")
				(number "49")
			)
			(pin power_out line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "VCAP_2")
				(number "73")
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "99")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F205Z_C-E-F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F205Z_C-E-F-G_Tx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-1024KB flash, 96-128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F205Z_C-E-F-G_Tx_0_1")
		(symbol "STM32F205Z_C-E-F-G_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FSMC_INT3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -68.58 0)
				(length 5.08)
				(name "VCAP_1")
				(number "71")
			)
			(pin power_out line
				(at -33.02 -71.12 0)
				(length 5.08)
				(name "VCAP_2")
				(number "106")
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "143")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F207I_C-E-F-G_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207I_C-E-F-G_Hx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ic.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32F207I_C-E-F-G_Hx_0_1")
		(symbol "STM32F207I_C-E-F-G_Hx_1_1"
			(pin input line
				(at -35.56 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -35.56 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "D6")
			)
			(pin input line
				(at -35.56 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "P1")
			)
			(pin input line
				(at -35.56 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "N1")
			)
			(pin input line
				(at -35.56 88.9 0)
				(length 5.08)
				(name "REGOFF")
				(number "L4")
			)
			(pin bidirectional line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "PI0")
				(number "E14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 81.28 0)
				(length 5.08)
				(name "PI1")
				(number "D14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "PI2")
				(number "C14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "PI3")
				(number "C13")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "PI4")
				(number "D4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "PI5")
				(number "C4")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 68.58 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PI7")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PI8")
				(number "D2")
				(alternate "RTC_AF2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "PI9")
				(number "D3")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PI10")
				(number "E3")
				(alternate "ETH_RX_ER" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PI11")
				(number "E4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PH0")
				(number "G1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PH1")
				(number "H1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PH2")
				(number "F4")
				(alternate "ETH_CRS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PH3")
				(number "G4")
				(alternate "ETH_COL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PH4")
				(number "H4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PH5")
				(number "J4")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PH6")
				(number "M11")
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PH7")
				(number "N12")
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PH10")
				(number "L13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PH11")
				(number "L12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PH12")
				(number "K12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PH13")
				(number "E12")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PH14")
				(number "E13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PH15")
				(number "D13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PG0")
				(number "N7")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PG1")
				(number "M7")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PG2")
				(number "L15")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PG3")
				(number "K15")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PG4")
				(number "K14")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PG5")
				(number "K13")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PG6")
				(number "J15")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PG7")
				(number "J14")
				(alternate "FSMC_INT3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PG8")
				(number "H14")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PG9")
				(number "C10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PG10")
				(number "B10")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PG11")
				(number "B9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "FSMC_NE4" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PG13")
				(number "A8")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FSMC_A24" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PG14")
				(number "A7")
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FSMC_A25" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FSMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PF1")
				(number "H3")
				(alternate "FSMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "FSMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PF3")
				(number "J2")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PF4")
				(number "J3")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PF5")
				(number "K3")
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PF6")
				(number "K2")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PF7")
				(number "K1")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PF8")
				(number "L3")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PF9")
				(number "L2")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PF10")
				(number "L1")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "PF12")
				(number "P6")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "PF13")
				(number "N6")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -73.66 0)
				(length 5.08)
				(name "PF15")
				(number "P7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin power_out line
				(at -35.56 -78.74 0)
				(length 5.08)
				(name "VCAP_1")
				(number "M10")
			)
			(pin power_out line
				(at -35.56 -81.28 0)
				(length 5.08)
				(name "VCAP_2")
				(number "F13")
			)
			(pin no_connect line
				(at -30.48 -109.22 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "C6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C8")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C9")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F3")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G13")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H13")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M1")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "K4")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N8")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N9")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N10")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "R1")
			)
			(pin bidirectional line
				(at 35.56 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "N3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "N2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "P2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "R2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "N4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "P4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "D15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B15")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA13")
				(number "A15")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA14")
				(number "A14")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA15")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "R4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "M6")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PB3")
				(number "A10")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PB4")
				(number "A9")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "B5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "A5")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "B4")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "R12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "R13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "P12")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "P13")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "R14")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "R15")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "M2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "M3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "M4")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "M5")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "H15")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PC8")
				(number "G14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F14")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "B14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "A12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "D1")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "C12")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "D12")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "D11")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D10")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "C11")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B11")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A11")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "P15")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "P14")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "N15")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "N14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "N13")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "M15")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "M14")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "L14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "B2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "B3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R8")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P8")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "P9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R9")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R10")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "N11")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "P11")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "R11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F207I_C-E-F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207I_C-E-F-G_Tx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ic.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F207I_C-E-F-G_Tx_0_1")
		(symbol "STM32F207I_C-E-F-G_Tx_1_1"
			(pin input line
				(at -35.56 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "31")
			)
			(pin input line
				(at -35.56 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin input line
				(at -35.56 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 91.44 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 88.9 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 86.36 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 81.28 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "RTC_AF2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 68.58 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "ETH_RX_ER" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "30")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "43")
				(alternate "ETH_CRS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PH3")
				(number "44")
				(alternate "ETH_COL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PH4")
				(number "45")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PH5")
				(number "46")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PH6")
				(number "83")
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PH7")
				(number "84")
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PH8")
				(number "85")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PH9")
				(number "86")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PH10")
				(number "87")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PH11")
				(number "88")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PH12")
				(number "89")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PG0")
				(number "66")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PG1")
				(number "67")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "FSMC_INT3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "FSMC_NE4" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FSMC_A24" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FSMC_A25" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FSMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FSMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FSMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PF10")
				(number "28")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PF11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PF12")
				(number "60")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PF13")
				(number "63")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PF14")
				(number "64")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "PF15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin power_out line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "VCAP_1")
				(number "81")
			)
			(pin power_out line
				(at -35.56 -73.66 0)
				(length 5.08)
				(name "VCAP_2")
				(number "125")
			)
			(pin no_connect line
				(at -30.48 -109.22 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "171")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "82")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "90")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "37")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "149")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "39")
			)
			(pin bidirectional line
				(at 35.56 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "40")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "41")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "42")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "47")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "50")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "51")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "52")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "53")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA13")
				(number "124")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA14")
				(number "137")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA15")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "56")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "57")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "58")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PB3")
				(number "161")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PB4")
				(number "162")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "79")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "32")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "33")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "34")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "54")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "55")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "68")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "69")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "70")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "73")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "74")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "75")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "76")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "77")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F207V_C-E-F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F207V_C-E-F-G_Tx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F207V_C-E-F-G_Tx_0_1")
		(symbol "STM32F207V_C-E-F-G_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "VCAP_1")
				(number "49")
			)
			(pin power_out line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "VCAP_2")
				(number "73")
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "99")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F207Z_C-E-F-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F207Z_C-E-F-G_Tx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F207Z_C-E-F-G_Tx_0_1")
		(symbol "STM32F207Z_C-E-F-G_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FSMC_INT3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FSMC_A24" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FSMC_A25" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -68.58 0)
				(length 5.08)
				(name "VCAP_1")
				(number "71")
			)
			(pin power_out line
				(at -33.02 -71.12 0)
				(length 5.08)
				(name "VCAP_2")
				(number "106")
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "143")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F215R_E-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F215R_E-G_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F215R_E-G_Tx_0_1")
		(symbol "STM32F215R_E-G_Tx_1_1"
			(pin input line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "VCAP_1")
				(number "31")
			)
			(pin power_out line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "VCAP_2")
				(number "47")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F215V_E-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F215V_E-G_Tx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F215V_E-G_Tx_0_1")
		(symbol "STM32F215V_E-G_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "VCAP_1")
				(number "49")
			)
			(pin power_out line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "VCAP_2")
				(number "73")
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "99")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F215Z_E-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F215Z_E-G_Tx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F215Z_E-G_Tx_0_1")
		(symbol "STM32F215Z_E-G_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FSMC_INT3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -68.58 0)
				(length 5.08)
				(name "VCAP_1")
				(number "71")
			)
			(pin power_out line
				(at -33.02 -71.12 0)
				(length 5.08)
				(name "VCAP_2")
				(number "106")
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "143")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F217I_E-G_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F217I_E-G_Hx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ie.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32F217I_E-G_Hx_0_1")
		(symbol "STM32F217I_E-G_Hx_1_1"
			(pin input line
				(at -35.56 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -35.56 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "D6")
			)
			(pin input line
				(at -35.56 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "P1")
			)
			(pin input line
				(at -35.56 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "N1")
			)
			(pin input line
				(at -35.56 88.9 0)
				(length 5.08)
				(name "REGOFF")
				(number "L4")
			)
			(pin bidirectional line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "PI0")
				(number "E14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 81.28 0)
				(length 5.08)
				(name "PI1")
				(number "D14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "PI2")
				(number "C14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "PI3")
				(number "C13")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "PI4")
				(number "D4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "PI5")
				(number "C4")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 68.58 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PI7")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PI8")
				(number "D2")
				(alternate "RTC_AF2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "PI9")
				(number "D3")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PI10")
				(number "E3")
				(alternate "ETH_RX_ER" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PI11")
				(number "E4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PH0")
				(number "G1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PH1")
				(number "H1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PH2")
				(number "F4")
				(alternate "ETH_CRS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PH3")
				(number "G4")
				(alternate "ETH_COL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PH4")
				(number "H4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PH5")
				(number "J4")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PH6")
				(number "M11")
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PH7")
				(number "N12")
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PH10")
				(number "L13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PH11")
				(number "L12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PH12")
				(number "K12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PH13")
				(number "E12")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PH14")
				(number "E13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PH15")
				(number "D13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PG0")
				(number "N7")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PG1")
				(number "M7")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PG2")
				(number "L15")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PG3")
				(number "K15")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PG4")
				(number "K14")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PG5")
				(number "K13")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PG6")
				(number "J15")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PG7")
				(number "J14")
				(alternate "FSMC_INT3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PG8")
				(number "H14")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PG9")
				(number "C10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PG10")
				(number "B10")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PG11")
				(number "B9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "FSMC_NE4" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PG13")
				(number "A8")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FSMC_A24" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PG14")
				(number "A7")
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FSMC_A25" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FSMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PF1")
				(number "H3")
				(alternate "FSMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "FSMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PF3")
				(number "J2")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PF4")
				(number "J3")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PF5")
				(number "K3")
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PF6")
				(number "K2")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PF7")
				(number "K1")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PF8")
				(number "L3")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PF9")
				(number "L2")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PF10")
				(number "L1")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "PF12")
				(number "P6")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "PF13")
				(number "N6")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -73.66 0)
				(length 5.08)
				(name "PF15")
				(number "P7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin power_out line
				(at -35.56 -78.74 0)
				(length 5.08)
				(name "VCAP_1")
				(number "M10")
			)
			(pin power_out line
				(at -35.56 -81.28 0)
				(length 5.08)
				(name "VCAP_2")
				(number "F13")
			)
			(pin no_connect line
				(at -30.48 -109.22 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "C6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C8")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C9")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F3")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G13")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H13")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M1")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "K4")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N8")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N9")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N10")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "R1")
			)
			(pin bidirectional line
				(at 35.56 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "N3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "N2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "P2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "R2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "N4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "P4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "D15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B15")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA13")
				(number "A15")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA14")
				(number "A14")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA15")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "R4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "M6")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PB3")
				(number "A10")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PB4")
				(number "A9")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "B5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "A5")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "B4")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "R12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "R13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "P12")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "P13")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "R14")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "R15")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "M2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "M3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "M4")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "M5")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "H15")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PC8")
				(number "G14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F14")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "B14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "A12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "D1")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "C12")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "D12")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "D11")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D10")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "C11")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B11")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A11")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "P15")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "P14")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "N15")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "N14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "N13")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "M15")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "M14")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "L14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "B2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "B3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R8")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P8")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "P9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R9")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R10")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "N11")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "P11")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "R11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F217I_E-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F217I_E-G_Tx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ie.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F217I_E-G_Tx_0_1")
		(symbol "STM32F217I_E-G_Tx_1_1"
			(pin input line
				(at -35.56 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "31")
			)
			(pin input line
				(at -35.56 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin input line
				(at -35.56 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 91.44 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 88.9 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 86.36 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 81.28 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "RTC_AF2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 68.58 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "ETH_RX_ER" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "30")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "43")
				(alternate "ETH_CRS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PH3")
				(number "44")
				(alternate "ETH_COL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PH4")
				(number "45")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PH5")
				(number "46")
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PH6")
				(number "83")
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PH7")
				(number "84")
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PH8")
				(number "85")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PH9")
				(number "86")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PH10")
				(number "87")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PH11")
				(number "88")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PH12")
				(number "89")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PG0")
				(number "66")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PG1")
				(number "67")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "FSMC_INT3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "FSMC_NE4" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FSMC_A24" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FSMC_A25" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FSMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FSMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FSMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PF10")
				(number "28")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PF11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PF12")
				(number "60")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PF13")
				(number "63")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PF14")
				(number "64")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "PF15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin power_out line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "VCAP_1")
				(number "81")
			)
			(pin power_out line
				(at -35.56 -73.66 0)
				(length 5.08)
				(name "VCAP_2")
				(number "125")
			)
			(pin no_connect line
				(at -30.48 -109.22 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "171")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "82")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "90")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "37")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "149")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "39")
			)
			(pin bidirectional line
				(at 35.56 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "40")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "41")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "42")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "47")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "50")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "51")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "52")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "53")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA13")
				(number "124")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA14")
				(number "137")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA15")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "56")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "57")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "58")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PB3")
				(number "161")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PB4")
				(number "162")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "79")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "32")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "33")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "34")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "35")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "54")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "55")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "68")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "69")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "70")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "73")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "74")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "75")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "76")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "77")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F217V_E-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F217V_E-G_Tx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F217V_E-G_Tx_0_1")
		(symbol "STM32F217V_E-G_Tx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "VCAP_1")
				(number "49")
			)
			(pin power_out line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "VCAP_2")
				(number "73")
			)
			(pin no_connect line
				(at -20.32 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "99")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F217Z_E-G_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F217Z_E-G_Tx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512-1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F217Z_E-G_Tx_0_1")
		(symbol "STM32F217Z_E-G_Tx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FSMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FSMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FSMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FSMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FSMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FSMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FSMC_INT3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NCE3" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NCE4_1" bidirectional line)
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FSMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FSMC_A24" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FSMC_A25" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "FSMC_NIORD" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FSMC_NREG" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "FSMC_NIOWR" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_CD" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "FSMC_INTR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FSMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FSMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FSMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FSMC_NBL1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FSMC_A22" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -68.58 0)
				(length 5.08)
				(name "VCAP_1")
				(number "71")
			)
			(pin power_out line
				(at -33.02 -71.12 0)
				(length 5.08)
				(name "VCAP_2")
				(number "106")
			)
			(pin no_connect line
				(at -27.94 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "RFU")
				(number "143")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "ADC2_IN0" bidirectional line)
				(alternate "ADC3_IN0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "SYS_WKUP" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_SCK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_AF1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "FSMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "FSMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F205RBTx"
		(extends "STM32F205R_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F205RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 64KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205RCTx"
		(extends "STM32F205R_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F205RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 96KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205RETx"
		(extends "STM32F205R_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F205RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205REYx"
		(extends "STM32F205R_E-G_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F205REYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-66_Die411"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, WLCSP66"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die411*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205RFTx"
		(extends "STM32F205R_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F205RFTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205rf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205RGTx"
		(extends "STM32F205R_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F205RGTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205RGYx"
		(extends "STM32F205R_E-G_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F205RGYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-66_Die411"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, WLCSP66"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die411*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205VBTx"
		(extends "STM32F205V_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F205VBTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 64KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205VCTx"
		(extends "STM32F205V_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F205VCTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 96KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205VETx"
		(extends "STM32F205V_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F205VETx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205VFTx"
		(extends "STM32F205V_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F205VFTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205vf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205VGTx"
		(extends "STM32F205V_B-C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F205VGTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205ZCTx"
		(extends "STM32F205Z_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F205ZCTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 96KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205ZETx"
		(extends "STM32F205Z_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F205ZETx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205ZFTx"
		(extends "STM32F205Z_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F205ZFTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205zf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F205ZGTx"
		(extends "STM32F205Z_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F205ZGTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f205zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207ICHx"
		(extends "STM32F207I_C-E-F-G_Hx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207ICHx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ic.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207ICTx"
		(extends "STM32F207I_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207ICTx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ic.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207IEHx"
		(extends "STM32F207I_C-E-F-G_Hx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207IEHx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ie.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207IETx"
		(extends "STM32F207I_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207IETx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ie.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207IFHx"
		(extends "STM32F207I_C-E-F-G_Hx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207IFHx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207if.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207IFTx"
		(extends "STM32F207I_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207IFTx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207if.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207IGHx"
		(extends "STM32F207I_C-E-F-G_Hx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207IGHx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ig.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207IGTx"
		(extends "STM32F207I_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F207IGTx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ig.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207VCTx"
		(extends "STM32F207V_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F207VCTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207VETx"
		(extends "STM32F207V_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F207VETx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207VFTx"
		(extends "STM32F207V_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F207VFTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207vf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207VGTx"
		(extends "STM32F207V_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F207VGTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207ZCTx"
		(extends "STM32F207Z_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F207ZCTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207ZETx"
		(extends "STM32F207Z_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F207ZETx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207ZFTx"
		(extends "STM32F207Z_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F207ZFTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207zf.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 768KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F207ZGTx"
		(extends "STM32F207Z_C-E-F-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F207ZGTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f207zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F215RETx"
		(extends "STM32F215R_E-G_Tx")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F215RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F215RGTx"
		(extends "STM32F215R_E-G_Tx")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32F215RGTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F215VETx"
		(extends "STM32F215V_E-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F215VETx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F215VGTx"
		(extends "STM32F215V_E-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F215VGTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F215ZETx"
		(extends "STM32F215Z_E-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F215ZETx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F215ZGTx"
		(extends "STM32F215Z_E-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F215ZGTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f215zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x5"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F217IEHx"
		(extends "STM32F217I_E-G_Hx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F217IEHx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ie.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F217IETx"
		(extends "STM32F217I_E-G_Tx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F217IETx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ie.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F217IGHx"
		(extends "STM32F217I_E-G_Hx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F217IGHx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ig.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F217IGTx"
		(extends "STM32F217I_E-G_Tx")
		(property "Reference" "U"
			(at -30.48 113.03 0)
		)
		(property "Value" "STM32F217IGTx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -30.48 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ig.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F217VETx"
		(extends "STM32F217V_E-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F217VETx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F217VGTx"
		(extends "STM32F217V_E-G_Tx")
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F217VGTx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 82 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F217ZETx"
		(extends "STM32F217Z_E-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F217ZETx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F217ZGTx"
		(extends "STM32F217Z_E-G_Tx")
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32F217ZGTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f217zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 1024KB flash, 128KB RAM, 120 MHz, 1.8-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32F2 STM32F2x7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
