(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32F301C8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F301C8Yx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die439"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die439*"
			(at 0 0 0)
		)
		(symbol "STM32F301C8Yx_0_1")
		(symbol "STM32F301C8Yx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "D7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "D6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "D5")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "C7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "G5")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "G4")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "G3")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "D4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "C5")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E3")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "G2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "E2")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "B6")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "B7")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "E6")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "A6")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "G7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "G6")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "B3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F301C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F301C_6-8_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F301C_6-8_Tx_0_1")
		(symbol "STM32F301C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F301K_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F301K_6-8_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F301K_6-8_Tx_0_1")
		(symbol "STM32F301K_6-8_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F301K_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F301K_6-8_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F301K_6-8_Ux_0_1")
		(symbol "STM32F301K_6-8_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F301R_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F301R_6-8_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F301R_6-8_Tx_0_1")
		(symbol "STM32F301R_6-8_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302C8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F302C8Yx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die439"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die439*"
			(at 0 0 0)
		)
		(symbol "STM32F302C8Yx_0_1")
		(symbol "STM32F302C8Yx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "D7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "D6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "D5")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "C7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "G5")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "G4")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "G3")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "D4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "C5")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E3")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "G2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "E2")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "B6")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "B7")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "E6")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "A6")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "G7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "G6")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "B3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F302C_6-8_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302C_6-8_Tx_0_1")
		(symbol "STM32F302C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302C_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F302C_B-C_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-256KB flash, 32-40KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302C_B-C_Tx_0_1")
		(symbol "STM32F302C_B-C_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302K_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F302K_6-8_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302K_6-8_Ux_0_1")
		(symbol "STM32F302K_6-8_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302R_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302R_6-8_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302R_6-8_Tx_0_1")
		(symbol "STM32F302R_6-8_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302R_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302R_B-C_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-256KB flash, 32-40KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302R_B-C_Tx_0_1")
		(symbol "STM32F302R_B-C_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF4")
				(number "18")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302R_D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302R_D-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384-512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302R_D-E_Tx_0_1")
		(symbol "STM32F302R_D-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302VCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F302VCYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-100_Die422"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 40KB RAM, 72 MHz, 2.0-3.6V, 78 GPIO, WLCSP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die422*"
			(at 0 0 0)
		)
		(symbol "STM32F302VCYx_0_1")
		(symbol "STM32F302VCYx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "E9")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A7")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "F10")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "F9")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "E8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "C1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "E10")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "B7")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE1")
				(number "A8")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE2")
				(number "D6")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE3")
				(number "D7")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE4")
				(number "C8")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE5")
				(number "B9")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE6")
				(number "E7")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE7")
				(number "F8")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE8")
				(number "E6")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "H5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "G5")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PD0")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PD1")
				(number "C3")
				(alternate "CAN_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD2")
				(number "A4")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD3")
				(number "B4")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD4")
				(number "C4")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD7")
				(number "D4")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD9")
				(number "G4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD10")
				(number "H3")
				(alternate "COMP6_INM" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD11")
				(number "H2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD12")
				(number "H1")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD13")
				(number "G3")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD14")
				(number "G2")
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD15")
				(number "G1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D8")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B8")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B10")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "H8")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "J5")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "K8")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "J10")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "H9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "J9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "F7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "J7")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "H7")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "H6")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K7")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "F5")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "E5")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "E1")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "E2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "D1")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "E3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "C2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "J6")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K6")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "K5")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "B5")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "D5")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "C6")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "K4")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "K3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "J4")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "J2")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "H4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "G10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "G9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "G8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "H10")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "F6")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F4")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F2")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F1")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "F3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "E4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "D3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C9")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "C10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302V_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302V_B-C_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-256KB flash, 32-40KB RAM, 72 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302V_B-C_Tx_0_1")
		(symbol "STM32F302V_B-C_Tx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF4")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF6")
				(number "73")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "COMP6_INM" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302V_D-E_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302V_D-E_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384-512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302V_D-E_Hx_0_1")
		(symbol "STM32F302V_D-E_Hx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "M1")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
				(alternate "FMC_NIORD" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_CD" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
				(alternate "FMC_INTR" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "FMC_A23" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "FMC_A19" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "FMC_CLK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "FMC_NCE2" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "COMP6_INM" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "L1")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302V_D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302V_D-E_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384-512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302V_D-E_Tx_0_1")
		(symbol "STM32F302V_D-E_Tx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "73")
				(alternate "FMC_NIORD" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_CD" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "FMC_INTR" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FMC_A23" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FMC_A19" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FMC_CLK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE2" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "COMP6_INM" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F302Z_D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32F302Z_D-E_Tx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384-512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F302Z_D-E_Tx_0_1")
		(symbol "STM32F302Z_D-E_Tx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FMC_INT3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE3" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FMC_NCE4_1" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "24")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "FMC_NIORD" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "FMC_NREG" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "FMC_NIOWR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_CD" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "FMC_INTR" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FMC_A23" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FMC_A19" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FMC_CLK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE2" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "COMP6_INM" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303C8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "STM32F303C8Yx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die438"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 38 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die438*"
			(at 0 0 0)
		)
		(symbol "STM32F303C8Yx_0_1")
		(symbol "STM32F303C8Yx_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "D7")
			)
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "VREF+")
				(number "F7")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "C7")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "C6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "C5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "G4")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "E3")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "D4")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "G3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "F2")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "B3")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "B5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "B6")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "A6")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "G2")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "G1")
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "F1")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "E2")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "E1")
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "D3")
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "E7")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "E6")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "G7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "D5")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "E5")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "G5")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "E4")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "C4")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F303C_6-8_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303C_6-8_Tx_0_1")
		(symbol "STM32F303C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303C_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F303C_B-C_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-256KB flash, 40-48KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303C_B-C_Tx_0_1")
		(symbol "STM32F303C_B-C_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303K_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F303K_6-8_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303K_6-8_Tx_0_1")
		(symbol "STM32F303K_6-8_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303K_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F303K_6-8_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303K_6-8_Ux_0_1")
		(symbol "STM32F303K_6-8_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303R_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303R_6-8_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303R_6-8_Tx_0_1")
		(symbol "STM32F303R_6-8_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303R_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303R_B-C_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-256KB flash, 40-48KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303R_B-C_Tx_0_1")
		(symbol "STM32F303R_B-C_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF4")
				(number "18")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303R_D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303R_D-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384-512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303R_D-E_Tx_0_1")
		(symbol "STM32F303R_D-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303VCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F303VCYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-100_Die422"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 78 GPIO, WLCSP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die422*"
			(at 0 0 0)
		)
		(symbol "STM32F303VCYx_0_1")
		(symbol "STM32F303VCYx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "E9")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A7")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "F10")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "F9")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "E8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "C1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "E10")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "B7")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE1")
				(number "A8")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE2")
				(number "D6")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE3")
				(number "D7")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE4")
				(number "C8")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE5")
				(number "B9")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE6")
				(number "E7")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE7")
				(number "F8")
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE8")
				(number "E6")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "H5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "G5")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PD0")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PD1")
				(number "C3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD2")
				(number "A4")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD3")
				(number "B4")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD4")
				(number "C4")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD7")
				(number "D4")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD9")
				(number "G4")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD10")
				(number "H3")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD11")
				(number "H2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD12")
				(number "H1")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD13")
				(number "G3")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD14")
				(number "G2")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD15")
				(number "G1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D8")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B8")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B10")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "H8")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "J5")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "K8")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "J10")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "H9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "J9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "F7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "J7")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "H7")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "H6")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K7")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "F5")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "E5")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "E1")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "E2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "D1")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "E3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "C2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "J6")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K6")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "K5")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "B5")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "D5")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "C6")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "K4")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "K3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "J4")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J3")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "J2")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "H4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "G10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "G9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "G8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "H10")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "F6")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F4")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F2")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F1")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "F3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "E4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "D3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C9")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "C10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303VEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F303VEYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-100_Die446"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 78 GPIO, WLCSP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die446*"
			(at 0 0 0)
		)
		(symbol "STM32F303VEYx_0_1")
		(symbol "STM32F303VEYx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "E9")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A7")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "J8")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "F10")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "F9")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "E8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "C1")
				(alternate "FMC_NIORD" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_CD" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "E10")
				(alternate "FMC_INTR" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "B7")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PE1")
				(number "A8")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PE2")
				(number "D6")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PE3")
				(number "D7")
				(alternate "FMC_A19" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE4")
				(number "C8")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE5")
				(number "B9")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE6")
				(number "E7")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE7")
				(number "F8")
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE8")
				(number "E6")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "H5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "G5")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PD0")
				(number "B3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PD1")
				(number "C3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PD2")
				(number "A4")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PD3")
				(number "B4")
				(alternate "FMC_CLK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PD4")
				(number "C4")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PD7")
				(number "D4")
				(alternate "FMC_NCE2" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PD9")
				(number "G4")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PD10")
				(number "H3")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PD11")
				(number "H2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD12")
				(number "H1")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD13")
				(number "G3")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD14")
				(number "G2")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD15")
				(number "G1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D8")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B8")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "B10")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "H8")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "J5")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "K8")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "J10")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "H9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "J9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "F7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "J7")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "H7")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "H6")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K7")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "F5")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "E5")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "E1")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "E2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "D1")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "E3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "C2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "J6")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K6")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "K5")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "B5")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB8")
				(number "D5")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "C6")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "K4")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "K3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "J4")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J3")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "J2")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "H4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "G10")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "G9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "G8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "H10")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "G6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "F6")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F4")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F2")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "F1")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "F3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "E4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "D3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C9")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "C10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303V_B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303V_B-C_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-256KB flash, 40-48KB RAM, 72 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303V_B-C_Tx_0_1")
		(symbol "STM32F303V_B-C_Tx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF4")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF6")
				(number "73")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303V_D-E_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303V_D-E_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384-512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303V_D-E_Hx_0_1")
		(symbol "STM32F303V_D-E_Hx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "M1")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
				(alternate "FMC_NIORD" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_CD" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
				(alternate "FMC_INTR" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "FMC_A19" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "FMC_CLK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "FMC_NCE2" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "L1")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303V_D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303V_D-E_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384-512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303V_D-E_Tx_0_1")
		(symbol "STM32F303V_D-E_Tx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "73")
				(alternate "FMC_NIORD" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_CD" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "FMC_INTR" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FMC_A19" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FMC_CLK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE2" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F303Z_D-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32F303Z_D-E_Tx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384-512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F303Z_D-E_Tx_0_1")
		(symbol "STM32F303Z_D-E_Tx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "FMC_INT2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "FMC_INT3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE3" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FMC_NCE4_1" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NCE4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "23")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "24")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "FMC_NIORD" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "FMC_NREG" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "FMC_NIOWR" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_CD" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "FMC_INTR" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FMC_A7" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FMC_A8" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FMC_A19" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FMC_CLK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE2" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F318C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F318C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f318c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 1.65-1.95V, 36 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F318C8Tx_0_1")
		(symbol "STM32F318C8Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F318C8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F318C8Yx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die439"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f318c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 1.65-1.95V, 36 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die439*"
			(at 0 0 0)
		)
		(symbol "STM32F318C8Yx_0_1")
		(symbol "STM32F318C8Yx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NPOR")
				(number "G3")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF0")
				(number "D7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF1")
				(number "D6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "D5")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "C7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "C6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "G5")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "G4")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "D4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "C5")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E3")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "G2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "E2")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "A7")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "B6")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "B7")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "E6")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "A6")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "G7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "G6")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "B3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F318K8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F318K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f318k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 1.65-1.95V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F318K8Ux_0_1")
		(symbol "STM32F318K8Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NPOR")
				(number "30")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F328C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 41.91 0)
		)
		(property "Value" "STM32F328C8Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f328c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 1.65-1.95V, 36 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F328C8Tx_0_1")
		(symbol "STM32F328C8Tx_1_1"
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "COMP6_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F334C8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "STM32F334C8Yx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die438"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 38 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die438*"
			(at 0 0 0)
		)
		(symbol "STM32F334C8Yx_0_1")
		(symbol "STM32F334C8Yx_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "D7")
			)
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "VREF+")
				(number "F7")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "C7")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "C6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "C5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "G4")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "E3")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "D4")
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "G3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "F2")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "B3")
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "B5")
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "B6")
				(alternate "CAN_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "A6")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "G2")
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "G1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "F1")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "E2")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "E1")
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "D3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "E7")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "E6")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "G7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "D5")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "E5")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "G5")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "E4")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_DIG" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "C4")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F334C_4-6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F334C_4-6-8_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 16-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F334C_4-6-8_Tx_0_1")
		(symbol "STM32F334C_4-6-8_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_DIG" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F334K_4-6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F334K_4-6-8_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 16-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32F334K_4-6-8_Tx_0_1")
		(symbol "STM32F334K_4-6-8_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_DIG" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F334K_4-6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F334K_4-6-8_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 16-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F334K_4-6-8_Ux_0_1")
		(symbol "STM32F334K_4-6-8_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_DIG" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F334R_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F334R_6-8_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F334R_6-8_Tx_0_1")
		(symbol "STM32F334R_6-8_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "OPAMP2_DIG" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F358CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F358CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f358cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 48KB RAM, 72 MHz, 1.65-1.95V, 36 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F358CCTx_0_1")
		(symbol "STM32F358CCTx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F358RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F358RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f358rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 48KB RAM, 72 MHz, 1.65-1.95V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F358RCTx_0_1")
		(symbol "STM32F358RCTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NPOR")
				(number "28")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF4")
				(number "18")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F358VCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 67.31 0)
		)
		(property "Value" "STM32F358VCTx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f358vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 48KB RAM, 72 MHz, 1.65-1.95V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F358VCTx_0_1")
		(symbol "STM32F358VCTx_1_1"
			(pin input line
				(at -20.32 60.96 0)
				(length 5.08)
				(name "NPOR")
				(number "37")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF4")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PF6")
				(number "73")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -58.42 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F373C_8-B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 41.91 0)
		)
		(property "Value" "STM32F373C_8-B-C_Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -17.78 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64-256KB flash, 16-32KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F373C_8-B-C_Tx_0_1")
		(symbol "STM32F373C_8-B-C_Tx_1_1"
			(pin input line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "VREFSD+")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PE8")
				(number "21")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PE9")
				(number "22")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "28")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSD")
				(number "23")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDSD")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "SDADC1_AIN4P" bidirectional line)
				(alternate "SDADC2_AIN6P" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F373R_8-B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 49.53 0)
		)
		(property "Value" "STM32F373R_8-B-C_Tx"
			(at 7.62 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64-256KB flash, 16-32KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F373R_8-B-C_Tx_0_1")
		(symbol "STM32F373R_8-B-C_Tx_1_1"
			(pin input line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin input line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "17")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "VREFSD+")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PF6")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PF7")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE8")
				(number "29")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PE9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD8")
				(number "36")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSSD")
				(number "31")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 2.54)
				(name "VDDSD")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "18")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "SDADC1_AIN4P" bidirectional line)
				(alternate "SDADC2_AIN6P" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F373V_8-B-C_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "STM32F373V_8-B-C_Hx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64-256KB flash, 16-32KB RAM, 72 MHz, 2.0-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F373V_8-B-C_Hx_0_1")
		(symbol "STM32F373V_8-B-C_Hx_1_1"
			(pin input line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "VREFSD+")
				(number "K12")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "VREFSD-")
				(number "L11")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "SDADC1_AIN3P" bidirectional line)
				(alternate "SDADC1_AIN4M" bidirectional line)
				(alternate "SDADC2_AIN5P" bidirectional line)
				(alternate "SDADC2_AIN6M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "SDADC1_AIN2P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SDADC1_AIN1P" bidirectional line)
				(alternate "SDADC1_AIN2M" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_AIN4P" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SDADC1_AIN0P" bidirectional line)
				(alternate "SDADC2_AIN3P" bidirectional line)
				(alternate "SDADC2_AIN4M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SDADC1_AIN0M" bidirectional line)
				(alternate "SDADC2_AIN2P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SDADC2_AIN1P" bidirectional line)
				(alternate "SDADC2_AIN2M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_AIN0P" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC3_AIN5P" bidirectional line)
				(alternate "SDADC3_AIN6M" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "SDADC3_AIN4P" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_AIN3P" bidirectional line)
				(alternate "SDADC3_AIN4M" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "SDADC3_AIN2P" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "SDADC3_AIN1P" bidirectional line)
				(alternate "SDADC3_AIN2M" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "SDADC3_AIN0P" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN0M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSSD")
				(number "F12")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDSD3")
				(number "L12")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDSD12")
				(number "G12")
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "SDADC1_AIN4P" bidirectional line)
				(alternate "SDADC2_AIN6P" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "CEC" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC2_AIN0M" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F373V_8-B-C_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "STM32F373V_8-B-C_Tx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64-256KB flash, 16-32KB RAM, 72 MHz, 2.0-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F373V_8-B-C_Tx_0_1")
		(symbol "STM32F373V_8-B-C_Tx_1_1"
			(pin input line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "22")
			)
			(pin input line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "VREFSD+")
				(number "52")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "VREFSD-")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PF6")
				(number "73")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PF10")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "SDADC1_AIN3P" bidirectional line)
				(alternate "SDADC1_AIN4M" bidirectional line)
				(alternate "SDADC2_AIN5P" bidirectional line)
				(alternate "SDADC2_AIN6M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "SDADC1_AIN2P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SDADC1_AIN1P" bidirectional line)
				(alternate "SDADC1_AIN2M" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_AIN4P" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SDADC1_AIN0P" bidirectional line)
				(alternate "SDADC2_AIN3P" bidirectional line)
				(alternate "SDADC2_AIN4M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SDADC1_AIN0M" bidirectional line)
				(alternate "SDADC2_AIN2P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SDADC2_AIN1P" bidirectional line)
				(alternate "SDADC2_AIN2M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_AIN0P" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC3_AIN5P" bidirectional line)
				(alternate "SDADC3_AIN6M" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "SDADC3_AIN4P" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_AIN3P" bidirectional line)
				(alternate "SDADC3_AIN4M" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "SDADC3_AIN2P" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "SDADC3_AIN1P" bidirectional line)
				(alternate "SDADC3_AIN2M" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "SDADC3_AIN0P" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN0M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSSD")
				(number "49")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDSD3")
				(number "51")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDSD12")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "SDADC1_AIN4P" bidirectional line)
				(alternate "SDADC2_AIN6P" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC2_AIN0M" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F378CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 39.37 0)
		)
		(property "Value" "STM32F378CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -17.78 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f378cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 1.65-1.95V, 36 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F378CCTx_0_1")
		(symbol "STM32F378CCTx_1_1"
			(pin input line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "NPOR")
				(number "20")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "VREFSD+")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PF6")
				(number "35")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PF7")
				(number "36")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PE8")
				(number "21")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PE9")
				(number "22")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD8")
				(number "28")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSSD")
				(number "23")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDSD")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F378RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 49.53 0)
		)
		(property "Value" "STM32F378RCTx"
			(at 7.62 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -48.26 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f378rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 1.65-1.95V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F378RCTx_0_1")
		(symbol "STM32F378RCTx_1_1"
			(pin input line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "NPOR")
				(number "28")
			)
			(pin input line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "17")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "VREFSD+")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PF6")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PF7")
				(number "48")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PE8")
				(number "29")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PE9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "36")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "VSSSD")
				(number "31")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 2.54)
				(name "VDDSD")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "18")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F378RCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 49.53 0)
		)
		(property "Value" "STM32F378RCYx"
			(at 7.62 49.53 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-66_Die432"
			(at -17.78 -48.26 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f378rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 1.65-1.95V, 51 GPIO, WLCSP66"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die432*"
			(at 0 0 0)
		)
		(symbol "STM32F378RCYx_0_1")
		(symbol "STM32F378RCYx_1_1"
			(pin input line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "NPOR")
				(number "G2")
			)
			(pin input line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "C7")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G6")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "VREFSD+")
				(number "G1")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "D7")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "E8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PF6")
				(number "B2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PF7")
				(number "B1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PE8")
				(number "H2")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PE9")
				(number "J2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "A4")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "F3")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "E6")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "F7")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "F6")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC4")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC5")
				(number "J4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "E2")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC7")
				(number "E1")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC8")
				(number "E3")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC9")
				(number "D2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC11")
				(number "A3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC12")
				(number "B4")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC13")
				(number "B8")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC14")
				(number "C8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC15")
				(number "D8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "VBAT")
				(number "A8")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "D6")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "VSS")
				(number "C6")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G4")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G5")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "J7")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSSA")
				(number "G8")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "VDDA")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "VSSSD")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 2.54)
				(name "VDDSD")
				(number "H1")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "H8")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "H7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "J8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "H6")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "J6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "H5")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "J5")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "G3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA9")
				(number "D3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA12")
				(number "C3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "C4")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "A1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB0")
				(number "H3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "J3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "C5")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "B5")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "B6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "A6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "B7")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB14")
				(number "F2")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F378VCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F378VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f378vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 1.65-1.95V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F378VCHx_0_1")
		(symbol "STM32F378VCHx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NPOR")
				(number "L6")
			)
			(pin input line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "VREFSD+")
				(number "K12")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "VREFSD-")
				(number "L11")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF1")
				(number "G1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF2")
				(number "J1")
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PF6")
				(number "C11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PF9")
				(number "F2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PF10")
				(number "G2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "SDADC1_AIN3P" bidirectional line)
				(alternate "SDADC1_AIN4M" bidirectional line)
				(alternate "SDADC2_AIN5P" bidirectional line)
				(alternate "SDADC2_AIN6M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "SDADC1_AIN2P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SDADC1_AIN1P" bidirectional line)
				(alternate "SDADC1_AIN2M" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_AIN4P" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SDADC1_AIN0P" bidirectional line)
				(alternate "SDADC2_AIN3P" bidirectional line)
				(alternate "SDADC2_AIN4M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SDADC1_AIN0M" bidirectional line)
				(alternate "SDADC2_AIN2P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SDADC2_AIN1P" bidirectional line)
				(alternate "SDADC2_AIN2M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_AIN0P" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC3_AIN5P" bidirectional line)
				(alternate "SDADC3_AIN6M" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "SDADC3_AIN4P" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_AIN3P" bidirectional line)
				(alternate "SDADC3_AIN4M" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "SDADC3_AIN2P" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "SDADC3_AIN1P" bidirectional line)
				(alternate "SDADC3_AIN2M" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "SDADC3_AIN0P" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN0M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K1")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSSD")
				(number "F12")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDSD3")
				(number "L12")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDSD12")
				(number "G12")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "CEC" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC2_AIN0M" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F378VCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32F378VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f378vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 1.65-1.95V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F378VCTx_0_1")
		(symbol "STM32F378VCTx_1_1"
			(pin input line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "NPOR")
				(number "37")
			)
			(pin input line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "22")
			)
			(pin input line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "VREFSD+")
				(number "52")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "VREFSD-")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PF6")
				(number "73")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PF10")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "SDADC1_AIN3P" bidirectional line)
				(alternate "SDADC1_AIN4M" bidirectional line)
				(alternate "SDADC2_AIN5P" bidirectional line)
				(alternate "SDADC2_AIN6M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "SDADC1_AIN8P" bidirectional line)
				(alternate "SDADC2_AIN8P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC1_AIN7P" bidirectional line)
				(alternate "SDADC1_AIN8M" bidirectional line)
				(alternate "SDADC2_AIN7P" bidirectional line)
				(alternate "SDADC2_AIN8M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "SDADC1_AIN2P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SDADC1_AIN1P" bidirectional line)
				(alternate "SDADC1_AIN2M" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_AIN4P" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SDADC1_AIN0P" bidirectional line)
				(alternate "SDADC2_AIN3P" bidirectional line)
				(alternate "SDADC2_AIN4M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SDADC1_AIN0M" bidirectional line)
				(alternate "SDADC2_AIN2P" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SDADC2_AIN1P" bidirectional line)
				(alternate "SDADC2_AIN2M" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_AIN0P" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC3_AIN6P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "SDADC3_AIN5P" bidirectional line)
				(alternate "SDADC3_AIN6M" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "SDADC3_AIN4P" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_AIN3P" bidirectional line)
				(alternate "SDADC3_AIN4M" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "SDADC3_AIN2P" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "SDADC3_AIN1P" bidirectional line)
				(alternate "SDADC3_AIN2M" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "SDADC3_AIN0P" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN0M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSSD")
				(number "49")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDSD3")
				(number "51")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDSD12")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SDADC1_AIN6P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "SDADC1_AIN5P" bidirectional line)
				(alternate "SDADC1_AIN6M" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_ETR" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM19_CH4" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SDADC2_AIN0M" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDADC3_AIN8P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_AIN7P" bidirectional line)
				(alternate "SDADC3_AIN8M" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM19_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDADC1_EXTI11" bidirectional line)
				(alternate "SDADC2_EXTI11" bidirectional line)
				(alternate "SDADC3_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM19_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM19_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "SDADC1_EXTI15" bidirectional line)
				(alternate "SDADC2_EXTI15" bidirectional line)
				(alternate "SDADC3_EXTI15" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F398VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 67.31 0)
		)
		(property "Value" "STM32F398VETx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f398ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 80KB RAM, 72 MHz, 1.65-1.95V, 85 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32F398VETx_0_1")
		(symbol "STM32F398VETx_1_1"
			(pin input line
				(at -20.32 60.96 0)
				(length 5.08)
				(name "NPOR")
				(number "37")
			)
			(pin input line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PF6")
				(number "73")
				(alternate "FMC_NIORD" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_CD" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "FMC_INTR" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FMC_A19" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN13" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "CAN_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "CAN_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FMC_CLK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE2" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_NJTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "CAN_RX" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "CAN_TX" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2S2_ext_SD" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2S3_ext_SD" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "ADC4_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32F301C6Tx"
		(extends "STM32F301C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F301C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F301C8Tx"
		(extends "STM32F301C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F301C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F301K6Tx"
		(extends "STM32F301K_6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F301K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F301K6Ux"
		(extends "STM32F301K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F301K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F301K8Tx"
		(extends "STM32F301K_6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F301K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F301K8Ux"
		(extends "STM32F301K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F301K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F301R6Tx"
		(extends "STM32F301R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F301R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F301R8Tx"
		(extends "STM32F301R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F301R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f301r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F301"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302C6Tx"
		(extends "STM32F302C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F302C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302C8Tx"
		(extends "STM32F302C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F302C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302CBTx"
		(extends "STM32F302C_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F302CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302CCTx"
		(extends "STM32F302C_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F302CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 40KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302K6Ux"
		(extends "STM32F302K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F302K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302K8Ux"
		(extends "STM32F302K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F302K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302R6Tx"
		(extends "STM32F302R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302R8Tx"
		(extends "STM32F302R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302RBTx"
		(extends "STM32F302R_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302RCTx"
		(extends "STM32F302R_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 40KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302RDTx"
		(extends "STM32F302R_D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302RDTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302RETx"
		(extends "STM32F302R_D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F302RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302VBTx"
		(extends "STM32F302V_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 72 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302VCTx"
		(extends "STM32F302V_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 40KB RAM, 72 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302VDHx"
		(extends "STM32F302V_D-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302VDHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302VDTx"
		(extends "STM32F302V_D-E_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302VDTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302VEHx"
		(extends "STM32F302V_D-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302VEHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302VETx"
		(extends "STM32F302V_D-E_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F302VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302ZDTx"
		(extends "STM32F302Z_D-E_Tx")
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32F302ZDTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F302ZETx"
		(extends "STM32F302Z_D-E_Tx")
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32F302ZETx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f302ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 64KB RAM, 72 MHz, 2.0-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F302"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303C6Tx"
		(extends "STM32F303C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F303C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303C8Tx"
		(extends "STM32F303C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F303C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303CBTx"
		(extends "STM32F303C_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F303CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 40KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303CCTx"
		(extends "STM32F303C_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F303CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303K6Tx"
		(extends "STM32F303K_6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F303K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303K6Ux"
		(extends "STM32F303K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F303K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303K8Tx"
		(extends "STM32F303K_6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F303K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303K8Ux"
		(extends "STM32F303K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F303K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F3x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303R6Tx"
		(extends "STM32F303R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303R8Tx"
		(extends "STM32F303R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303RBTx"
		(extends "STM32F303R_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 40KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303RCTx"
		(extends "STM32F303R_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303RDTx"
		(extends "STM32F303R_D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303RDTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303RETx"
		(extends "STM32F303R_D-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F303RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303VBTx"
		(extends "STM32F303V_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 40KB RAM, 72 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303VCTx"
		(extends "STM32F303V_B-C_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 87 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303VDHx"
		(extends "STM32F303V_D-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303VDHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303VDTx"
		(extends "STM32F303V_D-E_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303VDTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303VEHx"
		(extends "STM32F303V_D-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303VEHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303VETx"
		(extends "STM32F303V_D-E_Tx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32F303VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303ZDTx"
		(extends "STM32F303Z_D-E_Tx")
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32F303ZDTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 384KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F303ZETx"
		(extends "STM32F303Z_D-E_Tx")
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32F303ZETx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f303ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 80KB RAM, 72 MHz, 2.0-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F303"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334C4Tx"
		(extends "STM32F334C_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F334C4Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 16KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334C6Tx"
		(extends "STM32F334C_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F334C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334C8Tx"
		(extends "STM32F334C_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32F334C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334K4Tx"
		(extends "STM32F334K_4-6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F334K4Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 16KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334K4Ux"
		(extends "STM32F334K_4-6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F334K4Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 16KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334K6Tx"
		(extends "STM32F334K_4-6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F334K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334K6Ux"
		(extends "STM32F334K_4-6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F334K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334K8Tx"
		(extends "STM32F334K_4-6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F334K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334K8Ux"
		(extends "STM32F334K_4-6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32F334K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 24 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334R6Tx"
		(extends "STM32F334R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F334R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F334R8Tx"
		(extends "STM32F334R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32F334R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f334r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F334"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373C8Tx"
		(extends "STM32F373C_8-B-C_Tx")
		(property "Reference" "U"
			(at -17.78 41.91 0)
		)
		(property "Value" "STM32F373C8Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -17.78 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373CBTx"
		(extends "STM32F373C_8-B-C_Tx")
		(property "Reference" "U"
			(at -17.78 41.91 0)
		)
		(property "Value" "STM32F373CBTx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -17.78 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 24KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373CCTx"
		(extends "STM32F373C_8-B-C_Tx")
		(property "Reference" "U"
			(at -17.78 41.91 0)
		)
		(property "Value" "STM32F373CCTx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -17.78 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 2.0-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373R8Tx"
		(extends "STM32F373R_8-B-C_Tx")
		(property "Reference" "U"
			(at -17.78 49.53 0)
		)
		(property "Value" "STM32F373R8Tx"
			(at 7.62 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373RBTx"
		(extends "STM32F373R_8-B-C_Tx")
		(property "Reference" "U"
			(at -17.78 49.53 0)
		)
		(property "Value" "STM32F373RBTx"
			(at 7.62 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 24KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373RCTx"
		(extends "STM32F373R_8-B-C_Tx")
		(property "Reference" "U"
			(at -17.78 49.53 0)
		)
		(property "Value" "STM32F373RCTx"
			(at 7.62 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 2.0-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373V8Hx"
		(extends "STM32F373V_8-B-C_Hx")
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "STM32F373V8Hx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373V8Tx"
		(extends "STM32F373V_8-B-C_Tx")
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "STM32F373V8Tx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 16KB RAM, 72 MHz, 2.0-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373VBHx"
		(extends "STM32F373V_8-B-C_Hx")
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "STM32F373VBHx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 24KB RAM, 72 MHz, 2.0-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373VBTx"
		(extends "STM32F373V_8-B-C_Tx")
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "STM32F373VBTx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 24KB RAM, 72 MHz, 2.0-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373VCHx"
		(extends "STM32F373V_8-B-C_Hx")
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "STM32F373VCHx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 2.0-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32F373VCTx"
		(extends "STM32F373V_8-B-C_Tx")
		(property "Reference" "U"
			(at -20.32 67.31 0)
		)
		(property "Value" "STM32F373VCTx"
			(at 10.16 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f373vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 32KB RAM, 72 MHz, 2.0-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32F3 STM32F373"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
