(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32G030C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G030C_6-8_Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 43 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G030C_6-8_Tx_0_1")
		(symbol "STM32G030C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "10")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G030F6Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G030F6Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 17 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32G030F6Px_0_1")
		(symbol "STM32G030F6Px_1_1"
			(pin input line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "2")
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "15")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "16")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "17")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G030J6Mx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 11.43 0)
		)
		(property "Value" "STM32G030J6Mx"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -27.94 -7.62 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030j6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 6 GPIO, SO8N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STM32G030J6Mx_0_1")
		(symbol "STM32G030J6Mx_1_1"
			(pin input line
				(at -30.48 5.08 0)
				(length 2.54)
				(name "NRST/PA0/PA1/PA2")
				(number "4")
				(alternate "ADC1_IN0 (PA0)" bidirectional line)
				(alternate "ADC1_IN1 (PA1)" bidirectional line)
				(alternate "ADC1_IN2 (PA2)" bidirectional line)
				(alternate "I2C1_SMBA (PA1)" bidirectional line)
				(alternate "I2S1_CK (PA1)" bidirectional line)
				(alternate "I2S1_SD (PA2)" bidirectional line)
				(alternate "NRST" bidirectional line)
				(alternate "PA0" bidirectional line)
				(alternate "PA1" bidirectional line)
				(alternate "PA2" bidirectional line)
				(alternate "RCC_LSCO (PA2)" bidirectional line)
				(alternate "RTC_TAMP_IN2 (PA0)" bidirectional line)
				(alternate "SPI1_MOSI (PA2)" bidirectional line)
				(alternate "SPI1_SCK (PA1)" bidirectional line)
				(alternate "SPI2_SCK (PA0)" bidirectional line)
				(alternate "SYS_WKUP1 (PA0)" bidirectional line)
				(alternate "SYS_WKUP4 (PA2)" bidirectional line)
				(alternate "USART2_CK (PA1)" bidirectional line)
				(alternate "USART2_CTS (PA0)" bidirectional line)
				(alternate "USART2_DE (PA1)" bidirectional line)
				(alternate "USART2_NSS (PA0)" bidirectional line)
				(alternate "USART2_RTS (PA1)" bidirectional line)
				(alternate "USART2_TX (PA2)" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 2.54)
				(name "PB7/PB8/PB9/PC14")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 2.54)
				(name "PA8/PA9/PA11/PB0/PB1")
				(number "5")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "6")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 2.54)
				(name "PA13")
				(number "7")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 2.54)
				(name "PA14/PA15/PB5/PB6")
				(number "8")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G030K_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G030K_6-8_Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G030K_6-8_Tx_0_1")
		(symbol "STM32G030K_6-8_Tx_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G031C_4-6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G031C_4-6-8_Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G031C_4-6-8_Tx_0_1")
		(symbol "STM32G031C_4-6-8_Tx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G031C_4-6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G031C_4-6-8_Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G031C_4-6-8_Ux_0_1")
		(symbol "STM32G031C_4-6-8_Ux_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G031F_4-6-8_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G031F_4-6-8_Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32G031F_4-6-8_Px_0_1")
		(symbol "STM32G031F_4-6-8_Px_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "2")
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "15")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB2)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "16")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "17")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G031G_4-6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G031G_4-6-8_Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G031G_4-6-8_Ux_0_1")
		(symbol "STM32G031G_4-6-8_Ux_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "18")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "19")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G031J_4-6_Mx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 11.43 0)
		)
		(property "Value" "STM32G031J_4-6_Mx"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -27.94 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031j4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 6 GPIO, SO8N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STM32G031J_4-6_Mx_0_1")
		(symbol "STM32G031J_4-6_Mx_1_1"
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 2.54)
				(name "PB7/PB8/PB9/PC14")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 2.54)
				(name "PA0/PA1/PA2/PF2")
				(number "4")
				(alternate "ADC1_IN0 (PA0)" bidirectional line)
				(alternate "ADC1_IN1 (PA1)" bidirectional line)
				(alternate "ADC1_IN2 (PA2)" bidirectional line)
				(alternate "I2C1_SMBA (PA1)" bidirectional line)
				(alternate "I2S1_CK (PA1)" bidirectional line)
				(alternate "I2S1_SD (PA2)" bidirectional line)
				(alternate "LPTIM1_OUT (PA0)" bidirectional line)
				(alternate "LPUART1_TX (PA2)" bidirectional line)
				(alternate "PA0" bidirectional line)
				(alternate "PA1" bidirectional line)
				(alternate "PA2" bidirectional line)
				(alternate "PF2" bidirectional line)
				(alternate "RCC_LSCO (PA2)" bidirectional line)
				(alternate "RCC_MCO (PF2)" bidirectional line)
				(alternate "RTC_TAMP_IN2 (PA0)" bidirectional line)
				(alternate "SPI1_MOSI (PA2)" bidirectional line)
				(alternate "SPI1_SCK (PA1)" bidirectional line)
				(alternate "SPI2_SCK (PA0)" bidirectional line)
				(alternate "SYS_WKUP1 (PA0)" bidirectional line)
				(alternate "SYS_WKUP4 (PA2)" bidirectional line)
				(alternate "TIM2_CH1 (PA0)" bidirectional line)
				(alternate "TIM2_CH2 (PA1)" bidirectional line)
				(alternate "TIM2_CH3 (PA2)" bidirectional line)
				(alternate "TIM2_ETR (PA0)" bidirectional line)
				(alternate "USART2_CK (PA1)" bidirectional line)
				(alternate "USART2_CTS (PA0)" bidirectional line)
				(alternate "USART2_DE (PA1)" bidirectional line)
				(alternate "USART2_NSS (PA0)" bidirectional line)
				(alternate "USART2_RTS (PA1)" bidirectional line)
				(alternate "USART2_TX (PA2)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 2.54)
				(name "PA8/PA9/PA11/PB0/PB1")
				(number "5")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "6")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "7")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 2.54)
				(name "PA14/PA15/PB5/PB6")
				(number "8")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G031K_4-6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G031K_4-6-8_Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G031K_4-6-8_Tx_0_1")
		(symbol "STM32G031K_4-6-8_Tx_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G031K_4-6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G031K_4-6-8_Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G031K_4-6-8_Ux_0_1")
		(symbol "STM32G031K_4-6-8_Ux_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G031Y8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G031Y8Yx"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-18_1.86x2.14mm_Layout7x5_P0.4mm_Stagger"
			(at -22.86 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031y8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 16 GPIO, WLCSP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*1.86x2.14mm*Layout7x5*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32G031Y8Yx_0_1")
		(symbol "STM32G031Y8Yx_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC15")
				(number "A7")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "B4")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "A5")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "B6")
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "D6")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0/PF2")
				(number "E7")
				(alternate "ADC1_IN0 (PA0)" bidirectional line)
				(alternate "LPTIM1_OUT (PA0)" bidirectional line)
				(alternate "PA0" bidirectional line)
				(alternate "PF2" bidirectional line)
				(alternate "RCC_MCO (PF2)" bidirectional line)
				(alternate "RTC_TAMP_IN2 (PA0)" bidirectional line)
				(alternate "SPI2_SCK (PA0)" bidirectional line)
				(alternate "SYS_WKUP1 (PA0)" bidirectional line)
				(alternate "TIM2_CH1 (PA0)" bidirectional line)
				(alternate "TIM2_ETR (PA0)" bidirectional line)
				(alternate "USART2_CTS (PA0)" bidirectional line)
				(alternate "USART2_NSS (PA0)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "C5")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3/PA4")
				(number "D4")
				(alternate "ADC1_IN3 (PA3)" bidirectional line)
				(alternate "ADC1_IN4 (PA4)" bidirectional line)
				(alternate "I2S1_WS (PA4)" bidirectional line)
				(alternate "LPTIM2_OUT (PA4)" bidirectional line)
				(alternate "LPUART1_RX (PA3)" bidirectional line)
				(alternate "PA3" bidirectional line)
				(alternate "PA4" bidirectional line)
				(alternate "RTC_OUT_ALARM (PA4)" bidirectional line)
				(alternate "RTC_OUT_CALIB (PA4)" bidirectional line)
				(alternate "RTC_TAMP_IN1 (PA4)" bidirectional line)
				(alternate "RTC_TS (PA4)" bidirectional line)
				(alternate "SPI1_NSS (PA4)" bidirectional line)
				(alternate "SPI2_MISO (PA3)" bidirectional line)
				(alternate "SPI2_MOSI (PA4)" bidirectional line)
				(alternate "SYS_WKUP2 (PA4)" bidirectional line)
				(alternate "TIM14_CH1 (PA4)" bidirectional line)
				(alternate "TIM2_CH4 (PA3)" bidirectional line)
				(alternate "USART2_RX (PA3)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "C3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA7")
				(number "D2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "E1")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB2)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "C1")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "B2")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "A3")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G041C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G041C_6-8_Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G041C_6-8_Tx_0_1")
		(symbol "STM32G041C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G041C_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G041C_6-8_Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G041C_6-8_Ux_0_1")
		(symbol "STM32G041C_6-8_Ux_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G041F_6-8_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G041F_6-8_Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32G041F_6-8_Px_0_1")
		(symbol "STM32G041F_6-8_Px_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "2")
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "15")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB2)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "16")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "17")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G041G_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G041G_6-8_Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G041G_6-8_Ux_0_1")
		(symbol "STM32G041G_6-8_Ux_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "18")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "19")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G041J6Mx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 11.43 0)
		)
		(property "Value" "STM32G041J6Mx"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -27.94 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041j6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 6 GPIO, SO8N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STM32G041J6Mx_0_1")
		(symbol "STM32G041J6Mx_1_1"
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 2.54)
				(name "PB7/PB8/PB9/PC14")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 2.54)
				(name "PA0/PA1/PA2/PF2")
				(number "4")
				(alternate "ADC1_IN0 (PA0)" bidirectional line)
				(alternate "ADC1_IN1 (PA1)" bidirectional line)
				(alternate "ADC1_IN2 (PA2)" bidirectional line)
				(alternate "I2C1_SMBA (PA1)" bidirectional line)
				(alternate "I2S1_CK (PA1)" bidirectional line)
				(alternate "I2S1_SD (PA2)" bidirectional line)
				(alternate "LPTIM1_OUT (PA0)" bidirectional line)
				(alternate "LPUART1_TX (PA2)" bidirectional line)
				(alternate "PA0" bidirectional line)
				(alternate "PA1" bidirectional line)
				(alternate "PA2" bidirectional line)
				(alternate "PF2" bidirectional line)
				(alternate "RCC_LSCO (PA2)" bidirectional line)
				(alternate "RCC_MCO (PF2)" bidirectional line)
				(alternate "RTC_TAMP_IN2 (PA0)" bidirectional line)
				(alternate "SPI1_MOSI (PA2)" bidirectional line)
				(alternate "SPI1_SCK (PA1)" bidirectional line)
				(alternate "SPI2_SCK (PA0)" bidirectional line)
				(alternate "SYS_WKUP1 (PA0)" bidirectional line)
				(alternate "SYS_WKUP4 (PA2)" bidirectional line)
				(alternate "TIM2_CH1 (PA0)" bidirectional line)
				(alternate "TIM2_CH2 (PA1)" bidirectional line)
				(alternate "TIM2_CH3 (PA2)" bidirectional line)
				(alternate "TIM2_ETR (PA0)" bidirectional line)
				(alternate "USART2_CK (PA1)" bidirectional line)
				(alternate "USART2_CTS (PA0)" bidirectional line)
				(alternate "USART2_DE (PA1)" bidirectional line)
				(alternate "USART2_NSS (PA0)" bidirectional line)
				(alternate "USART2_RTS (PA1)" bidirectional line)
				(alternate "USART2_TX (PA2)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 2.54)
				(name "PA8/PA9/PA11/PB0/PB1")
				(number "5")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "6")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "7")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 2.54)
				(name "PA14/PA15/PB5/PB6")
				(number "8")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G041K_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G041K_6-8_Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G041K_6-8_Tx_0_1")
		(symbol "STM32G041K_6-8_Tx_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G041K_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G041K_6-8_Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G041K_6-8_Ux_0_1")
		(symbol "STM32G041K_6-8_Ux_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G041Y8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G041Y8Yx"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-18_1.86x2.14mm_Layout7x5_P0.4mm_Stagger"
			(at -22.86 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041y8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 16 GPIO, WLCSP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*1.86x2.14mm*Layout7x5*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32G041Y8Yx_0_1")
		(symbol "STM32G041Y8Yx_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC15")
				(number "A7")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "B4")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "A5")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "B6")
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "D6")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0/PF2")
				(number "E7")
				(alternate "ADC1_IN0 (PA0)" bidirectional line)
				(alternate "LPTIM1_OUT (PA0)" bidirectional line)
				(alternate "PA0" bidirectional line)
				(alternate "PF2" bidirectional line)
				(alternate "RCC_MCO (PF2)" bidirectional line)
				(alternate "RTC_TAMP_IN2 (PA0)" bidirectional line)
				(alternate "SPI2_SCK (PA0)" bidirectional line)
				(alternate "SYS_WKUP1 (PA0)" bidirectional line)
				(alternate "TIM2_CH1 (PA0)" bidirectional line)
				(alternate "TIM2_ETR (PA0)" bidirectional line)
				(alternate "USART2_CTS (PA0)" bidirectional line)
				(alternate "USART2_NSS (PA0)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "C5")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3/PA4")
				(number "D4")
				(alternate "ADC1_IN3 (PA3)" bidirectional line)
				(alternate "ADC1_IN4 (PA4)" bidirectional line)
				(alternate "I2S1_WS (PA4)" bidirectional line)
				(alternate "LPTIM2_OUT (PA4)" bidirectional line)
				(alternate "LPUART1_RX (PA3)" bidirectional line)
				(alternate "PA3" bidirectional line)
				(alternate "PA4" bidirectional line)
				(alternate "RTC_OUT_ALARM (PA4)" bidirectional line)
				(alternate "RTC_OUT_CALIB (PA4)" bidirectional line)
				(alternate "RTC_TAMP_IN1 (PA4)" bidirectional line)
				(alternate "RTC_TS (PA4)" bidirectional line)
				(alternate "SPI1_NSS (PA4)" bidirectional line)
				(alternate "SPI2_MISO (PA3)" bidirectional line)
				(alternate "SPI2_MOSI (PA4)" bidirectional line)
				(alternate "SYS_WKUP2 (PA4)" bidirectional line)
				(alternate "TIM14_CH1 (PA4)" bidirectional line)
				(alternate "TIM2_CH4 (PA3)" bidirectional line)
				(alternate "USART2_RX (PA3)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "C3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA7")
				(number "D2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "E1")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB2)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "C1")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "B2")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "A3")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G050C6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G050C6Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g050c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 2.0-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G050C6Tx_0_1")
		(symbol "STM32G050C6Tx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G050C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G050C8Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g050c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 2.0-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G050C8Tx_0_1")
		(symbol "STM32G050C8Tx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G050F6Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G050F6Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g050f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 2.0-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32G050F6Px_0_1")
		(symbol "STM32G050F6Px_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM15_BK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "2")
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "15")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "16")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "17")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G050K6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G050K6Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g050k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 2.0-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G050K6Tx_0_1")
		(symbol "STM32G050K6Tx_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G050K8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G050K8Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g050k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 2.0-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G050K8Tx_0_1")
		(symbol "STM32G050K8Tx_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G051C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G051C_6-8_Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G051C_6-8_Tx_0_1")
		(symbol "STM32G051C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G051C_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G051C_6-8_Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G051C_6-8_Ux_0_1")
		(symbol "STM32G051C_6-8_Ux_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G051F8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G051F8Yx"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-20_1.94x2.4mm_Layout4x5_P0.4mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, WLCSP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*1.94x2.4mm*Layout4x5*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G051F8Yx_0_1")
		(symbol "STM32G051F8Yx_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "E4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "B4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "A2")
				(alternate "COMP2_INM (PB3)" bidirectional line)
				(alternate "COMP2_INP (PB4)" bidirectional line)
				(alternate "COMP2_INP (PB6)" bidirectional line)
				(alternate "COMP2_OUT (PB5)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "A3")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "COMP2_INM (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM15_BK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "A4")
				(alternate "DAC1_EXTI9 (PB9)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "C3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "D3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "E3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "C2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "E2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "D2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "C1")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "D1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "E1")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "COMP1_INM (PB1)" bidirectional line)
				(alternate "COMP1_INP (PB2)" bidirectional line)
				(alternate "COMP1_OUT (PB0)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB2)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "B1")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "A1")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "B3")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G051F_6-8_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G051F_6-8_Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32G051F_6-8_Px_0_1")
		(symbol "STM32G051F_6-8_Px_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "COMP2_INM (PB3)" bidirectional line)
				(alternate "COMP2_INP (PB4)" bidirectional line)
				(alternate "COMP2_INP (PB6)" bidirectional line)
				(alternate "COMP2_OUT (PB5)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "COMP2_INM (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM15_BK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "2")
				(alternate "DAC1_EXTI9 (PB9)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "15")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "COMP1_INM (PB1)" bidirectional line)
				(alternate "COMP1_INP (PB2)" bidirectional line)
				(alternate "COMP1_OUT (PB0)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB2)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "16")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "17")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G051G_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G051G_6-8_Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G051G_6-8_Ux_0_1")
		(symbol "STM32G051G_6-8_Ux_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "18")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "19")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G051K_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G051K_6-8_Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G051K_6-8_Tx_0_1")
		(symbol "STM32G051K_6-8_Tx_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G051K_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G051K_6-8_Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G051K_6-8_Ux_0_1")
		(symbol "STM32G051K_6-8_Ux_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G061C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G061C_6-8_Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G061C_6-8_Tx_0_1")
		(symbol "STM32G061C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G061C_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G061C_6-8_Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G061C_6-8_Ux_0_1")
		(symbol "STM32G061C_6-8_Ux_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G061F8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G061F8Yx"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-20_1.94x2.4mm_Layout4x5_P0.4mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, WLCSP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*1.94x2.4mm*Layout4x5*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G061F8Yx_0_1")
		(symbol "STM32G061F8Yx_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "E4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "B4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "A2")
				(alternate "COMP2_INM (PB3)" bidirectional line)
				(alternate "COMP2_INP (PB4)" bidirectional line)
				(alternate "COMP2_INP (PB6)" bidirectional line)
				(alternate "COMP2_OUT (PB5)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "A3")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "COMP2_INM (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM15_BK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "A4")
				(alternate "DAC1_EXTI9 (PB9)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "C3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "D3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "E3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "C2")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "E2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "D2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "C1")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "D1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "E1")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "COMP1_INM (PB1)" bidirectional line)
				(alternate "COMP1_INP (PB2)" bidirectional line)
				(alternate "COMP1_OUT (PB0)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB2)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "B1")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "A1")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "B3")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G061F_6-8_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G061F_6-8_Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32G061F_6-8_Px_0_1")
		(symbol "STM32G061F_6-8_Px_1_1"
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB3/PB4/PB5/PB6")
				(number "20")
				(alternate "COMP2_INM (PB3)" bidirectional line)
				(alternate "COMP2_INP (PB4)" bidirectional line)
				(alternate "COMP2_INP (PB6)" bidirectional line)
				(alternate "COMP2_OUT (PB5)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C1_SMBA (PB5)" bidirectional line)
				(alternate "I2S1_CK (PB3)" bidirectional line)
				(alternate "I2S1_MCK (PB4)" bidirectional line)
				(alternate "I2S1_SD (PB5)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "PB3" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "SPI1_SCK (PB3)" bidirectional line)
				(alternate "SPI2_MISO (PB6)" bidirectional line)
				(alternate "SYS_WKUP6 (PB5)" bidirectional line)
				(alternate "TIM16_BK (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM17_BK (PB4)" bidirectional line)
				(alternate "TIM1_CH2 (PB3)" bidirectional line)
				(alternate "TIM1_CH3 (PB6)" bidirectional line)
				(alternate "TIM2_CH2 (PB3)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "USART1_CK (PB3)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_DE (PB3)" bidirectional line)
				(alternate "USART1_NSS (PB4)" bidirectional line)
				(alternate "USART1_RTS (PB3)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB7/PB8")
				(number "1")
				(alternate "ADC1_IN11 (PB7)" bidirectional line)
				(alternate "COMP2_INM (PB7)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB7)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB7)" bidirectional line)
				(alternate "PB7" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "SPI2_MOSI (PB7)" bidirectional line)
				(alternate "SPI2_SCK (PB8)" bidirectional line)
				(alternate "SYS_PVD_IN (PB7)" bidirectional line)
				(alternate "TIM15_BK (PB8)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "TIM17_CH1N (PB7)" bidirectional line)
				(alternate "USART1_RX (PB7)" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB9/PC14")
				(number "2")
				(alternate "DAC1_EXTI9 (PB9)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "PC14" bidirectional line)
				(alternate "RCC_OSC32_IN (PC14)" bidirectional line)
				(alternate "RCC_OSC_IN (PC14)" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM17_CH1 (PB9)" bidirectional line)
				(alternate "TIM1_BK2 (PC14)" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA8/PB0/PB1/PB2")
				(number "15")
				(alternate "ADC1_IN10 (PB2)" bidirectional line)
				(alternate "ADC1_IN8 (PB0)" bidirectional line)
				(alternate "ADC1_IN9 (PB1)" bidirectional line)
				(alternate "COMP1_INM (PB1)" bidirectional line)
				(alternate "COMP1_INP (PB2)" bidirectional line)
				(alternate "COMP1_OUT (PB0)" bidirectional line)
				(alternate "I2S1_WS (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB0)" bidirectional line)
				(alternate "LPTIM1_OUT (PB2)" bidirectional line)
				(alternate "LPTIM2_IN1 (PB1)" bidirectional line)
				(alternate "LPTIM2_OUT (PA8)" bidirectional line)
				(alternate "LPUART1_DE (PB1)" bidirectional line)
				(alternate "LPUART1_RTS (PB1)" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "PB1" bidirectional line)
				(alternate "PB2" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "SPI2_MISO (PB2)" bidirectional line)
				(alternate "SPI2_NSS (PA8)" bidirectional line)
				(alternate "TIM14_CH1 (PB1)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM1_CH3N (PB1)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TIM3_CH4 (PB1)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "16")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "17")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14/PA15")
				(number "19")
				(alternate "ADC1_IN18 (PA14)" bidirectional line)
				(alternate "I2S1_WS (PA15)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PA15" bidirectional line)
				(alternate "SPI1_NSS (PA15)" bidirectional line)
				(alternate "SYS_SWCLK (PA14)" bidirectional line)
				(alternate "TIM2_CH1 (PA15)" bidirectional line)
				(alternate "TIM2_ETR (PA15)" bidirectional line)
				(alternate "USART2_RX (PA15)" bidirectional line)
				(alternate "USART2_TX (PA14)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G061G_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G061G_6-8_Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G061G_6-8_Ux_0_1")
		(symbol "STM32G061G_6-8_Ux_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "18")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "19")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G061K_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G061K_6-8_Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G061K_6-8_Tx_0_1")
		(symbol "STM32G061K_6-8_Tx_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G061K_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G061K_6-8_Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G061K_6-8_Ux_0_1")
		(symbol "STM32G061K_6-8_Ux_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "ADC1_IN15 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "ADC1_IN16 (PA12)" bidirectional line)
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G070CBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G070CBTx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g070cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 2.0-3.6V, 43 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G070CBTx_0_1")
		(symbol "STM32G070CBTx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "10")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G070KBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G070KBTx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g070kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 2.0-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G070KBTx_0_1")
		(symbol "STM32G070KBTx_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G070RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G070RBTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g070rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 2.0-3.6V, 59 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G070RBTx_0_1")
		(symbol "STM32G070RBTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "12")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "40")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "41")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "14")
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "42")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "37")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "43")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "44")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G071EBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G071EBYx"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_2.3x2.48mm_Layout5x5_P0.4mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071eb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 23 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.3x2.48mm*Layout5x5*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G071EBYx_0_1")
		(symbol "STM32G071EBYx_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "E5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "A5")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "B5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "E2")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "E1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB5")
				(number "A3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB8")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "D5")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "C4")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "D4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "E4")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "C3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "D3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "E3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "C2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA7")
				(number "D2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "C1")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "B1")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "A2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A1")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G071G_8-B_UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G071G_8-B_UxN"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64-128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G071G_8-B_UxN_0_1")
		(symbol "STM32G071G_8-B_UxN_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD0")
				(number "22")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD1")
				(number "23")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD2")
				(number "24")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD3")
				(number "25")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB15")
				(number "15")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "18")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "19")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G071K_8-B_TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "STM32G071K_8-B_TxN"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64-128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G071K_8-B_TxN_0_1")
		(symbol "STM32G071K_8-B_TxN_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD0")
				(number "26")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD1")
				(number "27")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "28")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PD3")
				(number "29")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB15")
				(number "17")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G071K_8-B_UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "STM32G071K_8-B_UxN"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64-128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G071K_8-B_UxN_0_1")
		(symbol "STM32G071K_8-B_UxN_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD0")
				(number "26")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD1")
				(number "27")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "28")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PD3")
				(number "29")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB15")
				(number "17")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G071RBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G071RBIx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G071RBIx_0_1")
		(symbol "STM32G071RBIx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "D2")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "G1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "A7")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "A6")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "C5")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "B5")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "A5")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD8")
				(number "E8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PD9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC1")
				(number "F2")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC2")
				(number "G2")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC3")
				(number "H1")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC6")
				(number "E7")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC7")
				(number "E5")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC8")
				(number "A8")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC13")
				(number "C2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "D3")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "E1")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "H2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "F8")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "C8")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "E6")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "B8")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "D6")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D7")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H7")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "B4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G6")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G7")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081CBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G081CBTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081CBTx_0_1")
		(symbol "STM32G081CBTx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G081CBUx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081CBUx_0_1")
		(symbol "STM32G081CBUx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081EBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G081EBYx"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_2.3x2.48mm_Layout5x5_P0.4mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081eb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 23 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.3x2.48mm*Layout5x5*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081EBYx_0_1")
		(symbol "STM32G081EBYx_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "E5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "A5")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "B5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "E2")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "E1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB5")
				(number "A3")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB8")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "D5")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "C4")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "D4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "E4")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "C3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "D3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "E3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "C2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA7")
				(number "D2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "C1")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "B1")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "A2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A1")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081GBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G081GBUx"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081gb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081GBUx_0_1")
		(symbol "STM32G081GBUx_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "23")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "24")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "25")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "18")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "19")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "22")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081GBUxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G081GBUxN"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081gb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081GBUxN_0_1")
		(symbol "STM32G081GBUxN_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "5")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD0")
				(number "22")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD1")
				(number "23")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD2")
				(number "24")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD3")
				(number "25")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "17")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "28")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB15")
				(number "15")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "16")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "18")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "19")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "20")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "21")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081KBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G081KBTx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081KBTx_0_1")
		(symbol "STM32G081KBTx_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081KBTxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "STM32G081KBTxN"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081KBTxN_0_1")
		(symbol "STM32G081KBTxN_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD0")
				(number "26")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD1")
				(number "27")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "28")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PD3")
				(number "29")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB15")
				(number "17")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081KBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G081KBUx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081KBUx_0_1")
		(symbol "STM32G081KBUx_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081KBUxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "STM32G081KBUxN"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081KBUxN_0_1")
		(symbol "STM32G081KBUxN_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD0")
				(number "26")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD1")
				(number "27")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "28")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PD3")
				(number "29")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB15")
				(number "17")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081RBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G081RBIx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081RBIx_0_1")
		(symbol "STM32G081RBIx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "D2")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "G1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "A7")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "A6")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "C5")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "B5")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "A5")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD8")
				(number "E8")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PD9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC1")
				(number "F2")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC2")
				(number "G2")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC3")
				(number "H1")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC6")
				(number "E7")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC7")
				(number "E5")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC8")
				(number "A8")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC13")
				(number "C2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "D3")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "E1")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "H2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "F8")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "C8")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "E6")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "B8")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "D6")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D7")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C6")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H7")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "B4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G6")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G7")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G081RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G081RBTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g081rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G081RBTx_0_1")
		(symbol "STM32G081RBTx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD8")
				(number "40")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PD9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC0")
				(number "13")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC1")
				(number "14")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "43")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "37")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "44")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "42")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "CEC" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B0CETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G0B0CETx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b0ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 2.0-3.6V, 43 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B0CETx_0_1")
		(symbol "STM32G0B0CETx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "10")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "29")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B0KETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G0B0KETx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b0ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 2.0-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B0KETx_0_1")
		(symbol "STM32G0B0KETx_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "19")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B0RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G0B0RETx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b0re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 2.0-3.6V, 59 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B0RETx_0_1")
		(symbol "STM32G0B0RETx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "12")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "40")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "41")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "13")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "14")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA10")
				(number "42")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -15.24 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC/PA9")
				(number "37")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "43")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "44")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B0VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G0B0VETx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -68.58 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b0ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 2.0-3.6V, 93 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B0VETx_0_1")
		(symbol "STM32G0B0VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "17")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "VREF+")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "15")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "16")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF3")
				(number "18")
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF4")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF5")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PF6")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PF7")
				(number "39")
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PF8")
				(number "72")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PF9")
				(number "86")
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PF10")
				(number "87")
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PF11")
				(number "88")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PF12")
				(number "89")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PF13")
				(number "90")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE0")
				(number "94")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE1")
				(number "95")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE2")
				(number "96")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE3")
				(number "97")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE4")
				(number "4")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE5")
				(number "5")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE6")
				(number "6")
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE7")
				(number "40")
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE8")
				(number "41")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE9")
				(number "42")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PE10")
				(number "43")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PE11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PE12")
				(number "45")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PE13")
				(number "46")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PE14")
				(number "47")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PE15")
				(number "48")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD0")
				(number "78")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD1")
				(number "79")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD2")
				(number "80")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD3")
				(number "81")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD4")
				(number "82")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD5")
				(number "83")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD6")
				(number "84")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD7")
				(number "85")
				(alternate "RCC_MCO_2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD8")
				(number "59")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD9")
				(number "60")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -50.8 0)
				(length 5.08)
				(name "PD10")
				(number "61")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 5.08)
				(name "PD11")
				(number "62")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -55.88 0)
				(length 5.08)
				(name "PD12")
				(number "65")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -58.42 0)
				(length 5.08)
				(name "PD13")
				(number "66")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -60.96 0)
				(length 5.08)
				(name "PD14")
				(number "67")
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -63.5 0)
				(length 5.08)
				(name "PD15")
				(number "68")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin no_connect line
				(at -17.78 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC/PA10")
				(number "69")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin no_connect line
				(at -17.78 -68.58 0)
				(length 5.08)
				(hide yes)
				(name "NC/PA9")
				(number "56")
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "NC" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "25")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "26")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "27")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "28")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "55")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9/PA11")
				(number "70")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10/PA12")
				(number "71")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA13")
				(number "73")
				(alternate "IR_OUT" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA14")
				(number "74")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA15")
				(number "75")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB3")
				(number "91")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB4")
				(number "92")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB5")
				(number "93")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB6")
				(number "98")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB7")
				(number "99")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB8")
				(number "100")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB9")
				(number "1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB10")
				(number "49")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PC0")
				(number "21")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "PC1")
				(number "22")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC2")
				(number "23")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC3")
				(number "24")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC6")
				(number "57")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC7")
				(number "58")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC8")
				(number "76")
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC9")
				(number "77")
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC10")
				(number "2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC11")
				(number "3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC12")
				(number "7")
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1C_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1C_B-C-E_Tx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1C_B-C-E_Tx_0_1")
		(symbol "STM32G0B1C_B-C-E_Tx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1C_B-C-E_TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0B1C_B-C-E_TxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1C_B-C-E_TxN_0_1")
		(symbol "STM32G0B1C_B-C-E_TxN_1_1"
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1C_B-C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1C_B-C-E_Ux"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1C_B-C-E_Ux_0_1")
		(symbol "STM32G0B1C_B-C-E_Ux_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1C_B-C-E_UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0B1C_B-C-E_UxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1C_B-C-E_UxN_0_1")
		(symbol "STM32G0B1C_B-C-E_UxN_1_1"
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1K_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0B1K_B-C-E_Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1K_B-C-E_Tx_0_1")
		(symbol "STM32G0B1K_B-C-E_Tx_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1K_B-C-E_TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0B1K_B-C-E_TxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1K_B-C-E_TxN_0_1")
		(symbol "STM32G0B1K_B-C-E_TxN_1_1"
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD0")
				(number "26")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD1")
				(number "27")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD2")
				(number "28")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD3")
				(number "29")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB15")
				(number "17")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1K_B-C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0B1K_B-C-E_Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1K_B-C-E_Ux_0_1")
		(symbol "STM32G0B1K_B-C-E_Ux_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1K_B-C-E_UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0B1K_B-C-E_UxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1K_B-C-E_UxN_0_1")
		(symbol "STM32G0B1K_B-C-E_UxN_1_1"
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD0")
				(number "26")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD1")
				(number "27")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD2")
				(number "28")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD3")
				(number "29")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB15")
				(number "17")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1M_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 64.77 0)
		)
		(property "Value" "STM32G0B1M_B-C-E_Tx"
			(at 5.08 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -25.4 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 74 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1M_B-C-E_Tx_0_1")
		(symbol "STM32G0B1M_B-C-E_Tx_1_1"
			(pin input line
				(at -27.94 58.42 0)
				(length 2.54)
				(name "VREF+")
				(number "9")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 2.54)
				(name "PF0")
				(number "12")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 2.54)
				(name "PF1")
				(number "13")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 2.54)
				(name "PF2")
				(number "14")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 2.54)
				(name "PE0")
				(number "75")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "PE1")
				(number "76")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "PE3")
				(number "77")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PE7")
				(number "32")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PE8")
				(number "33")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PE9")
				(number "34")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "PE10")
				(number "35")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "64")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "65")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "66")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "67")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "68")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "69")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "70")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PD7")
				(number "71")
				(alternate "RCC_MCO_2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PD8")
				(number "46")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PD9")
				(number "47")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PD10")
				(number "48")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PD11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PD12")
				(number "52")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PD13")
				(number "53")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PD14")
				(number "54")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PD15")
				(number "55")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC0")
				(number "15")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC1")
				(number "16")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC2")
				(number "17")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC3")
				(number "18")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC4")
				(number "27")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC5")
				(number "28")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PC6")
				(number "44")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PC7")
				(number "45")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 2.54)
				(name "PC8")
				(number "62")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 2.54)
				(name "PC9")
				(number "63")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 2.54)
				(name "PC10")
				(number "2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 2.54)
				(name "PC11")
				(number "3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 2.54)
				(name "PC12")
				(number "4")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 2.54)
				(name "PC13")
				(number "5")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 2.54)
				(name "PC14")
				(number "6")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 2.54)
				(name "PC15")
				(number "7")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 2.54)
				(name "VBAT")
				(number "8")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 2.54)
				(name "PA0")
				(number "19")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 2.54)
				(name "PA1")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 2.54)
				(name "PA2")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 2.54)
				(name "PA3")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 2.54)
				(name "PA4")
				(number "23")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 2.54)
				(name "PA5")
				(number "24")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 2.54)
				(name "PA6")
				(number "25")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA7")
				(number "26")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "57")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "43")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "58")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "56")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA13")
				(number "59")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA14")
				(number "60")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA15")
				(number "61")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PB0")
				(number "29")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "30")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PB6")
				(number "78")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "79")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB8")
				(number "80")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB10")
				(number "36")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB12")
				(number "38")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB13")
				(number "39")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB14")
				(number "40")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB15")
				(number "41")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1NEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1NEYx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-52_3.09x3.15mm_Layout13x8_P0.4mm_Stagger"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ne.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 46 GPIO, WLCSP52"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.09x3.15mm*Layout13x8*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1NEYx_0_1")
		(symbol "STM32G0B1NEYx_1_1"
			(pin input line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "VREF+")
				(number "D11")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PF0")
				(number "F13")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PF1")
				(number "G12")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PF2")
				(number "F11")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PD0")
				(number "A4")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PD1")
				(number "C6")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PD3")
				(number "A6")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PC4")
				(number "G8")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PC5")
				(number "G6")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PC6")
				(number "D5")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PC7")
				(number "D3")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PC13")
				(number "B11")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PC14")
				(number "B13")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PC15")
				(number "C12")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 5.08)
				(name "VBAT")
				(number "C10")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 5.08)
				(name "VDD")
				(number "D1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E12")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 5.08)
				(name "VSS")
				(number "E2")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 5.08)
				(name "VDD")
				(number "D13")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA0")
				(number "H13")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA1")
				(number "E10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA2")
				(number "E8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA3")
				(number "H11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA4")
				(number "G10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA5")
				(number "F9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA6")
				(number "F7")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA7")
				(number "H9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PA8")
				(number "F1")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PA9/PA11")
				(number "C2")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PA9/UCPD1_DBCC1")
				(number "E4")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PA10/PA12")
				(number "B1")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PA10/UCPD1_DBCC2")
				(number "C4")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PA13")
				(number "B3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PA14")
				(number "B5")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PA15")
				(number "A2")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB0")
				(number "H7")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB2")
				(number "G4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB4")
				(number "B9")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB5")
				(number "A10")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB6")
				(number "C8")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PB7")
				(number "D7")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PB8")
				(number "A12")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PB9")
				(number "D9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PB10")
				(number "H3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PB11")
				(number "F5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PB12")
				(number "E6")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PB13")
				(number "H1")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PB14")
				(number "G2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PB15")
				(number "F3")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1R_B-C-E_IxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1R_B-C-E_IxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1R_B-C-E_IxN_0_1")
		(symbol "STM32G0B1R_B-C-E_IxN_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "D2")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "F1")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "G1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "A7")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "A6")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "C5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "B5")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "A5")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC1")
				(number "F2")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC2")
				(number "G2")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC3")
				(number "H1")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC6")
				(number "E7")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC7")
				(number "E5")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC8")
				(number "A8")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC13")
				(number "C2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "D3")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "E1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D8")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "H2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "F8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "C8")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "E6")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "B8")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "D6")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D7")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C7")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C6")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H7")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "B4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G6")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G7")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1R_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1R_B-C-E_Tx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1R_B-C-E_Tx_0_1")
		(symbol "STM32G0B1R_B-C-E_Tx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD8")
				(number "40")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PD9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC0")
				(number "13")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC1")
				(number "14")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "43")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "37")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "44")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "42")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1R_B-C-E_TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1R_B-C-E_TxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1R_B-C-E_TxN_0_1")
		(symbol "STM32G0B1R_B-C-E_TxN_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC0")
				(number "13")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC1")
				(number "14")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "43")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "37")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "44")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "42")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1V_B-C-E_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0B1V_B-C-E_Ix"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1V_B-C-E_Ix_0_1")
		(symbol "STM32G0B1V_B-C-E_Ix_1_1"
			(pin input line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "F2")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PF0")
				(number "H1")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PF1")
				(number "J1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PF2")
				(number "G2")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PF3")
				(number "H3")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PF4")
				(number "H2")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PF5")
				(number "J2")
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PF6")
				(number "M6")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PF7")
				(number "L7")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PF8")
				(number "D10")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PF9")
				(number "A8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PF10")
				(number "B7")
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PF11")
				(number "A7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PF12")
				(number "B6")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PF13")
				(number "A6")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "B4")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "A3")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "C2")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE6")
				(number "C1")
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE8")
				(number "M8")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PE9")
				(number "K8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PE14")
				(number "K9")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PE15")
				(number "L10")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD0")
				(number "B10")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD1")
				(number "C9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD2")
				(number "A11")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD4")
				(number "B9")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD5")
				(number "A10")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD6")
				(number "A9")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD7")
				(number "B8")
				(alternate "RCC_MCO_2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD8")
				(number "J12")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PD9")
				(number "H11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PD10")
				(number "H12")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PD11")
				(number "G11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PD12")
				(number "F11")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PD13")
				(number "E12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PD14")
				(number "E11")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PD15")
				(number "D11")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F1")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "G1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F12")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "K3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "L2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "M1")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "K4")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "M2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "M3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "L12")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA9/PA11")
				(number "D12")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9/UCPD1_DBCC1")
				(number "H10")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10/PA12")
				(number "C12")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA10/UCPD1_DBCC2")
				(number "E10")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "C11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "B12")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "L5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB8")
				(number "A1")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "C3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "M11")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K10")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "M12")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "J10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "K1")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J3")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "K2")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "L1")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "L4")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "M4")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "J11")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "K12")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "C10")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "A12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "D2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0B1V_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0B1V_B-C-E_Tx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0B1V_B-C-E_Tx_0_1")
		(symbol "STM32G0B1V_B-C-E_Tx_1_1"
			(pin input line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "12")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PF0")
				(number "15")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PF1")
				(number "16")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PF2")
				(number "17")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PF3")
				(number "18")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PF4")
				(number "19")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PF5")
				(number "20")
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PF6")
				(number "38")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PF7")
				(number "39")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PF8")
				(number "72")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PF9")
				(number "86")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PF10")
				(number "87")
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PF11")
				(number "88")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PF12")
				(number "89")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PF13")
				(number "90")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "94")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "95")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "96")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "97")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "4")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE5")
				(number "5")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE6")
				(number "6")
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE7")
				(number "40")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE8")
				(number "41")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PE9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PE10")
				(number "43")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PE11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PE12")
				(number "45")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PE13")
				(number "46")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PE14")
				(number "47")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PE15")
				(number "48")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD0")
				(number "78")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD1")
				(number "79")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD2")
				(number "80")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD3")
				(number "81")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD4")
				(number "82")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD5")
				(number "83")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD6")
				(number "84")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD7")
				(number "85")
				(alternate "RCC_MCO_2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD8")
				(number "59")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PD9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PD10")
				(number "61")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PD11")
				(number "62")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PD12")
				(number "65")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PD13")
				(number "66")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PD14")
				(number "67")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PD15")
				(number "68")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "25")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "26")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "27")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "28")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "55")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA9/PA11")
				(number "70")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9/UCPD1_DBCC1")
				(number "56")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10/PA12")
				(number "71")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA10/UCPD1_DBCC2")
				(number "69")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "73")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "74")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "75")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "91")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "93")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "98")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "99")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB8")
				(number "100")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "49")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "21")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "22")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "23")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "24")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "57")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "58")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "76")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "77")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "7")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1C_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1C_C-E_Tx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1C_C-E_Tx_0_1")
		(symbol "STM32G0C1C_C-E_Tx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1C_C-E_TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0C1C_C-E_TxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1C_C-E_TxN_0_1")
		(symbol "STM32G0C1C_C-E_TxN_1_1"
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1C_C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1C_C-E_Ux"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1C_C-E_Ux_0_1")
		(symbol "STM32G0C1C_C-E_Ux_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "30")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC7")
				(number "31")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1C_C-E_UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0C1C_C-E_UxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1C_C-E_UxN_0_1")
		(symbol "STM32G0C1C_C-E_UxN_1_1"
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF0")
				(number "8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF1")
				(number "9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "PF2")
				(number "10")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "38")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "39")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "40")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "41")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PB0")
				(number "19")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "42")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "44")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "46")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "47")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "23")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "24")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "25")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "26")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "27")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "11")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "15")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "16")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "17")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "18")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "28")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "33")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "29")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "34")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "32")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "35")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "36")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA15")
				(number "37")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1K_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0C1K_C-E_Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1K_C-E_Tx_0_1")
		(symbol "STM32G0C1K_C-E_Tx_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1K_C-E_TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0C1K_C-E_TxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1K_C-E_TxN_0_1")
		(symbol "STM32G0C1K_C-E_TxN_1_1"
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD0")
				(number "26")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD1")
				(number "27")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD2")
				(number "28")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD3")
				(number "29")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB15")
				(number "17")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1K_C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0C1K_C-E_Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1K_C-E_Ux_0_1")
		(symbol "STM32G0C1K_C-E_Ux_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC6")
				(number "20")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB2")
				(number "17")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "27")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "29")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "26")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1K_C-E_UxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0C1K_C-E_UxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1K_C-E_UxN_0_1")
		(symbol "STM32G0C1K_C-E_UxN_1_1"
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD0")
				(number "26")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD1")
				(number "27")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD2")
				(number "28")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD3")
				(number "29")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB0")
				(number "15")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB1")
				(number "16")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "31")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PB15")
				(number "17")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "7")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "12")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "13")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "14")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "22")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "19")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "23")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "21")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "24")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1M_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 64.77 0)
		)
		(property "Value" "STM32G0C1M_C-E_Tx"
			(at 5.08 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -25.4 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 74 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1M_C-E_Tx_0_1")
		(symbol "STM32G0C1M_C-E_Tx_1_1"
			(pin input line
				(at -27.94 58.42 0)
				(length 2.54)
				(name "VREF+")
				(number "9")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 2.54)
				(name "PF0")
				(number "12")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 2.54)
				(name "PF1")
				(number "13")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 2.54)
				(name "PF2")
				(number "14")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 2.54)
				(name "PE0")
				(number "75")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "PE1")
				(number "76")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "PE3")
				(number "77")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PE7")
				(number "32")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PE8")
				(number "33")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PE9")
				(number "34")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "PE10")
				(number "35")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "64")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "65")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "66")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "67")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "68")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "69")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "70")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PD7")
				(number "71")
				(alternate "RCC_MCO_2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PD8")
				(number "46")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PD9")
				(number "47")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PD10")
				(number "48")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PD11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PD12")
				(number "52")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PD13")
				(number "53")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PD14")
				(number "54")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PD15")
				(number "55")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC0")
				(number "15")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC1")
				(number "16")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC2")
				(number "17")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC3")
				(number "18")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC4")
				(number "27")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC5")
				(number "28")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PC6")
				(number "44")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PC7")
				(number "45")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 2.54)
				(name "PC8")
				(number "62")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 2.54)
				(name "PC9")
				(number "63")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 2.54)
				(name "PC10")
				(number "2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 2.54)
				(name "PC11")
				(number "3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 2.54)
				(name "PC12")
				(number "4")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 2.54)
				(name "PC13")
				(number "5")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 2.54)
				(name "PC14")
				(number "6")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 2.54)
				(name "PC15")
				(number "7")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 2.54)
				(name "VBAT")
				(number "8")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 2.54)
				(name "PA0")
				(number "19")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 2.54)
				(name "PA1")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 2.54)
				(name "PA2")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 2.54)
				(name "PA3")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 2.54)
				(name "PA4")
				(number "23")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 2.54)
				(name "PA5")
				(number "24")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 2.54)
				(name "PA6")
				(number "25")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA7")
				(number "26")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "57")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "43")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "58")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "56")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA13")
				(number "59")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA14")
				(number "60")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA15")
				(number "61")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PB0")
				(number "29")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "30")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PB6")
				(number "78")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "79")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB8")
				(number "80")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB10")
				(number "36")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB11")
				(number "37")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB12")
				(number "38")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB13")
				(number "39")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB14")
				(number "40")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB15")
				(number "41")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1NEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1NEYx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-52_3.09x3.15mm_Layout13x8_P0.4mm_Stagger"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ne.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 46 GPIO, WLCSP52"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.09x3.15mm*Layout13x8*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1NEYx_0_1")
		(symbol "STM32G0C1NEYx_1_1"
			(pin input line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "VREF+")
				(number "D11")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PF0")
				(number "F13")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PF1")
				(number "G12")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PF2")
				(number "F11")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PD0")
				(number "A4")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PD1")
				(number "C6")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PD3")
				(number "A6")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PC4")
				(number "G8")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PC5")
				(number "G6")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PC6")
				(number "D5")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PC7")
				(number "D3")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PC13")
				(number "B11")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PC14")
				(number "B13")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PC15")
				(number "C12")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 5.08)
				(name "VBAT")
				(number "C10")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 5.08)
				(name "VDD")
				(number "D1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E12")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 5.08)
				(name "VSS")
				(number "E2")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 5.08)
				(name "VDD")
				(number "D13")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA0")
				(number "H13")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA1")
				(number "E10")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA2")
				(number "E8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA3")
				(number "H11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA4")
				(number "G10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA5")
				(number "F9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA6")
				(number "F7")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA7")
				(number "H9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PA8")
				(number "F1")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PA9/PA11")
				(number "C2")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PA9/UCPD1_DBCC1")
				(number "E4")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PA10/PA12")
				(number "B1")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PA10/UCPD1_DBCC2")
				(number "C4")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PA13")
				(number "B3")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PA14")
				(number "B5")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PA15")
				(number "A2")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB0")
				(number "H7")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB2")
				(number "G4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB4")
				(number "B9")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB5")
				(number "A10")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB6")
				(number "C8")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PB7")
				(number "D7")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PB8")
				(number "A12")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PB9")
				(number "D9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PB10")
				(number "H3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PB11")
				(number "F5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PB12")
				(number "E6")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PB13")
				(number "H1")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PB14")
				(number "G2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PB15")
				(number "F3")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1R_C-E_IxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1R_C-E_IxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1R_C-E_IxN_0_1")
		(symbol "STM32G0C1R_C-E_IxN_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "D2")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "F1")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "G1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "A7")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "A6")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "C5")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "B5")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "A5")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC1")
				(number "F2")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC2")
				(number "G2")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC3")
				(number "H1")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC6")
				(number "E7")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC7")
				(number "E5")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC8")
				(number "A8")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC11")
				(number "A1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC13")
				(number "C2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "D3")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "E1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D8")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "H2")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "F4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "F8")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "C8")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "E6")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "B8")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "D6")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D7")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C7")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C6")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H7")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "B4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "D4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G6")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G7")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1R_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1R_C-E_Tx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1R_C-E_Tx_0_1")
		(symbol "STM32G0C1R_C-E_Tx_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PD8")
				(number "40")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PD9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC0")
				(number "13")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC1")
				(number "14")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "43")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "37")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "44")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "42")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1R_C-E_TxN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1R_C-E_TxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1R_C-E_TxN_0_1")
		(symbol "STM32G0C1R_C-E_TxN_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "7")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "PF0")
				(number "10")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "PF1")
				(number "11")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "PF2")
				(number "12")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "PD0")
				(number "50")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "PD1")
				(number "51")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "52")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PD3")
				(number "53")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PD4")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PD5")
				(number "55")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PD6")
				(number "56")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC0")
				(number "13")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC1")
				(number "14")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PC2")
				(number "15")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PC3")
				(number "16")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PC4")
				(number "25")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PC5")
				(number "26")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "PC8")
				(number "48")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "PC9")
				(number "49")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "PC10")
				(number "64")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "PC11")
				(number "1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "PC12")
				(number "2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "PC13")
				(number "3")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "21")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "36")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PA9/PA11")
				(number "43")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PA9/UCPD1_DBCC1")
				(number "37")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA10/PA12")
				(number "44")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA10/UCPD1_DBCC2")
				(number "42")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "45")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "46")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "47")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "57")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "62")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "63")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "31")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "32")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "33")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "35")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1V_C-E_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0C1V_C-E_Ix"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1V_C-E_Ix_0_1")
		(symbol "STM32G0C1V_C-E_Ix_1_1"
			(pin input line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "F2")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PF0")
				(number "H1")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PF1")
				(number "J1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PF2")
				(number "G2")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PF3")
				(number "H3")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PF4")
				(number "H2")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PF5")
				(number "J2")
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PF6")
				(number "M6")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PF7")
				(number "L7")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PF8")
				(number "D10")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PF9")
				(number "A8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PF10")
				(number "B7")
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PF11")
				(number "A7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PF12")
				(number "B6")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PF13")
				(number "A6")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "B4")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "A3")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "C2")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE6")
				(number "C1")
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE8")
				(number "M8")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PE9")
				(number "K8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PE14")
				(number "K9")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PE15")
				(number "L10")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD0")
				(number "B10")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD1")
				(number "C9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD2")
				(number "A11")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD4")
				(number "B9")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD5")
				(number "A10")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD6")
				(number "A9")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD7")
				(number "B8")
				(alternate "RCC_MCO_2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD8")
				(number "J12")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PD9")
				(number "H11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PD10")
				(number "H12")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PD11")
				(number "G11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PD12")
				(number "F11")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PD13")
				(number "E12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PD14")
				(number "E11")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PD15")
				(number "D11")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F1")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "G1")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F12")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "K3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "L2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "M1")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "K4")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "M2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "M3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "L12")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA9/PA11")
				(number "D12")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9/UCPD1_DBCC1")
				(number "H10")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10/PA12")
				(number "C12")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA10/UCPD1_DBCC2")
				(number "E10")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "C11")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "B12")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "L5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M5")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB8")
				(number "A1")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "C3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "M11")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K10")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "M12")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "J10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "K1")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J3")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "K2")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "L1")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "L4")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "M4")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "J11")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "K12")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "C10")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "A12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "B1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "D2")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G0C1V_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0C1V_C-E_Tx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256-512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G0C1V_C-E_Tx_0_1")
		(symbol "STM32G0C1V_C-E_Tx_1_1"
			(pin input line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "12")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PF0")
				(number "15")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PF1")
				(number "16")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PF2")
				(number "17")
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PF3")
				(number "18")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PF4")
				(number "19")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PF5")
				(number "20")
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PF6")
				(number "38")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PF7")
				(number "39")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PF8")
				(number "72")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PF9")
				(number "86")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PF10")
				(number "87")
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PF11")
				(number "88")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PF12")
				(number "89")
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PF13")
				(number "90")
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE0")
				(number "94")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE1")
				(number "95")
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE2")
				(number "96")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE3")
				(number "97")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE4")
				(number "4")
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE5")
				(number "5")
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE6")
				(number "6")
				(alternate "RTC_TAMP_IN3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE7")
				(number "40")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE8")
				(number "41")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PE9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PE10")
				(number "43")
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PE11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PE12")
				(number "45")
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PE13")
				(number "46")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PE14")
				(number "47")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PE15")
				(number "48")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD0")
				(number "78")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UCPD2_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD1")
				(number "79")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UCPD2_DBCC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD2")
				(number "80")
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UCPD2_CC2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD3")
				(number "81")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD2_DBCC2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD4")
				(number "82")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD5")
				(number "83")
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD6")
				(number "84")
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD7")
				(number "85")
				(alternate "RCC_MCO_2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD8")
				(number "59")
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PD9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PD10")
				(number "61")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PD11")
				(number "62")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PD12")
				(number "65")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PD13")
				(number "66")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PD14")
				(number "67")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PD15")
				(number "68")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "25")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RTC_TAMP_IN2" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "26")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "27")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "28")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "55")
				(alternate "CRS1_SYNC" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA9/PA11")
				(number "70")
				(alternate "ADC1_EXTI11 (PA11)" bidirectional line)
				(alternate "COMP1_OUT (PA11)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "FDCAN1_RX (PA11)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA11)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S1_MCK (PA11)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA11" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI1_MISO (PA11)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_BK2 (PA11)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH4 (PA11)" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "USART1_CTS (PA11)" bidirectional line)
				(alternate "USART1_NSS (PA11)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
				(alternate "USB_DM (PA11)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9/UCPD1_DBCC1")
				(number "56")
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2S2_MCK (PA9)" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "SPI2_MISO (PA9)" bidirectional line)
				(alternate "TIM15_BK (PA9)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "UCPD1_DBCC1 (PA9)" bidirectional line)
				(alternate "UCPD1_DBCC1 (UCPD1_DBCC1)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10/PA12")
				(number "71")
				(alternate "COMP2_OUT (PA12)" bidirectional line)
				(alternate "FDCAN1_TX (PA12)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA12)" bidirectional line)
				(alternate "I2S1_SD (PA12)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "I2S_CKIN (PA12)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA12" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI1_MOSI (PA12)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TIM1_ETR (PA12)" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA12)" bidirectional line)
				(alternate "USART1_DE (PA12)" bidirectional line)
				(alternate "USART1_RTS (PA12)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USB_DP (PA12)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA10/UCPD1_DBCC2")
				(number "69")
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "I2S2_SD (PA10)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "RCC_MCO_2 (PA10)" bidirectional line)
				(alternate "SPI2_MOSI (PA10)" bidirectional line)
				(alternate "TIM17_BK (PA10)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "UCPD1_DBCC2 (PA10)" bidirectional line)
				(alternate "UCPD1_DBCC2 (UCPD1_DBCC2)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "73")
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "74")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "75")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "91")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "93")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SYS_WKUP6" bidirectional line)
				(alternate "TIM16_BK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "98")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART5_CTS" bidirectional line)
				(alternate "USART5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "99")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
				(alternate "USART4_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB8")
				(number "100")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "49")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "21")
				(alternate "COMP3_INM" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "22")
				(alternate "COMP3_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "23")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "24")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "57")
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "58")
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "76")
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "UCPD2_FRSTX1" bidirectional line)
				(alternate "UCPD2_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "77")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "2")
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "7")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP_IN1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIM1_BK2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "TIM15_BK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G030C6Tx"
		(extends "STM32G030C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G030C6Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 43 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G030C8Tx"
		(extends "STM32G030C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G030C8Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 43 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G030K6Tx"
		(extends "STM32G030K_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G030K6Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G030K8Tx"
		(extends "STM32G030K_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G030K8Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x0 Value line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031C4Tx"
		(extends "STM32G031C_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G031C4Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031C4Ux"
		(extends "STM32G031C_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G031C4Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031C6Tx"
		(extends "STM32G031C_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G031C6Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031C6Ux"
		(extends "STM32G031C_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G031C6Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031C8Tx"
		(extends "STM32G031C_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G031C8Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031C8Ux"
		(extends "STM32G031C_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G031C8Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031F4Px"
		(extends "STM32G031F_4-6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G031F4Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031F6Px"
		(extends "STM32G031F_4-6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G031F6Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031F8Px"
		(extends "STM32G031F_4-6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G031F8Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031G4Ux"
		(extends "STM32G031G_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G031G4Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031G6Ux"
		(extends "STM32G031G_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G031G6Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031G8Ux"
		(extends "STM32G031G_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G031G8Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031J4Mx"
		(extends "STM32G031J_4-6_Mx")
		(property "Reference" "U"
			(at -27.94 11.43 0)
		)
		(property "Value" "STM32G031J4Mx"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -27.94 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031j4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 6 GPIO, SO8N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031J6Mx"
		(extends "STM32G031J_4-6_Mx")
		(property "Reference" "U"
			(at -27.94 11.43 0)
		)
		(property "Value" "STM32G031J6Mx"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -27.94 -10.16 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031j6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 6 GPIO, SO8N"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031K4Tx"
		(extends "STM32G031K_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G031K4Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031K4Ux"
		(extends "STM32G031K_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G031K4Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031K6Tx"
		(extends "STM32G031K_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G031K6Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031K6Ux"
		(extends "STM32G031K_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G031K6Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031K8Tx"
		(extends "STM32G031K_4-6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G031K8Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G031K8Ux"
		(extends "STM32G031K_4-6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G031K8Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g031k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041C6Tx"
		(extends "STM32G041C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G041C6Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041C6Ux"
		(extends "STM32G041C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G041C6Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041C8Tx"
		(extends "STM32G041C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G041C8Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041C8Ux"
		(extends "STM32G041C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G041C8Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041F6Px"
		(extends "STM32G041F_6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G041F6Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041F8Px"
		(extends "STM32G041F_6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G041F8Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041G6Ux"
		(extends "STM32G041G_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G041G6Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041G8Ux"
		(extends "STM32G041G_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G041G8Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041K6Tx"
		(extends "STM32G041K_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G041K6Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041K6Ux"
		(extends "STM32G041K_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G041K6Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041K8Tx"
		(extends "STM32G041K_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G041K8Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G041K8Ux"
		(extends "STM32G041K_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G041K8Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g041k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051C6Tx"
		(extends "STM32G051C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G051C6Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051C6Ux"
		(extends "STM32G051C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G051C6Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051C8Tx"
		(extends "STM32G051C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G051C8Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051C8Ux"
		(extends "STM32G051C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G051C8Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051F6Px"
		(extends "STM32G051F_6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G051F6Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051F8Px"
		(extends "STM32G051F_6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G051F8Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051G6Ux"
		(extends "STM32G051G_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G051G6Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051G8Ux"
		(extends "STM32G051G_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G051G8Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051K6Tx"
		(extends "STM32G051K_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G051K6Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051K6Ux"
		(extends "STM32G051K_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G051K6Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051K8Tx"
		(extends "STM32G051K_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G051K8Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G051K8Ux"
		(extends "STM32G051K_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G051K8Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g051k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061C6Tx"
		(extends "STM32G061C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G061C6Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061C6Ux"
		(extends "STM32G061C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G061C6Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061C8Tx"
		(extends "STM32G061C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G061C8Tx"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061C8Ux"
		(extends "STM32G061C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G061C8Ux"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061F6Px"
		(extends "STM32G061F_6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G061F6Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061F8Px"
		(extends "STM32G061F_6-8_Px")
		(property "Reference" "U"
			(at -22.86 21.59 0)
		)
		(property "Value" "STM32G061F8Px"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -22.86 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 18 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061G6Ux"
		(extends "STM32G061G_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G061G6Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061G8Ux"
		(extends "STM32G061G_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "STM32G061G8Ux"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061K6Tx"
		(extends "STM32G061K_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G061K6Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061K6Ux"
		(extends "STM32G061K_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G061K6Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061K8Tx"
		(extends "STM32G061K_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G061K8Tx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G061K8Ux"
		(extends "STM32G061K_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G061K8Ux"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g061k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 18KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G071G8UxN"
		(extends "STM32G071G_8-B_UxN")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G071G8UxN"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G071GBUxN"
		(extends "STM32G071G_8-B_UxN")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "STM32G071GBUxN"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -15.24 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071gb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 26 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G071K8TxN"
		(extends "STM32G071K_8-B_TxN")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "STM32G071K8TxN"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G071K8UxN"
		(extends "STM32G071K_8-B_UxN")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "STM32G071K8UxN"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G071KBTxN"
		(extends "STM32G071K_8-B_TxN")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "STM32G071KBTxN"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G071KBUxN"
		(extends "STM32G071K_8-B_UxN")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "STM32G071KBUxN"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 36KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CBTx"
		(extends "STM32G0B1C_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1CBTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CBTxN"
		(extends "STM32G0B1C_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0B1CBTxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CBUx"
		(extends "STM32G0B1C_B-C-E_Ux")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1CBUx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CBUxN"
		(extends "STM32G0B1C_B-C-E_UxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0B1CBUxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CCTx"
		(extends "STM32G0B1C_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1CCTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CCTxN"
		(extends "STM32G0B1C_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0B1CCTxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CCUx"
		(extends "STM32G0B1C_B-C-E_Ux")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1CCUx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CCUxN"
		(extends "STM32G0B1C_B-C-E_UxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0B1CCUxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CETx"
		(extends "STM32G0B1C_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1CETx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CETxN"
		(extends "STM32G0B1C_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0B1CETxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CEUx"
		(extends "STM32G0B1C_B-C-E_Ux")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1CEUx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1CEUxN"
		(extends "STM32G0B1C_B-C-E_UxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0B1CEUxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KBTx"
		(extends "STM32G0B1K_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0B1KBTx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KBTxN"
		(extends "STM32G0B1K_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0B1KBTxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KBUx"
		(extends "STM32G0B1K_B-C-E_Ux")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0B1KBUx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KBUxN"
		(extends "STM32G0B1K_B-C-E_UxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0B1KBUxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KCTx"
		(extends "STM32G0B1K_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0B1KCTx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KCTxN"
		(extends "STM32G0B1K_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0B1KCTxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KCUx"
		(extends "STM32G0B1K_B-C-E_Ux")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0B1KCUx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KCUxN"
		(extends "STM32G0B1K_B-C-E_UxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0B1KCUxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KETx"
		(extends "STM32G0B1K_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0B1KETx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KETxN"
		(extends "STM32G0B1K_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0B1KETxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KEUx"
		(extends "STM32G0B1K_B-C-E_Ux")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0B1KEUx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1KEUxN"
		(extends "STM32G0B1K_B-C-E_UxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0B1KEUxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1MBTx"
		(extends "STM32G0B1M_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 64.77 0)
		)
		(property "Value" "STM32G0B1MBTx"
			(at 5.08 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -25.4 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 74 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1MCTx"
		(extends "STM32G0B1M_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 64.77 0)
		)
		(property "Value" "STM32G0B1MCTx"
			(at 5.08 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -25.4 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 74 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1METx"
		(extends "STM32G0B1M_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 64.77 0)
		)
		(property "Value" "STM32G0B1METx"
			(at 5.08 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -25.4 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 74 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1RBIxN"
		(extends "STM32G0B1R_B-C-E_IxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1RBIxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1RBTx"
		(extends "STM32G0B1R_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1RBTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1RBTxN"
		(extends "STM32G0B1R_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1RBTxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1RCIxN"
		(extends "STM32G0B1R_B-C-E_IxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1RCIxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1RCTx"
		(extends "STM32G0B1R_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1RCTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1RCTxN"
		(extends "STM32G0B1R_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1RCTxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1REIxN"
		(extends "STM32G0B1R_B-C-E_IxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1REIxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1RETx"
		(extends "STM32G0B1R_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1RETx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1RETxN"
		(extends "STM32G0B1R_B-C-E_TxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0B1RETxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1VBIx"
		(extends "STM32G0B1V_B-C-E_Ix")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0B1VBIx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1VBTx"
		(extends "STM32G0B1V_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0B1VBTx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1VCIx"
		(extends "STM32G0B1V_B-C-E_Ix")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0B1VCIx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1VCTx"
		(extends "STM32G0B1V_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0B1VCTx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1VEIx"
		(extends "STM32G0B1V_B-C-E_Ix")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0B1VEIx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0B1VETx"
		(extends "STM32G0B1V_B-C-E_Tx")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0B1VETx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0b1ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1CCTx"
		(extends "STM32G0C1C_C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1CCTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1CCTxN"
		(extends "STM32G0C1C_C-E_TxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0C1CCTxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1CCUx"
		(extends "STM32G0C1C_C-E_Ux")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1CCUx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1CCUxN"
		(extends "STM32G0C1C_C-E_UxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0C1CCUxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1CETx"
		(extends "STM32G0C1C_C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1CETx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1CETxN"
		(extends "STM32G0C1C_C-E_TxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0C1CETxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1CEUx"
		(extends "STM32G0C1C_C-E_Ux")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1CEUx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 44 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1CEUxN"
		(extends "STM32G0C1C_C-E_UxN")
		(property "Reference" "U"
			(at -25.4 44.45 0)
		)
		(property "Value" "STM32G0C1CEUxN"
			(at 5.08 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -25.4 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1KCTx"
		(extends "STM32G0C1K_C-E_Tx")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0C1KCTx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1KCTxN"
		(extends "STM32G0C1K_C-E_TxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0C1KCTxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1KCUx"
		(extends "STM32G0C1K_C-E_Ux")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0C1KCUx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1KCUxN"
		(extends "STM32G0C1K_C-E_UxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0C1KCUxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1KETx"
		(extends "STM32G0C1K_C-E_Tx")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0C1KETx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1KETxN"
		(extends "STM32G0C1K_C-E_TxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0C1KETxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1KEUx"
		(extends "STM32G0C1K_C-E_Ux")
		(property "Reference" "U"
			(at -22.86 26.67 0)
		)
		(property "Value" "STM32G0C1KEUx"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -22.86 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 30 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1KEUxN"
		(extends "STM32G0C1K_C-E_UxN")
		(property "Reference" "U"
			(at -25.4 26.67 0)
		)
		(property "Value" "STM32G0C1KEUxN"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 29 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1MCTx"
		(extends "STM32G0C1M_C-E_Tx")
		(property "Reference" "U"
			(at -25.4 64.77 0)
		)
		(property "Value" "STM32G0C1MCTx"
			(at 5.08 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -25.4 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 74 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1METx"
		(extends "STM32G0C1M_C-E_Tx")
		(property "Reference" "U"
			(at -25.4 64.77 0)
		)
		(property "Value" "STM32G0C1METx"
			(at 5.08 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -25.4 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 74 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1RCIxN"
		(extends "STM32G0C1R_C-E_IxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1RCIxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1RCTx"
		(extends "STM32G0C1R_C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1RCTx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1RCTxN"
		(extends "STM32G0C1R_C-E_TxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1RCTxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1REIxN"
		(extends "STM32G0C1R_C-E_IxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1REIxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1RETx"
		(extends "STM32G0C1R_C-E_Tx")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1RETx"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 60 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1RETxN"
		(extends "STM32G0C1R_C-E_TxN")
		(property "Reference" "U"
			(at -25.4 46.99 0)
		)
		(property "Value" "STM32G0C1RETxN"
			(at 5.08 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -25.4 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 58 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1VCIx"
		(extends "STM32G0C1V_C-E_Ix")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0C1VCIx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1VCTx"
		(extends "STM32G0C1V_C-E_Tx")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0C1VCTx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1VEIx"
		(extends "STM32G0C1V_C-E_Ix")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0C1VEIx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G0C1VETx"
		(extends "STM32G0C1V_C-E_Tx")
		(property "Reference" "U"
			(at -25.4 69.85 0)
		)
		(property "Value" "STM32G0C1VETx"
			(at 5.08 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g0c1ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 512KB flash, 144KB RAM, 64 MHz, 1.7-3.6V, 94 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32G0 STM32G0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
