(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32G431CBTxZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G431CBTxZ"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431CBTxZ_0_1")
		(symbol "STM32G431CBTxZ_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431CBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "STM32G431CBYx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_3.15x3.13mm_Layout7x7_P0.4mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 41 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.15x3.13mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431CBYx_0_1")
		(symbol "STM32G431CBYx_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "F3")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "C6")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "E7")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "E6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "D4")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "D1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC11")
				(number "A2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "C5")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "C7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "D7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "G5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "E4")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "F4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "A5")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "F2")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "E3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "F1")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "E2")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "D3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "B7")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "A6")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "G3")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "F7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "D6")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "F6")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "E5")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "G6")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "D5")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "D2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "C3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "B3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA15")
				(number "A1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431C_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G431C_6-8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431C_6-8-B_Tx_0_1")
		(symbol "STM32G431C_6-8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431C_6-8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G431C_6-8-B_Ux"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431C_6-8-B_Ux_0_1")
		(symbol "STM32G431C_6-8-B_Ux_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "16")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "29")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC11")
				(number "40")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "42")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "43")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "44")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "45")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "47")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "24")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431K_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G431K_6-8-B_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431K_6-8-B_Tx_0_1")
		(symbol "STM32G431K_6-8-B_Tx_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PG10")
				(number "4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "13")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB8")
				(number "31")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "9")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "10")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "11")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "12")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431K_6-8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G431K_6-8-B_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431K_6-8-B_Ux_0_1")
		(symbol "STM32G431K_6-8-B_Ux_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PG10")
				(number "4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "13")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB8")
				(number "31")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "9")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "10")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "11")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "12")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431M_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G431M_6-8-B_Tx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431m6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431M_6-8-B_Tx_0_1")
		(symbol "STM32G431M_6-8-B_Tx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431RBTxZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431RBTxZ"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431RBTxZ_0_1")
		(symbol "STM32G431RBTxZ_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431R_6-8-B_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431R_6-8-B_Ix"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431R_6-8-B_Ix_0_1")
		(symbol "STM32G431R_6-8-B_Ix_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "G5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "D2")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "E1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "F1")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "D5")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "F4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "F6")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "C5")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "A6")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "B1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "D4")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E4")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G3")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "E5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F5")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H6")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G6")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431R_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431R_6-8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431R_6-8-B_Tx_0_1")
		(symbol "STM32G431R_6-8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431V_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G431V_6-8-B_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431v6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32-128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G431V_6-8-B_Tx_0_1")
		(symbol "STM32G431V_6-8-B_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "36")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "14")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "82")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "83")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "84")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "85")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "86")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "87")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "88")
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "89")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "35")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "26")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "27")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "28")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "29")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "69")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "71")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "72")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "73")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "76")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "77")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "90")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "91")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "92")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "93")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "94")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "30")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "31")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "65")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "66")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "79")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "81")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441CBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G441CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441CBTx_0_1")
		(symbol "STM32G441CBTx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G441CBUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441CBUx_0_1")
		(symbol "STM32G441CBUx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "16")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "29")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC11")
				(number "40")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "42")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "43")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "44")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "45")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "47")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "24")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441CBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "STM32G441CBYx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_3.15x3.13mm_Layout7x7_P0.4mm"
			(at -12.7 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 41 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.15x3.13mm*Layout7x7*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441CBYx_0_1")
		(symbol "STM32G441CBYx_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "F3")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "C6")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "E7")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "E6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "D4")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "D1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC11")
				(number "A2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC13")
				(number "C5")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "C7")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "D7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "G5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "E4")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "F4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "C4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "A5")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB10")
				(number "F2")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB11")
				(number "E3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB12")
				(number "F1")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB13")
				(number "E2")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB14")
				(number "D3")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "B7")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "A6")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "G3")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "F7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "D6")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "F6")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "E5")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "F5")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "G6")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "D5")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "D2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "C3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "B3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA15")
				(number "A1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441KBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G441KBTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441KBTx_0_1")
		(symbol "STM32G441KBTx_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PG10")
				(number "4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "13")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB8")
				(number "31")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "9")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "10")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "11")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "12")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441KBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G441KBUx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441KBUx_0_1")
		(symbol "STM32G441KBUx_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PG10")
				(number "4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "13")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB8")
				(number "31")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "9")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "10")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "11")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "12")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441MBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G441MBTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441MBTx_0_1")
		(symbol "STM32G441MBTx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441RBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G441RBIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441RBIx_0_1")
		(symbol "STM32G441RBIx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "G5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "D2")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "E1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "F1")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "D5")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "F4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "F6")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "C5")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "A6")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "B1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "D4")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E4")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G3")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "E5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F5")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H6")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G6")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G441RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441RBTx_0_1")
		(symbol "STM32G441RBTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G441VBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G441VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g441vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G441VBTx_0_1")
		(symbol "STM32G441VBTx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "36")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "14")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "82")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "83")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "84")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "85")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "86")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "87")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "88")
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "89")
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "35")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "26")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "27")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "28")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "29")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "69")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "71")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "72")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "73")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "76")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "77")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "90")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "91")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "92")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "93")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "94")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "30")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "31")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "65")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "66")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "79")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "81")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473C_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G473C_B-C-E_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473C_B-C-E_Tx_0_1")
		(symbol "STM32G473C_B-C-E_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473C_B-C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G473C_B-C-E_Ux"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473C_B-C-E_Ux_0_1")
		(symbol "STM32G473C_B-C-E_Ux_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "16")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "29")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC11")
				(number "40")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "41")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "42")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "43")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "44")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "45")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "47")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "24")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473MEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G473MEYx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-81_4.02x4.27mm_Layout9x9_P0.4mm"
			(at -17.78 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 67 GPIO, WLCSP81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.02x4.27mm*Layout9x9*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473MEYx_0_1")
		(symbol "STM32G473MEYx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "J6")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "D8")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "E9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "F9")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "H5")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "G5")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "F5")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "J4")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "H4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "E5")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "G4")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "J3")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "F4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "B4")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "A4")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "G1")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "F3")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "F2")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD11")
				(number "E2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C8")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "G9")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "E6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "H7")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "E3")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "D5")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "C5")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "D2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "C4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "B8")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "C9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "A8")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "J1")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "H6")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "D7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "E7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "G8")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "H8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "D6")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "F7")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "G7")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "J8")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "D4")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "C1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "J7")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "C6")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "B6")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "C7")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "B7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "H3")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "H2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "G3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "H1")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "G2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "E4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473M_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G473M_B-C-E_Tx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473M_B-C-E_Tx_0_1")
		(symbol "STM32G473M_B-C-E_Tx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473P_B-C-E_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G473P_B-C-E_Ix"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473pb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473P_B-C-E_Ix_0_1")
		(symbol "STM32G473P_B-C-E_Ix_1_1"
			(pin input line
				(at -25.4 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L4")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 68.58 0)
				(length 5.08)
				(name "PG0")
				(number "F9")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 66.04 0)
				(length 5.08)
				(name "PG1")
				(number "F8")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "PG2")
				(number "F7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "PG3")
				(number "E11")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "PG4")
				(number "E10")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "PG10")
				(number "F5")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PF1")
				(number "F2")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF4")
				(number "D4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF5")
				(number "E3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF6")
				(number "A11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PF7")
				(number "E4")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PF8")
				(number "E5")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PF9")
				(number "F3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PF10")
				(number "F4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PF11")
				(number "J5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PF12")
				(number "H5")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PF13")
				(number "J6")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PF14")
				(number "H6")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PF15")
				(number "G6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE0")
				(number "B4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE1")
				(number "C4")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PE4")
				(number "A1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PE5")
				(number "B1")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PE6")
				(number "C3")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PE7")
				(number "L7")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PE8")
				(number "K7")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PE9")
				(number "J7")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PE10")
				(number "H7")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PE11")
				(number "L8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PE13")
				(number "J8")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PE14")
				(number "K9")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PE15")
				(number "L9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD0")
				(number "B9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD2")
				(number "C7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD3")
				(number "B7")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "PD4")
				(number "A7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "PD5")
				(number "E6")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "PD6")
				(number "D6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "PD8")
				(number "H9")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "PD9")
				(number "H10")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "PD10")
				(number "H11")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -63.5 0)
				(length 5.08)
				(name "PD11")
				(number "G7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -66.04 0)
				(length 5.08)
				(name "PD12")
				(number "G8")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -68.58 0)
				(length 5.08)
				(name "PD13")
				(number "G9")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -71.12 0)
				(length 5.08)
				(name "PD14")
				(number "G10")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -73.66 0)
				(length 5.08)
				(name "PD15")
				(number "F6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 83.82 270)
				(length 5.08)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at 0 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -83.82 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C10")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 2.54 -83.82 90)
				(length 5.08)
				(name "VSSA")
				(number "K5")
			)
			(pin power_in line
				(at 5.08 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "K11")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "L6")
			)
			(pin power_in line
				(at 12.7 83.82 270)
				(length 5.08)
				(name "VDDA")
				(number "L5")
			)
			(pin bidirectional line
				(at 25.4 73.66 180)
				(length 5.08)
				(name "PA0")
				(number "G4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 71.12 180)
				(length 5.08)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 68.58 180)
				(length 5.08)
				(name "PA2")
				(number "J3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 66.04 180)
				(length 5.08)
				(name "PA3")
				(number "K1")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA4")
				(number "L1")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA5")
				(number "K2")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA8")
				(number "E7")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA9")
				(number "D8")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA10")
				(number "D9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA11")
				(number "D11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA12")
				(number "D10")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA13")
				(number "B11")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA14")
				(number "B10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA15")
				(number "A10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PB0")
				(number "J4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "PB3")
				(number "A6")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB4")
				(number "C6")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB5")
				(number "B5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB8")
				(number "D5")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB12")
				(number "J9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB13")
				(number "J11")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB14")
				(number "J10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB15")
				(number "H8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PC0")
				(number "G2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PC1")
				(number "G1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PC2")
				(number "G3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PC3")
				(number "H1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC4")
				(number "L3")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC5")
				(number "H4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC8")
				(number "E9")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC9")
				(number "E8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC10")
				(number "C9")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC12")
				(number "D7")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC15")
				(number "D2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473QETxZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G473QETxZ"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473QETxZ_0_1")
		(symbol "STM32G473QETxZ_1_1"
			(pin input line
				(at -27.94 81.28 0)
				(length 5.08)
				(name "VREF+")
				(number "43")
				(alternate "VREFBUF_OUT1" bidirectional line)
			)
			(pin input line
				(at -27.94 78.74 0)
				(length 5.08)
				(name "VREF_+")
				(number "44")
				(alternate "VREFBUF_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 5.08)
				(name "PG0")
				(number "82")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 5.08)
				(name "PG1")
				(number "83")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 5.08)
				(name "PG2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "PG3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "PG4")
				(number "86")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "PG5")
				(number "103")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "PG6")
				(number "104")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "PG7")
				(number "105")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "PG8")
				(number "106")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PG9")
				(number "107")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PG10")
				(number "21")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PF0")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PF1")
				(number "20")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PF2")
				(number "26")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PF3")
				(number "10")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PF5")
				(number "14")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PF6")
				(number "97")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PF7")
				(number "15")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PF8")
				(number "16")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PF9")
				(number "17")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PF10")
				(number "18")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PF11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PF12")
				(number "49")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PE0")
				(number "125")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PE1")
				(number "126")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PE7")
				(number "53")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PE8")
				(number "54")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PE9")
				(number "55")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PE10")
				(number "56")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PE11")
				(number "57")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PE12")
				(number "58")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PE13")
				(number "59")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PE14")
				(number "60")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PE15")
				(number "61")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PD0")
				(number "108")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PD1")
				(number "109")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PD2")
				(number "112")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "PD3")
				(number "113")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 5.08)
				(name "PD4")
				(number "114")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "PD5")
				(number "115")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "PD6")
				(number "116")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 5.08)
				(name "PD7")
				(number "117")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -63.5 0)
				(length 5.08)
				(name "PD8")
				(number "70")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -66.04 0)
				(length 5.08)
				(name "PD9")
				(number "71")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -68.58 0)
				(length 5.08)
				(name "PD10")
				(number "72")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -71.12 0)
				(length 5.08)
				(name "PD11")
				(number "73")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 5.08)
				(name "PD12")
				(number "74")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -76.2 0)
				(length 5.08)
				(name "PD13")
				(number "75")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -78.74 0)
				(length 5.08)
				(name "PD14")
				(number "76")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -81.28 0)
				(length 5.08)
				(name "PD15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "47")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "110")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "127")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "46")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "78")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "79")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "42")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "111")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "128")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "27")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "28")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "29")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "32")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "33")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "34")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "35")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "36")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "89")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "90")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "91")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "92")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "93")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA13")
				(number "96")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA14")
				(number "98")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA15")
				(number "99")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "39")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "40")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "41")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PB3")
				(number "118")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PB4")
				(number "119")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "120")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "121")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "122")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "123")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "124")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "62")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "65")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB12")
				(number "66")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB13")
				(number "67")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB14")
				(number "68")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB15")
				(number "69")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PC0")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PC1")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PC2")
				(number "24")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PC3")
				(number "25")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PC4")
				(number "37")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PC5")
				(number "38")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PC6")
				(number "80")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC7")
				(number "81")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC8")
				(number "87")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC9")
				(number "88")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC10")
				(number "100")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC11")
				(number "101")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC12")
				(number "102")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473Q_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G473Q_B-C-E_Tx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473qb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473Q_B-C-E_Tx_0_1")
		(symbol "STM32G473Q_B-C-E_Tx_1_1"
			(pin input line
				(at -27.94 81.28 0)
				(length 5.08)
				(name "VREF+")
				(number "43")
				(alternate "VREFBUF_OUT1" bidirectional line)
			)
			(pin input line
				(at -27.94 78.74 0)
				(length 5.08)
				(name "VREF_+")
				(number "44")
				(alternate "VREFBUF_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 5.08)
				(name "PG0")
				(number "82")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 5.08)
				(name "PG1")
				(number "83")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 5.08)
				(name "PG2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "PG3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "PG4")
				(number "86")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "PG5")
				(number "103")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "PG6")
				(number "104")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "PG7")
				(number "105")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "PG8")
				(number "106")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PG9")
				(number "107")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PG10")
				(number "21")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PF0")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PF1")
				(number "20")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PF2")
				(number "26")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PF3")
				(number "10")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PF5")
				(number "14")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PF6")
				(number "97")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PF7")
				(number "15")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PF8")
				(number "16")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PF9")
				(number "17")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PF10")
				(number "18")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PF11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PF12")
				(number "49")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PE0")
				(number "125")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PE1")
				(number "126")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PE7")
				(number "53")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PE8")
				(number "54")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PE9")
				(number "55")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PE10")
				(number "56")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PE11")
				(number "57")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PE12")
				(number "58")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PE13")
				(number "59")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PE14")
				(number "60")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PE15")
				(number "61")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PD0")
				(number "108")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PD1")
				(number "109")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PD2")
				(number "112")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "PD3")
				(number "113")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 5.08)
				(name "PD4")
				(number "114")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "PD5")
				(number "115")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "PD6")
				(number "116")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 5.08)
				(name "PD7")
				(number "117")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -63.5 0)
				(length 5.08)
				(name "PD8")
				(number "70")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -66.04 0)
				(length 5.08)
				(name "PD9")
				(number "71")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -68.58 0)
				(length 5.08)
				(name "PD10")
				(number "72")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -71.12 0)
				(length 5.08)
				(name "PD11")
				(number "73")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 5.08)
				(name "PD12")
				(number "74")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -76.2 0)
				(length 5.08)
				(name "PD13")
				(number "75")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -78.74 0)
				(length 5.08)
				(name "PD14")
				(number "76")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -81.28 0)
				(length 5.08)
				(name "PD15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "47")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "110")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "127")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "46")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "78")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "79")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "42")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "111")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "128")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "27")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "28")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "29")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "32")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "33")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "34")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "35")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "36")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "89")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "90")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "91")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "92")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "93")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA13")
				(number "96")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA14")
				(number "98")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA15")
				(number "99")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "39")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "40")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "41")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PB3")
				(number "118")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PB4")
				(number "119")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "120")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "121")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "122")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "123")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "124")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "62")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "65")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB12")
				(number "66")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB13")
				(number "67")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB14")
				(number "68")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB15")
				(number "69")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PC0")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PC1")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PC2")
				(number "24")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PC3")
				(number "25")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PC4")
				(number "37")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PC5")
				(number "38")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PC6")
				(number "80")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC7")
				(number "81")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC8")
				(number "87")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC9")
				(number "88")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC10")
				(number "100")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC11")
				(number "101")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC12")
				(number "102")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473RETxZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G473RETxZ"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473RETxZ_0_1")
		(symbol "STM32G473RETxZ_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473R_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G473R_B-C-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473R_B-C-E_Tx_0_1")
		(symbol "STM32G473R_B-C-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473V_B-C-E_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G473V_B-C-E_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473V_B-C-E_Hx_0_1")
		(symbol "STM32G473V_B-C-E_Hx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "K5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "F3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "E1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "G3")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "E3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "E4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "B3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "C3")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "A1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "B1")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "G5")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "H5")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "H6")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "K6")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "G6")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "K7")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "J7")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE15")
				(number "H7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "B8")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "C6")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "A8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "A7")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "A6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K10")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "G8")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "G7")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "G9")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "F8")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D3")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D5")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D7")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K4")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "G2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "H1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "H2")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "J1")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "J2")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K1")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "D9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "C9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "D8")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "B10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "H4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "J4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "C5")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "B5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "A4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "J8")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J9")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "H9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "F4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "F1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K2")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E8")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "C8")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "A10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "D4")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G473V_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G473V_B-C-E_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G473V_B-C-E_Tx_0_1")
		(symbol "STM32G473V_B-C-E_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "36")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "14")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "82")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "83")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "86")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "87")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "88")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "89")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "35")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "26")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "27")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "28")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "29")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "69")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "70")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "71")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "72")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "73")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "76")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "77")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "90")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "91")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "92")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "93")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "94")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "30")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "31")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "65")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "66")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "67")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "79")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "81")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474C_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G474C_B-C-E_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474C_B-C-E_Tx_0_1")
		(symbol "STM32G474C_B-C-E_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474C_B-C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G474C_B-C-E_Ux"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474C_B-C-E_Ux_0_1")
		(symbol "STM32G474C_B-C-E_Ux_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "16")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "29")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC11")
				(number "40")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "41")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "42")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "43")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "44")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "45")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "47")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "24")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474MEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G474MEYx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-81_4.02x4.27mm_Layout9x9_P0.4mm"
			(at -17.78 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 67 GPIO, WLCSP81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.02x4.27mm*Layout9x9*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474MEYx_0_1")
		(symbol "STM32G474MEYx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "J6")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "D8")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "E9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "F9")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "H5")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "G5")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "F5")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "J4")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "H4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "E5")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "G4")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "J3")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "F4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "B4")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "A4")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "G1")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "F3")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "F2")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD11")
				(number "E2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C8")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "G9")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "E6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "H7")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "E3")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "D5")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "C5")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "D2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "C4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "A3")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "B8")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "C9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "A8")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "J1")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "H6")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "D7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "E7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "G8")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "H8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "D6")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "F7")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "G7")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "J8")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "D4")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "C1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "J7")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "C6")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "B6")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "C7")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "B7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "H3")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "H2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "G3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "H1")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "G2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "E4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474M_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G474M_B-C-E_Tx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474M_B-C-E_Tx_0_1")
		(symbol "STM32G474M_B-C-E_Tx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474P_B-C-E_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G474P_B-C-E_Ix"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474pb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474P_B-C-E_Ix_0_1")
		(symbol "STM32G474P_B-C-E_Ix_1_1"
			(pin input line
				(at -25.4 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L4")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 68.58 0)
				(length 5.08)
				(name "PG0")
				(number "F9")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 66.04 0)
				(length 5.08)
				(name "PG1")
				(number "F8")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "PG2")
				(number "F7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "PG3")
				(number "E11")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "PG4")
				(number "E10")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "PG10")
				(number "F5")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PF1")
				(number "F2")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF4")
				(number "D4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF5")
				(number "E3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF6")
				(number "A11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PF7")
				(number "E4")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PF8")
				(number "E5")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PF9")
				(number "F3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PF10")
				(number "F4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PF11")
				(number "J5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PF12")
				(number "H5")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PF13")
				(number "J6")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PF14")
				(number "H6")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PF15")
				(number "G6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE0")
				(number "B4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE1")
				(number "C4")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PE4")
				(number "A1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PE5")
				(number "B1")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PE6")
				(number "C3")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PE7")
				(number "L7")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PE8")
				(number "K7")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PE9")
				(number "J7")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PE10")
				(number "H7")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PE11")
				(number "L8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PE13")
				(number "J8")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PE14")
				(number "K9")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PE15")
				(number "L9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD0")
				(number "B9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD2")
				(number "C7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD3")
				(number "B7")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "PD4")
				(number "A7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "PD5")
				(number "E6")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "PD6")
				(number "D6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "PD8")
				(number "H9")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "PD9")
				(number "H10")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "PD10")
				(number "H11")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -63.5 0)
				(length 5.08)
				(name "PD11")
				(number "G7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -66.04 0)
				(length 5.08)
				(name "PD12")
				(number "G8")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -68.58 0)
				(length 5.08)
				(name "PD13")
				(number "G9")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -71.12 0)
				(length 5.08)
				(name "PD14")
				(number "G10")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -73.66 0)
				(length 5.08)
				(name "PD15")
				(number "F6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 83.82 270)
				(length 5.08)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at 0 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -83.82 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C10")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 2.54 -83.82 90)
				(length 5.08)
				(name "VSSA")
				(number "K5")
			)
			(pin power_in line
				(at 5.08 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "K11")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "L6")
			)
			(pin power_in line
				(at 12.7 83.82 270)
				(length 5.08)
				(name "VDDA")
				(number "L5")
			)
			(pin bidirectional line
				(at 25.4 73.66 180)
				(length 5.08)
				(name "PA0")
				(number "G4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 71.12 180)
				(length 5.08)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 68.58 180)
				(length 5.08)
				(name "PA2")
				(number "J3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 66.04 180)
				(length 5.08)
				(name "PA3")
				(number "K1")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA4")
				(number "L1")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA5")
				(number "K2")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA8")
				(number "E7")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA9")
				(number "D8")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA10")
				(number "D9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA11")
				(number "D11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA12")
				(number "D10")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA13")
				(number "B11")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA14")
				(number "B10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA15")
				(number "A10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PB0")
				(number "J4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "PB3")
				(number "A6")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB4")
				(number "C6")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB5")
				(number "B5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB8")
				(number "D5")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB12")
				(number "J9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB13")
				(number "J11")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB14")
				(number "J10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB15")
				(number "H8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PC0")
				(number "G2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PC1")
				(number "G1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PC2")
				(number "G3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PC3")
				(number "H1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC4")
				(number "L3")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC5")
				(number "H4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC8")
				(number "E9")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC9")
				(number "E8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC10")
				(number "C9")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC12")
				(number "D7")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC15")
				(number "D2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474Q_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G474Q_B-C-E_Tx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474qb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474Q_B-C-E_Tx_0_1")
		(symbol "STM32G474Q_B-C-E_Tx_1_1"
			(pin input line
				(at -27.94 81.28 0)
				(length 5.08)
				(name "VREF+")
				(number "43")
				(alternate "VREFBUF_OUT1" bidirectional line)
			)
			(pin input line
				(at -27.94 78.74 0)
				(length 5.08)
				(name "VREF_+")
				(number "44")
				(alternate "VREFBUF_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 5.08)
				(name "PG0")
				(number "82")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 5.08)
				(name "PG1")
				(number "83")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 5.08)
				(name "PG2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "PG3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "PG4")
				(number "86")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "PG5")
				(number "103")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "PG6")
				(number "104")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "PG7")
				(number "105")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "PG8")
				(number "106")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PG9")
				(number "107")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PG10")
				(number "21")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PF0")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PF1")
				(number "20")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PF2")
				(number "26")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PF3")
				(number "10")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PF5")
				(number "14")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PF6")
				(number "97")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PF7")
				(number "15")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PF8")
				(number "16")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PF9")
				(number "17")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PF10")
				(number "18")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PF11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PF12")
				(number "49")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PE0")
				(number "125")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PE1")
				(number "126")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PE7")
				(number "53")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PE8")
				(number "54")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PE9")
				(number "55")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PE10")
				(number "56")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PE11")
				(number "57")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PE12")
				(number "58")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PE13")
				(number "59")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PE14")
				(number "60")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PE15")
				(number "61")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PD0")
				(number "108")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PD1")
				(number "109")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PD2")
				(number "112")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "PD3")
				(number "113")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 5.08)
				(name "PD4")
				(number "114")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "PD5")
				(number "115")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "PD6")
				(number "116")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 5.08)
				(name "PD7")
				(number "117")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -63.5 0)
				(length 5.08)
				(name "PD8")
				(number "70")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -66.04 0)
				(length 5.08)
				(name "PD9")
				(number "71")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -68.58 0)
				(length 5.08)
				(name "PD10")
				(number "72")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -71.12 0)
				(length 5.08)
				(name "PD11")
				(number "73")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 5.08)
				(name "PD12")
				(number "74")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -76.2 0)
				(length 5.08)
				(name "PD13")
				(number "75")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -78.74 0)
				(length 5.08)
				(name "PD14")
				(number "76")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -81.28 0)
				(length 5.08)
				(name "PD15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "47")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "110")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "127")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "46")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "78")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "79")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "42")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "111")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "128")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "27")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "28")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "29")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "32")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "33")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "34")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "35")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "36")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "89")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "90")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "91")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "92")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "93")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA13")
				(number "96")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA14")
				(number "98")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA15")
				(number "99")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "39")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "40")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "41")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PB3")
				(number "118")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PB4")
				(number "119")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "120")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "121")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "122")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "123")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "124")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "62")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "65")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB12")
				(number "66")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB13")
				(number "67")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB14")
				(number "68")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB15")
				(number "69")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PC0")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PC1")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PC2")
				(number "24")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PC3")
				(number "25")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PC4")
				(number "37")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PC5")
				(number "38")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PC6")
				(number "80")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC7")
				(number "81")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC8")
				(number "87")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC9")
				(number "88")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC10")
				(number "100")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC11")
				(number "101")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC12")
				(number "102")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474R_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G474R_B-C-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474R_B-C-E_Tx_0_1")
		(symbol "STM32G474R_B-C-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474V_B-C-E_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G474V_B-C-E_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474V_B-C-E_Hx_0_1")
		(symbol "STM32G474V_B-C-E_Hx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "K5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "F3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "E1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "G3")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "E3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "E4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "B3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "C3")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "A1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "B1")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "G5")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "H5")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "H6")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "K6")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "G6")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "K7")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "J7")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE15")
				(number "H7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "B8")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "C6")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "A8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "A7")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "A6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K10")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "G8")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "G7")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "G9")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "F8")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D3")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D5")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D7")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K4")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "G2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "H1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "H2")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "J1")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "J2")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K1")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "D9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "C9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "D8")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "B10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "H4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "J4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "C5")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "B5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "A4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "J8")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J9")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "H9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "F4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "F1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K2")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E8")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "C8")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "A10")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "D4")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G474V_B-C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G474V_B-C-E_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128-512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G474V_B-C-E_Tx_0_1")
		(symbol "STM32G474V_B-C-E_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "36")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "14")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "82")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "83")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "86")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "87")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "88")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "89")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "35")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "26")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "27")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "28")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "29")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "69")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "70")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "71")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "72")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "73")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "76")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "77")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "90")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "91")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "92")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "93")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "94")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "30")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "31")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "65")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "66")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "67")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "79")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "81")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483CETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G483CETx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483CETx_0_1")
		(symbol "STM32G483CETx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G483CEUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483CEUx_0_1")
		(symbol "STM32G483CEUx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "16")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "29")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC11")
				(number "40")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "41")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "42")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "43")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "44")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "45")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "47")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "24")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483METx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G483METx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483METx_0_1")
		(symbol "STM32G483METx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483MEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G483MEYx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-81_4.02x4.27mm_Layout9x9_P0.4mm"
			(at -17.78 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 67 GPIO, WLCSP81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.02x4.27mm*Layout9x9*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483MEYx_0_1")
		(symbol "STM32G483MEYx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "J6")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "D8")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "E9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "F9")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "H5")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "G5")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "F5")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "J4")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "H4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "E5")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "G4")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "J3")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "F4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "B4")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "A4")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "G1")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "F3")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "F2")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD11")
				(number "E2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C8")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "G9")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "E6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "H7")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "E3")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "D5")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "C5")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "D2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "C4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "B8")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "C9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "A8")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "J1")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "H6")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "D7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "E7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "G8")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "H8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "D6")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "F7")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "G7")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "J8")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "D4")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "C1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "J7")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "C6")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "B6")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "C7")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "B7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "H3")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "H2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "G3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "H1")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "G2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "E4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483PEIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G483PEIx"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483pe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483PEIx_0_1")
		(symbol "STM32G483PEIx_1_1"
			(pin input line
				(at -25.4 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L4")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 68.58 0)
				(length 5.08)
				(name "PG0")
				(number "F9")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 66.04 0)
				(length 5.08)
				(name "PG1")
				(number "F8")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "PG2")
				(number "F7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "PG3")
				(number "E11")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "PG4")
				(number "E10")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "PG10")
				(number "F5")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PF1")
				(number "F2")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF4")
				(number "D4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF5")
				(number "E3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF6")
				(number "A11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PF7")
				(number "E4")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PF8")
				(number "E5")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PF9")
				(number "F3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PF10")
				(number "F4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PF11")
				(number "J5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PF12")
				(number "H5")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PF13")
				(number "J6")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PF14")
				(number "H6")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PF15")
				(number "G6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE0")
				(number "B4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE1")
				(number "C4")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PE4")
				(number "A1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PE5")
				(number "B1")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PE6")
				(number "C3")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PE7")
				(number "L7")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PE8")
				(number "K7")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PE9")
				(number "J7")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PE10")
				(number "H7")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PE11")
				(number "L8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PE13")
				(number "J8")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PE14")
				(number "K9")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PE15")
				(number "L9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD0")
				(number "B9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD2")
				(number "C7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD3")
				(number "B7")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "PD4")
				(number "A7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "PD5")
				(number "E6")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "PD6")
				(number "D6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "PD8")
				(number "H9")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "PD9")
				(number "H10")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "PD10")
				(number "H11")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -63.5 0)
				(length 5.08)
				(name "PD11")
				(number "G7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -66.04 0)
				(length 5.08)
				(name "PD12")
				(number "G8")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -68.58 0)
				(length 5.08)
				(name "PD13")
				(number "G9")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -71.12 0)
				(length 5.08)
				(name "PD14")
				(number "G10")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -73.66 0)
				(length 5.08)
				(name "PD15")
				(number "F6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 83.82 270)
				(length 5.08)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at 0 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -83.82 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C10")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 2.54 -83.82 90)
				(length 5.08)
				(name "VSSA")
				(number "K5")
			)
			(pin power_in line
				(at 5.08 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "K11")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "L6")
			)
			(pin power_in line
				(at 12.7 83.82 270)
				(length 5.08)
				(name "VDDA")
				(number "L5")
			)
			(pin bidirectional line
				(at 25.4 73.66 180)
				(length 5.08)
				(name "PA0")
				(number "G4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 71.12 180)
				(length 5.08)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 68.58 180)
				(length 5.08)
				(name "PA2")
				(number "J3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 66.04 180)
				(length 5.08)
				(name "PA3")
				(number "K1")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA4")
				(number "L1")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA5")
				(number "K2")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA8")
				(number "E7")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA9")
				(number "D8")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA10")
				(number "D9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA11")
				(number "D11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA12")
				(number "D10")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA13")
				(number "B11")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA14")
				(number "B10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA15")
				(number "A10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PB0")
				(number "J4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "PB3")
				(number "A6")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB4")
				(number "C6")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB5")
				(number "B5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB8")
				(number "D5")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB12")
				(number "J9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB13")
				(number "J11")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB14")
				(number "J10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB15")
				(number "H8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PC0")
				(number "G2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PC1")
				(number "G1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PC2")
				(number "G3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PC3")
				(number "H1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC4")
				(number "L3")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC5")
				(number "H4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC8")
				(number "E9")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC9")
				(number "E8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC10")
				(number "C9")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC12")
				(number "D7")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC15")
				(number "D2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483QETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G483QETx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483QETx_0_1")
		(symbol "STM32G483QETx_1_1"
			(pin input line
				(at -27.94 81.28 0)
				(length 5.08)
				(name "VREF+")
				(number "43")
				(alternate "VREFBUF_OUT1" bidirectional line)
			)
			(pin input line
				(at -27.94 78.74 0)
				(length 5.08)
				(name "VREF_+")
				(number "44")
				(alternate "VREFBUF_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 5.08)
				(name "PG0")
				(number "82")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 5.08)
				(name "PG1")
				(number "83")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 5.08)
				(name "PG2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "PG3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "PG4")
				(number "86")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "PG5")
				(number "103")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "PG6")
				(number "104")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "PG7")
				(number "105")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "PG8")
				(number "106")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PG9")
				(number "107")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PG10")
				(number "21")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PF0")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PF1")
				(number "20")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PF2")
				(number "26")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PF3")
				(number "10")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PF5")
				(number "14")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PF6")
				(number "97")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PF7")
				(number "15")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PF8")
				(number "16")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PF9")
				(number "17")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PF10")
				(number "18")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PF11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PF12")
				(number "49")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PE0")
				(number "125")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PE1")
				(number "126")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PE7")
				(number "53")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PE8")
				(number "54")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PE9")
				(number "55")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PE10")
				(number "56")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PE11")
				(number "57")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PE12")
				(number "58")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PE13")
				(number "59")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PE14")
				(number "60")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PE15")
				(number "61")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PD0")
				(number "108")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PD1")
				(number "109")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PD2")
				(number "112")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "PD3")
				(number "113")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 5.08)
				(name "PD4")
				(number "114")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "PD5")
				(number "115")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "PD6")
				(number "116")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 5.08)
				(name "PD7")
				(number "117")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -63.5 0)
				(length 5.08)
				(name "PD8")
				(number "70")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -66.04 0)
				(length 5.08)
				(name "PD9")
				(number "71")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -68.58 0)
				(length 5.08)
				(name "PD10")
				(number "72")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -71.12 0)
				(length 5.08)
				(name "PD11")
				(number "73")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 5.08)
				(name "PD12")
				(number "74")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -76.2 0)
				(length 5.08)
				(name "PD13")
				(number "75")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -78.74 0)
				(length 5.08)
				(name "PD14")
				(number "76")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -81.28 0)
				(length 5.08)
				(name "PD15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "47")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "110")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "127")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "46")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "78")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "79")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "42")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "111")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "128")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "27")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "28")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "29")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "32")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "33")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "34")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "35")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "36")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "89")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "90")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "91")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "92")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "93")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA13")
				(number "96")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA14")
				(number "98")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA15")
				(number "99")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "39")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "40")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "41")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PB3")
				(number "118")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PB4")
				(number "119")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "120")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "121")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "122")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "123")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "124")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "62")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "65")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB12")
				(number "66")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB13")
				(number "67")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB14")
				(number "68")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB15")
				(number "69")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PC0")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PC1")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PC2")
				(number "24")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PC3")
				(number "25")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PC4")
				(number "37")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PC5")
				(number "38")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PC6")
				(number "80")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC7")
				(number "81")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC8")
				(number "87")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC9")
				(number "88")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC10")
				(number "100")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC11")
				(number "101")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC12")
				(number "102")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G483RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483RETx_0_1")
		(symbol "STM32G483RETx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483VEHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G483VEHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483VEHx_0_1")
		(symbol "STM32G483VEHx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "K5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "F3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "E1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "G3")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "E3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "E4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "B3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "C3")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "A1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "B1")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "G5")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "H5")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "H6")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "K6")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "G6")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "K7")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "J7")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE15")
				(number "H7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "B8")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "C6")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "A8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "A7")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "A6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K10")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "G8")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "G7")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "G9")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "F8")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D3")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D5")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D7")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K4")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "G2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "H1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "H2")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "J1")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "J2")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K1")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "D9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "C9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "D8")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "B10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "H4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "J4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "C5")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "B5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "A4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "J8")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J9")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "H9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "F4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "F1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K2")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E8")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "C8")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "A10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "D4")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G483VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G483VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g483ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G483VETx_0_1")
		(symbol "STM32G483VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "36")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "14")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "82")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "83")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "86")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "87")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "88")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "89")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "35")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "26")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "27")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "28")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "29")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "69")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "70")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "71")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "72")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "73")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "76")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "77")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "90")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "91")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "92")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "93")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "94")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "30")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "31")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "65")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "66")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "67")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "79")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "81")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484CETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G484CETx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484CETx_0_1")
		(symbol "STM32G484CETx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G484CEUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484CEUx_0_1")
		(symbol "STM32G484CEUx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "16")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "29")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC11")
				(number "40")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "41")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "42")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "43")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "44")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "45")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "47")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "24")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484METx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G484METx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484METx_0_1")
		(symbol "STM32G484METx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484MEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G484MEYx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-81_4.02x4.27mm_Layout9x9_P0.4mm"
			(at -17.78 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 67 GPIO, WLCSP81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.02x4.27mm*Layout9x9*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484MEYx_0_1")
		(symbol "STM32G484MEYx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "J6")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "D8")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "E9")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "F9")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "H5")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "G5")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "F5")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "J4")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "H4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "E5")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "G4")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "J3")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "F4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "B4")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "A4")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "G1")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "F3")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "F2")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD11")
				(number "E2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C8")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F8")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "G9")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "E6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "H7")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "E3")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "D5")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "C5")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "D2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "C4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "A3")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "B8")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "C9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "A8")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "J1")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "H6")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "D7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "E7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "G8")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "H8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "D6")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "F7")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "G7")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "J8")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "D4")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "C1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "B2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "F6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "J7")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "C6")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "B6")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "C7")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "B7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "H3")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "H2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "G3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "H1")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "G2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "E4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484PEIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G484PEIx"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484pe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484PEIx_0_1")
		(symbol "STM32G484PEIx_1_1"
			(pin input line
				(at -25.4 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L4")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 68.58 0)
				(length 5.08)
				(name "PG0")
				(number "F9")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 66.04 0)
				(length 5.08)
				(name "PG1")
				(number "F8")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 63.5 0)
				(length 5.08)
				(name "PG2")
				(number "F7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "PG3")
				(number "E11")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "PG4")
				(number "E10")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 5.08)
				(name "PG10")
				(number "F5")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "PF0")
				(number "F1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 5.08)
				(name "PF1")
				(number "F2")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PF4")
				(number "D4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PF5")
				(number "E3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PF6")
				(number "A11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PF7")
				(number "E4")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PF8")
				(number "E5")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PF9")
				(number "F3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PF10")
				(number "F4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PF11")
				(number "J5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PF12")
				(number "H5")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PF13")
				(number "J6")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PF14")
				(number "H6")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PF15")
				(number "G6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PE0")
				(number "B4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PE1")
				(number "C4")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PE4")
				(number "A1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PE5")
				(number "B1")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PE6")
				(number "C3")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PE7")
				(number "L7")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PE8")
				(number "K7")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PE9")
				(number "J7")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PE10")
				(number "H7")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PE11")
				(number "L8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "PE13")
				(number "J8")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "PE14")
				(number "K9")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "PE15")
				(number "L9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "PD0")
				(number "B9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "PD2")
				(number "C7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "PD3")
				(number "B7")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "PD4")
				(number "A7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "PD5")
				(number "E6")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "PD6")
				(number "D6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "PD8")
				(number "H9")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "PD9")
				(number "H10")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "PD10")
				(number "H11")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -63.5 0)
				(length 5.08)
				(name "PD11")
				(number "G7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -66.04 0)
				(length 5.08)
				(name "PD12")
				(number "G8")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -68.58 0)
				(length 5.08)
				(name "PD13")
				(number "G9")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -71.12 0)
				(length 5.08)
				(name "PD14")
				(number "G10")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -73.66 0)
				(length 5.08)
				(name "PD15")
				(number "F6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 83.82 270)
				(length 5.08)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at 0 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "E1")
			)
			(pin power_in line
				(at 0 -83.82 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C10")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 2.54 -83.82 90)
				(length 5.08)
				(name "VSSA")
				(number "K5")
			)
			(pin power_in line
				(at 5.08 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "K11")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 5.08)
				(name "VDD")
				(number "L6")
			)
			(pin power_in line
				(at 12.7 83.82 270)
				(length 5.08)
				(name "VDDA")
				(number "L5")
			)
			(pin bidirectional line
				(at 25.4 73.66 180)
				(length 5.08)
				(name "PA0")
				(number "G4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 71.12 180)
				(length 5.08)
				(name "PA1")
				(number "H3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 68.58 180)
				(length 5.08)
				(name "PA2")
				(number "J3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 66.04 180)
				(length 5.08)
				(name "PA3")
				(number "K1")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "PA4")
				(number "L1")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "PA5")
				(number "K2")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "PA8")
				(number "E7")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "PA9")
				(number "D8")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "PA10")
				(number "D9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "PA11")
				(number "D11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "PA12")
				(number "D10")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "PA13")
				(number "B11")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "PA14")
				(number "B10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "PA15")
				(number "A10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "PB0")
				(number "J4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "PB3")
				(number "A6")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PB4")
				(number "C6")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PB5")
				(number "B5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PB8")
				(number "D5")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PB12")
				(number "J9")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PB13")
				(number "J11")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PB14")
				(number "J10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PB15")
				(number "H8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PC0")
				(number "G2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PC1")
				(number "G1")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PC2")
				(number "G3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PC3")
				(number "H1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PC4")
				(number "L3")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "PC5")
				(number "H4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "PC8")
				(number "E9")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "PC9")
				(number "E8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "PC10")
				(number "C9")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "PC11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "PC12")
				(number "D7")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "PC15")
				(number "D2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484QETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G484QETx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484QETx_0_1")
		(symbol "STM32G484QETx_1_1"
			(pin input line
				(at -27.94 81.28 0)
				(length 5.08)
				(name "VREF+")
				(number "43")
				(alternate "VREFBUF_OUT1" bidirectional line)
			)
			(pin input line
				(at -27.94 78.74 0)
				(length 5.08)
				(name "VREF_+")
				(number "44")
				(alternate "VREFBUF_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 5.08)
				(name "PG0")
				(number "82")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 5.08)
				(name "PG1")
				(number "83")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 5.08)
				(name "PG2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A12" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "PG3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A13" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "PG4")
				(number "86")
				(alternate "FMC_A14" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "PG5")
				(number "103")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "PG6")
				(number "104")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "PG7")
				(number "105")
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "PG8")
				(number "106")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PG9")
				(number "107")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PG10")
				(number "21")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PF0")
				(number "19")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PF1")
				(number "20")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PF2")
				(number "26")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PF3")
				(number "10")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PF4")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PF5")
				(number "14")
				(alternate "FMC_A5" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PF6")
				(number "97")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PF7")
				(number "15")
				(alternate "FMC_A1" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PF8")
				(number "16")
				(alternate "FMC_A24" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PF9")
				(number "17")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PF10")
				(number "18")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PF11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PF12")
				(number "49")
				(alternate "FMC_A6" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PE0")
				(number "125")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PE1")
				(number "126")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PE7")
				(number "53")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PE8")
				(number "54")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PE9")
				(number "55")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PE10")
				(number "56")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PE11")
				(number "57")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PE12")
				(number "58")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PE13")
				(number "59")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PE14")
				(number "60")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PE15")
				(number "61")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PD0")
				(number "108")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PD1")
				(number "109")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PD2")
				(number "112")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "PD3")
				(number "113")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 5.08)
				(name "PD4")
				(number "114")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "PD5")
				(number "115")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "PD6")
				(number "116")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 5.08)
				(name "PD7")
				(number "117")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -63.5 0)
				(length 5.08)
				(name "PD8")
				(number "70")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -66.04 0)
				(length 5.08)
				(name "PD9")
				(number "71")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -68.58 0)
				(length 5.08)
				(name "PD10")
				(number "72")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -71.12 0)
				(length 5.08)
				(name "PD11")
				(number "73")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 5.08)
				(name "PD12")
				(number "74")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -76.2 0)
				(length 5.08)
				(name "PD13")
				(number "75")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -78.74 0)
				(length 5.08)
				(name "PD14")
				(number "76")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -81.28 0)
				(length 5.08)
				(name "PD15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "47")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "110")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "127")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "46")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "78")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "79")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "42")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "111")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "128")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "27")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "28")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "29")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "32")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "33")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "34")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "35")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "36")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "89")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "90")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "91")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "92")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "93")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA13")
				(number "96")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA14")
				(number "98")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA15")
				(number "99")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "39")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "40")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "41")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PB3")
				(number "118")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PB4")
				(number "119")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "120")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "121")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "122")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "123")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "124")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "62")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "65")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB12")
				(number "66")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB13")
				(number "67")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB14")
				(number "68")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB15")
				(number "69")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PC0")
				(number "22")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PC1")
				(number "23")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PC2")
				(number "24")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PC3")
				(number "25")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PC4")
				(number "37")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PC5")
				(number "38")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PC6")
				(number "80")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC7")
				(number "81")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC8")
				(number "87")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC9")
				(number "88")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC10")
				(number "100")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC11")
				(number "101")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC12")
				(number "102")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G484RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484RETx_0_1")
		(symbol "STM32G484RETx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484VEHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G484VEHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484VEHx_0_1")
		(symbol "STM32G484VEHx_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "K5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "F3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "E1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "G3")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "E3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "E4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "B3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "C3")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "A1")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "B1")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "G5")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "H5")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "H6")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "K6")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "G6")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "K7")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "J7")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PE15")
				(number "H7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "B8")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "B7")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "C6")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "A8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "A7")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "A6")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "K10")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "G8")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "G7")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "G9")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "F8")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "D3")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D5")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "D7")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E5")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E7")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F5")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "K4")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "G4")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "G2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "H1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "H3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "H2")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "J1")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "J2")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "K1")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "D9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "C10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "C9")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "D8")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "B10")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "B9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "H4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "J4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "C5")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "B5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "A4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "J8")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "K8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "J9")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "H9")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "F2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "F4")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "F1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K2")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E8")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "C8")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "A10")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "D4")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G484VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G484VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g484ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G484VETx_0_1")
		(symbol "STM32G484VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "36")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "14")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_A0" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "FMC_A22" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "ADC4_IN6" bidirectional line)
				(alternate "ADC5_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "ADC4_IN14" bidirectional line)
				(alternate "ADC5_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "ADC4_IN15" bidirectional line)
				(alternate "ADC5_IN15" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "ADC4_IN16" bidirectional line)
				(alternate "ADC5_IN16" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "ADC4_IN1" bidirectional line)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC4_IN2" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "82")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "83")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "86")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "87")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "88")
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "89")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "ADC4_IN12" bidirectional line)
				(alternate "ADC5_IN12" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM1" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "ADC4_IN13" bidirectional line)
				(alternate "ADC5_IN13" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "ADC4_IN7" bidirectional line)
				(alternate "ADC5_IN7" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "ADC4_IN8" bidirectional line)
				(alternate "ADC5_IN8" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "ADC4_IN9" bidirectional line)
				(alternate "ADC5_IN9" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "ADC4_IN10" bidirectional line)
				(alternate "ADC5_IN10" bidirectional line)
				(alternate "COMP5_INM" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "ADC4_IN11" bidirectional line)
				(alternate "ADC5_IN11" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "35")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM1" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "26")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "27")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "28")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DAC2_OUT1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "29")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "69")
				(alternate "ADC5_IN1" bidirectional line)
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_CHA1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OPAMP5_VOUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "70")
				(alternate "ADC5_IN2" bidirectional line)
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHA2" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "71")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_CHB1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "72")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_CHB2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "73")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_FLT1" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "76")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "77")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_FLT2" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "90")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "FDCAN3_RX" bidirectional line)
				(alternate "HRTIM1_EEV9" bidirectional line)
				(alternate "HRTIM1_SCOUT" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "91")
				(alternate "FDCAN3_TX" bidirectional line)
				(alternate "HRTIM1_EEV7" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "92")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_EEV6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "93")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_EEV4" bidirectional line)
				(alternate "HRTIM1_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "94")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM1_EEV3" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM1_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM1_EEV5" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP5_INM" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "OPAMP4_VINM" bidirectional line)
				(alternate "OPAMP4_VINM0" bidirectional line)
				(alternate "OPAMP4_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP6_INP" bidirectional line)
				(alternate "HRTIM1_FLT4" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC4_IN3" bidirectional line)
				(alternate "COMP7_INM" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "HRTIM1_CHC1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP4_VOUT" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "COMP5_INP" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "HRTIM1_CHC2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP4_VINP" bidirectional line)
				(alternate "OPAMP4_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC4_IN4" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "COMP7_INP" bidirectional line)
				(alternate "HRTIM1_CHD1" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "ADC4_IN5" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "COMP6_INM" bidirectional line)
				(alternate "HRTIM1_CHD2" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPAMP5_VINM" bidirectional line)
				(alternate "OPAMP5_VINM0" bidirectional line)
				(alternate "OPAMP5_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "ADC4_EXTI2" bidirectional line)
				(alternate "ADC5_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "ADC4_EXTI3" bidirectional line)
				(alternate "ADC5_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OPAMP5_VINP" bidirectional line)
				(alternate "OPAMP5_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "30")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "31")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "65")
				(alternate "COMP6_OUT" bidirectional line)
				(alternate "HRTIM1_CHF1" bidirectional line)
				(alternate "HRTIM1_EEV10" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "66")
				(alternate "COMP5_OUT" bidirectional line)
				(alternate "HRTIM1_CHF2" bidirectional line)
				(alternate "HRTIM1_FLT5" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "67")
				(alternate "COMP7_OUT" bidirectional line)
				(alternate "HRTIM1_CHE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC2_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "DAC4_EXTI9" bidirectional line)
				(alternate "HRTIM1_CHE2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "79")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC2_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "DAC4_EXTI10" bidirectional line)
				(alternate "HRTIM1_FLT6" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "HRTIM1_EEV2" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "81")
				(alternate "HRTIM1_EEV1" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491C_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G491C_C-E_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491C_C-E_Tx_0_1")
		(symbol "STM32G491C_C-E_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491C_C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G491C_C-E_Ux"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491C_C-E_Ux_0_1")
		(symbol "STM32G491C_C-E_Ux_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "16")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "29")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC11")
				(number "40")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "41")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "42")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "43")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "44")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "45")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "47")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "24")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491K_C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G491K_C-E_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491K_C-E_Ux_0_1")
		(symbol "STM32G491K_C-E_Ux_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PG10")
				(number "4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "13")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB8")
				(number "31")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "9")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "10")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "11")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "12")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491M_C-E_Sx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G491M_C-E_Sx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491M_C-E_Sx_0_1")
		(symbol "STM32G491M_C-E_Sx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491M_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G491M_C-E_Tx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491M_C-E_Tx_0_1")
		(symbol "STM32G491M_C-E_Tx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491RETxZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G491RETxZ"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491RETxZ_0_1")
		(symbol "STM32G491RETxZ_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491REYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G491REYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_3.56x3.52mm_Layout8x8_P0.4mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.56x3.52mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491REYx_0_1")
		(symbol "STM32G491REYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "H5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "D7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "E8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "E7")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "A4")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "F8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C7")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "E6")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "G6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "F4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E3")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "A2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "C6")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "C8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "D8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B8")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "G5")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H4")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "F7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "D5")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "F6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "E5")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E4")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "H7")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "F5")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "H6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "D4")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C5")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A6")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H2")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491R_C-E_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G491R_C-E_Ix"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491R_C-E_Ix_0_1")
		(symbol "STM32G491R_C-E_Ix_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "G5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "D2")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "E1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "F1")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "D5")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "F4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "F6")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "C5")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "A6")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "B1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "D4")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E4")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G3")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "E5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F5")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H6")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G6")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491R_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G491R_C-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491R_C-E_Tx_0_1")
		(symbol "STM32G491R_C-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G491V_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G491V_C-E_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256-512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G491V_C-E_Tx_0_1")
		(symbol "STM32G491V_C-E_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "36")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "14")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "82")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "83")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "86")
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "87")
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "88")
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "89")
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "35")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "26")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "27")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "28")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "29")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "69")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "71")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "72")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "73")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "76")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "77")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "90")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "91")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "92")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "93")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "94")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "30")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "31")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "65")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "66")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "79")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "81")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1CETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G4A1CETx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1CETx_0_1")
		(symbol "STM32G4A1CETx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "16")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "18")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "40")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "41")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "42")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "43")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "44")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "25")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "26")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "27")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "28")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "29")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "37")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "38")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "39")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G4A1CEUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1CEUx_0_1")
		(symbol "STM32G4A1CEUx_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC4")
				(number "16")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC6")
				(number "29")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC11")
				(number "40")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "41")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "42")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "43")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "44")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "45")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "47")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "22")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "24")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "12")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "13")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "14")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "15")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "30")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "31")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "32")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "34")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "36")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1KEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G4A1KEUx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1KEUx_0_1")
		(symbol "STM32G4A1KEUx_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PG10")
				(number "4")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "2")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "3")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "13")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB8")
				(number "31")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "9")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "10")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "11")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "12")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1MESx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G4A1MESx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1MESx_0_1")
		(symbol "STM32G4A1MESx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1METx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G4A1METx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1METx_0_1")
		(symbol "STM32G4A1METx_1_1"
			(pin input line
				(at -20.32 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "30")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "31")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "32")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PE10")
				(number "33")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PE11")
				(number "34")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PE12")
				(number "35")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PE13")
				(number "36")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PE14")
				(number "37")
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PE15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PD0")
				(number "69")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PD1")
				(number "70")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD2")
				(number "71")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD8")
				(number "47")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD9")
				(number "48")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD10")
				(number "49")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "PC6")
				(number "52")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "PC7")
				(number "53")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "PC8")
				(number "54")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "PC9")
				(number "55")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "PC10")
				(number "66")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "PC11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "PC12")
				(number "68")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "56")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "58")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "60")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "63")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "64")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "72")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "73")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "74")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "75")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "76")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "77")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "78")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "39")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "43")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "44")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "45")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1REIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G4A1REIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1REIx_0_1")
		(symbol "STM32G4A1REIx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "G5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "D2")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "E1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "F1")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "D5")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "F4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "F6")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "C5")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "A6")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "B1")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "C2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "H2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "D4")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E4")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G3")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H3")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E6")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "E5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F5")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C4")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "B4")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "A4")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A3")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H6")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G8")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G6")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G4A1RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1RETx_0_1")
		(symbol "STM32G4A1RETx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "28")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "55")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "22")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "23")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "38")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "39")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "40")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "41")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "52")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "53")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "54")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "12")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "13")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "14")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "18")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "19")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "20")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "21")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "42")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "43")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "44")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "46")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "49")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "50")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "51")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "56")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "57")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "58")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "59")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "60")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "30")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "33")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1REYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G4A1REYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_3.56x3.52mm_Layout8x8_P0.4mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.56x3.52mm*Layout8x8*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1REYx_0_1")
		(symbol "STM32G4A1REYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "H5")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PG10")
				(number "D7")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "E8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "E7")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "A4")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "F8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C7")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "E6")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "G6")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "F4")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E3")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E2")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "A2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "A3")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "C6")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "C8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "D8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B8")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "G5")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H4")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "F7")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "D5")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "F6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "E5")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E4")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "H7")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "F5")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D2")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "B4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "H6")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G4")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "D4")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "C5")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "A6")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B6")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "H2")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G3")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G4A1VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G4A1VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g4a1ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32G4A1VETx_0_1")
		(symbol "STM32G4A1VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "VREF+")
				(number "36")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "PG10")
				(number "14")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "PF0")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PF1")
				(number "13")
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PF2")
				(number "19")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PF9")
				(number "10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM20_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PF10")
				(number "11")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM20_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM20_CH4N" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM20_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SYS_TRACECLK" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM20_CH1N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM20_CH2N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM20_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC3_IN4" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC3_IN6" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC3_IN2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC3_IN14" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN15" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "ADC3_IN16" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "ADC3_IN3" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "82")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "83")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "84")
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "85")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "QUADSPI1_BK2_NCS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "86")
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "87")
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "88")
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "89")
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "ADC3_IN7" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_IN8" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "ADC3_IN9" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "ADC3_IN10" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "ADC3_IN11" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "35")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "20")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "21")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM0" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "22")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SYS_WKUP4" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "26")
				(alternate "ADC2_IN17" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "27")
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "28")
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "29")
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "OPAMP1_VINP_SEC" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "69")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "71")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "72")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "73")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "76")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "77")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM20_ETR" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC3_IN12" bidirectional line)
				(alternate "COMP4_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC3_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "OPAMP6_VINM" bidirectional line)
				(alternate "OPAMP6_VINM1" bidirectional line)
				(alternate "OPAMP6_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP4_INM" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM0" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TIM20_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "90")
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-SWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "91")
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "92")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "93")
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "94")
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "OPAMP3_VINM1" bidirectional line)
				(alternate "OPAMP3_VINM_SEC" bidirectional line)
				(alternate "QUADSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "50")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OPAMP6_VOUT" bidirectional line)
				(alternate "QUADSPI1_BK1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC3_IN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "OPAMP3_VINP_SEC" bidirectional line)
				(alternate "OPAMP6_VINP" bidirectional line)
				(alternate "OPAMP6_VINP_SEC" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP4_OUT" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "OPAMP2_VINP_SEC" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "COMP3_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP3_INP" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI1_BK2_IO0" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "ADC3_EXTI2" bidirectional line)
				(alternate "COMP3_OUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "QUADSPI1_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM20_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "ADC3_EXTI3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "QUADSPI1_BK2_IO2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "30")
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "QUADSPI1_BK2_IO3" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "31")
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "OPAMP1_VINM_SEC" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
				(alternate "OPAMP2_VINM_SEC" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SYS_WKUP5" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "65")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "66")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "TIM20_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DAC3_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "79")
				(alternate "DAC1_EXTI10" bidirectional line)
				(alternate "DAC3_EXTI10" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "81")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32G431C6Tx"
		(extends "STM32G431C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G431C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431C6Ux"
		(extends "STM32G431C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G431C6Ux"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431C8Tx"
		(extends "STM32G431C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G431C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431C8Ux"
		(extends "STM32G431C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G431C8Ux"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431CBTx"
		(extends "STM32G431C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G431CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431CBUx"
		(extends "STM32G431C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G431CBUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431K6Tx"
		(extends "STM32G431K_6-8-B_Tx")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G431K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431K6Ux"
		(extends "STM32G431K_6-8-B_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G431K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431K8Tx"
		(extends "STM32G431K_6-8-B_Tx")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G431K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431K8Ux"
		(extends "STM32G431K_6-8-B_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G431K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431KBTx"
		(extends "STM32G431K_6-8-B_Tx")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G431KBTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431KBUx"
		(extends "STM32G431K_6-8-B_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G431KBUx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431M6Tx"
		(extends "STM32G431M_6-8-B_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G431M6Tx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431m6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431M8Tx"
		(extends "STM32G431M_6-8-B_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G431M8Tx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431m8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431MBTx"
		(extends "STM32G431M_6-8-B_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G431MBTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431R6Ix"
		(extends "STM32G431R_6-8-B_Ix")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431R6Ix"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431R6Tx"
		(extends "STM32G431R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431R8Ix"
		(extends "STM32G431R_6-8-B_Ix")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431R8Ix"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431R8Tx"
		(extends "STM32G431R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431RBIx"
		(extends "STM32G431R_6-8-B_Ix")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431RBIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431RBTx"
		(extends "STM32G431R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G431RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431V6Tx"
		(extends "STM32G431V_6-8-B_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G431V6Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431v6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 32KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431V8Tx"
		(extends "STM32G431V_6-8-B_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G431V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 64KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G431VBTx"
		(extends "STM32G431V_6-8-B_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G431VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g431vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 32KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473CBTx"
		(extends "STM32G473C_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G473CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473CBUx"
		(extends "STM32G473C_B-C-E_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G473CBUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473CCTx"
		(extends "STM32G473C_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G473CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473CCUx"
		(extends "STM32G473C_B-C-E_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G473CCUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473CETx"
		(extends "STM32G473C_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G473CETx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473CEUx"
		(extends "STM32G473C_B-C-E_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G473CEUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473MBTx"
		(extends "STM32G473M_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G473MBTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473MCTx"
		(extends "STM32G473M_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G473MCTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473METx"
		(extends "STM32G473M_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G473METx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473PBIx"
		(extends "STM32G473P_B-C-E_Ix")
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G473PBIx"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473pb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473PCIx"
		(extends "STM32G473P_B-C-E_Ix")
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G473PCIx"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473pc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473PEIx"
		(extends "STM32G473P_B-C-E_Ix")
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G473PEIx"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473pe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473QBTx"
		(extends "STM32G473Q_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G473QBTx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473qb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473QCTx"
		(extends "STM32G473Q_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G473QCTx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473qc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473QETx"
		(extends "STM32G473Q_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G473QETx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473RBTx"
		(extends "STM32G473R_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G473RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473RCTx"
		(extends "STM32G473R_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G473RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473RETx"
		(extends "STM32G473R_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G473RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473VBHx"
		(extends "STM32G473V_B-C-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G473VBHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473VBTx"
		(extends "STM32G473V_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G473VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473VCHx"
		(extends "STM32G473V_B-C-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G473VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473VCTx"
		(extends "STM32G473V_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G473VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473VEHx"
		(extends "STM32G473V_B-C-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G473VEHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G473VETx"
		(extends "STM32G473V_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G473VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474CBTx"
		(extends "STM32G474C_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G474CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474CBUx"
		(extends "STM32G474C_B-C-E_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G474CBUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474CCTx"
		(extends "STM32G474C_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G474CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474CCUx"
		(extends "STM32G474C_B-C-E_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G474CCUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474CETx"
		(extends "STM32G474C_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G474CETx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474CEUx"
		(extends "STM32G474C_B-C-E_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G474CEUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474MBTx"
		(extends "STM32G474M_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G474MBTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474MCTx"
		(extends "STM32G474M_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G474MCTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474METx"
		(extends "STM32G474M_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G474METx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474PBIx"
		(extends "STM32G474P_B-C-E_Ix")
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G474PBIx"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474pb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474PCIx"
		(extends "STM32G474P_B-C-E_Ix")
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G474PCIx"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474pc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474PEIx"
		(extends "STM32G474P_B-C-E_Ix")
		(property "Reference" "U"
			(at -20.32 80.01 0)
		)
		(property "Value" "STM32G474PEIx"
			(at 15.24 80.01 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-121_6x6mm_Layout11x11_P0.5mm"
			(at -20.32 -78.74 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474pe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 102 GPIO, UFBGA121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*6x6mm*Layout11x11*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474QBTx"
		(extends "STM32G474Q_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G474QBTx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474qb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474QCTx"
		(extends "STM32G474Q_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G474QCTx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474qc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474QETx"
		(extends "STM32G474Q_B-C-E_Tx")
		(property "Reference" "U"
			(at -22.86 87.63 0)
		)
		(property "Value" "STM32G474QETx"
			(at 15.24 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-128_14x14mm_P0.4mm"
			(at -22.86 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 107 GPIO, LQFP128"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474RBTx"
		(extends "STM32G474R_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G474RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474RCTx"
		(extends "STM32G474R_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G474RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474RETx"
		(extends "STM32G474R_B-C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G474RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474VBHx"
		(extends "STM32G474V_B-C-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G474VBHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474VBTx"
		(extends "STM32G474V_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G474VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 128KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474VCHx"
		(extends "STM32G474V_B-C-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G474VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474VCTx"
		(extends "STM32G474V_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G474VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474VEHx"
		(extends "STM32G474V_B-C-E_Hx")
		(property "Reference" "U"
			(at -15.24 69.85 0)
		)
		(property "Value" "STM32G474VEHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_8x8mm_Layout10x10_P0.8mm"
			(at -15.24 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, TFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*8x8mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G474VETx"
		(extends "STM32G474V_B-C-E_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G474VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g474ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 128KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491CCTx"
		(extends "STM32G491C_C-E_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G491CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491CCUx"
		(extends "STM32G491C_C-E_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G491CCUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491CETx"
		(extends "STM32G491C_C-E_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32G491CETx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491CEUx"
		(extends "STM32G491C_C-E_Ux")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "STM32G491CEUx"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 42 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491KCUx"
		(extends "STM32G491K_C-E_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G491KCUx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491KEUx"
		(extends "STM32G491K_C-E_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32G491KEUx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491ke.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491MCSx"
		(extends "STM32G491M_C-E_Sx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G491MCSx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491MCTx"
		(extends "STM32G491M_C-E_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G491MCTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491MESx"
		(extends "STM32G491M_C-E_Sx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G491MESx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491METx"
		(extends "STM32G491M_C-E_Tx")
		(property "Reference" "U"
			(at -17.78 57.15 0)
		)
		(property "Value" "STM32G491METx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -17.78 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 66 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491RCIx"
		(extends "STM32G491R_C-E_Ix")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G491RCIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491RCTx"
		(extends "STM32G491R_C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G491RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491REIx"
		(extends "STM32G491R_C-E_Ix")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G491REIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491RETx"
		(extends "STM32G491R_C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32G491RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491VCTx"
		(extends "STM32G491V_C-E_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G491VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32G491VETx"
		(extends "STM32G491V_C-E_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32G491VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g491ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 512KB flash, 112KB RAM, 170 MHz, 1.71-3.6V, 86 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M4 STM32G4 STM32G4x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
